{"text_format":"2","workbook":"xlsx","n_sheets":11,"sheets":["城市生命线数据分类","燃气分类","供水分类","排水分类","第三方分类","桥梁分类","道路分类","综合应用","综合管线","行政区划代码表","监测设备及指标字典"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"城市生命线数据分类","index":0,"n_rows":180,"n_cols":16,"rows_kept":180,"cut":false,"hidden":false,"merged":[[0,0,0,1],[0,2,0,4],[171,0,171,7],[2,0,41,0],[42,0,68,0],[69,0,104,0],[105,0,122,0],[123,0,141,0],[142,0,152,0],[153,0,170,0],[172,0,179,0],[2,1,9,1],[10,1,24,1],[25,1,41,1],[42,1,48,1],[49,1,56,1],[57,1,68,1],[69,1,81,1],[82,1,90,1],[91,1,104,1],[105,1,107,1],[109,1,122,1],[123,1,124,1],[125,1,133,1],[134,1,141,1],[142,1,143,1],[144,1,152,1],[153,1,166,1],[167,1,170,1],[172,1,179,1],[2,2,41,2],[42,2,68,2],[69,2,104,2],[105,2,122,2],[123,2,141,2],[142,2,152,2],[153,2,170,2],[172,2,179,2],[2,3,9,3],[10,3,24,3],[25,3,41,3],[42,3,48,3],[49,3,56,3],[57,3,68,3],[69,3,81,3],[82,3,90,3],[91,3,104,3],[105,3,107,3],[109,3,122,3],[123,3,124,3],[125,3,133,3],[134,3,141,3],[142,3,143,3],[144,3,152,3],[153,3,166,3],[167,3,170,3],[172,3,179,3],[4,4,6,4],[8,4,9,4],[10,4,11,4],[12,4,13,4],[14,4,15,4],[17,4,18,4],[19,4,20,4],[21,4,22,4],[23,4,24,4],[0,5,1,5],[4,5,6,5],[8,5,9,5],[10,5,11,5],[12,5,13,5],[14,5,15,5],[17,5,18,5],[19,5,20,5],[21,5,22,5],[23,5,24,5],[0,6,1,6],[4,6,6,6],[8,6,9,6],[10,6,11,6],[12,6,13,6],[14,6,15,6],[17,6,18,6],[19,6,20,6],[21,6,22,6],[23,6,24,6],[0,7,1,7],[4,7,6,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,12,1,12],[0,13,1,13],[0,14,1,14],[4,14,6,14],[8,14,9,14],[10,14,11,14],[0,15,1,15],[4,15,6,15],[8,15,9,15],[10,15,11,15]]}
["数据分类",null,"代号",null,null,"中文表名","表名","要素类型","备注","是否对接(已对接、待对接、无法提供)","对接时间","来源系统","提供方式","更新频率","缺失必给字段","上报数据量"]
["大类","一级","大类","一级","二级"]
["燃气设施","基础数据","RQ","JC","GX","管线","RQ_JS_GX、 RQ_JS_GX_ATT","线","已提供部分数据","已对接","2023-06-09","地下官网系统","线下","年"]
[{"$nulls":4},"GD","管点","RQ_JS_GD","点","已提供部分数据","已对接","2023-06-09","地下官网系统","线下","年"]
[{"$nulls":4},"CZ","场站","RQ_JS_CZ","面","门站、储配站：新区储备站（门站 ，已提供）、青阳门站（数据未提供）","已对接","2023-06-16","台账","填报","年","1.华润车用气加气站：缺少必给字段：BSM,XZQHDM,CQNL,SJCQL,GZNL\n2.新区储配站信息：缺少必给字段：标识码\n",12]
[{"$nulls":8},"加气站","已对接","2023-06-15","台账","填报","年"]
[{"$nulls":8},"调压站","已对接","2023-07-27","台账","填报","年"]
[{"$nulls":4},"RQYH","燃气用户","RQ_JS_RQYH",null,"excel 表格，CIS客服系统，业务问题联系人：宁骥良；提供部分","已对接","2023-06-09","CIS客服系统","线下","半年","1.燃气用户：缺少必给字段：标识码，启用日期，气源种类，液化气瓶种类，液化气存瓶数，供气单位，是否重点用气场所，报警器，是否有切断装置",10013]
[{"$nulls":4},"JCD","监测点","RQ_JS_JCD","点","可燃气体探测器西维斯--地下燃气井泄露监测平台（给一部分）","已对接","2023-07-27","地下燃气井泄露监测平台","填报",null,"缺少标识码",81]
[{"$nulls":8},"流量、压力、温度SCADA系统--管美玲","已对接","7月6号","SCADA系统","线下"]
[null,"监测数据",null,"JC","JCSB","监测设备","RQ_JC_JCSB","-","可燃气体探测器","已对接","7月6号","地下燃气井泄露监测平台","线下",null,"缺少点位标识码、设备类型、设备名称、检测指标、采集频率、上传频率、设备状态",3763]
[{"$nulls":8},"流量、压力、温度","已对接","2023-08-28","SCADA系统","填报"]
[{"$nulls":4},"JCXYZ","监测项阈值","RQ_JC_JCXYZ","-","可燃气体探测器，暂无法提供","无法提供",null,"地下燃气井泄露监测平台","填报"]
[{"$nulls":8},"流量、压力、温度，暂无法提供","已对接",null,"SCADA系统","线下",null,"缺少：设备标识码，设备类型"]
[{"$nulls":4},"SSJC","实时监测","RQ_JC_SSJC","-","可燃气体探测器","已对接",null,"地下燃气井泄露监测平台","kafka",null,null,1859]
[{"$nulls":8},"流量、压力、温度","待对接",null,"SCADA系统","kafka"]
[{"$nulls":4},"SPJK","视频监控","RQ_JC_SPJK","点","高压管道视频监控系统--互联网--可提供","待对接","2023-06-09","高压管道视频监控系统","填报","半年",null,23]
[{"$nulls":4},"JCBJ","监测报警","RQ_JC_JCBJ","-","可燃气体探测器，暂无法提供","无法提供",null,"地下燃气井泄露监测平台"]
[{"$nulls":8},"流量、压力、温度，暂无法提供","无法提供",null,"SCADA系统"]
[{"$nulls":4},"BJFX","报警分析","RQ_JC_BJFX","-","可燃气体探测器，暂无法提供","无法提供",null,"地下燃气井泄露监测平台"]
[{"$nulls":8},"流量、压力、温度，暂无法提供","无法提供",null,"SCADA系统"]
[{"$nulls":4},"BJCZ","报警处置","RQ_JC_BJCZ","-","可燃气体探测器，暂无法提供","无法提供",null,"地下燃气井泄露监测平台"]
[{"$nulls":8},"流量、压力、温度，暂无法提供","无法提供",null,"SCADA系统"]
[{"$nulls":4},"JCYJ","监测预警","RQ_JC_JCYJ",null,"可燃气体探测器，暂无法提供","无法提供",null,"地下燃气井泄露监测平台"]
[{"$nulls":7},"-","流量、压力、温度，暂无法提供","无法提供",null,"SCADA系统"]
[null,"监管数据",null,"JG","JHXM","计划项目","RQ_JG_JHXM","面","23年部分数据","已对接","2023-08-28",null,null,null,"缺少：项目类型（新建/改建/扩建），主管单位，项目内容，项目投资额"]
[{"$nulls":4},"JSXM","建设项目","RQ_JG_JSXM","面","工程部，100条","已对接","2023-08-28"]
[{"$nulls":4},"QXQXD","抢修抢险点","RQ_JG_QXQXD","点","有系统，先手工","已对接，未提供数据","2023-08-28","台账","填报","半年"]
[{"$nulls":4},"QXQXQY","抢修抢险区域","RQ_JG_QXQXQY","面","有系统，先手工","已对接，未提供数据","2023-08-28","台账","填报","半年"]
[{"$nulls":4},"RCWHWX","日常维护维修","RQ_JG_RCWHWX","-","业务问题联系人：宁骥良","已对接","2023-08-28","台账","填报","半年","1.维修记录查询：缺少必给字段：标识码，检测方法",24842]
[{"$nulls":4},"TFSJQX","突发事件抢修","RQ_JG_TFSJQX","-","业务问题联系人：宁骥良","已对接","2023-06-07","台账","填报","半年","燃气工单抢修信息：缺少必给字段：标识码，行政区划代码，事件名称，响应级别，现场照片，附件",52346]
[{"$nulls":4},"XJJL","巡检记录","RQ_JG_XJJL","-","excel表格、半年，巡检、隐患，提供表 瞿乐依，巡检系统","已对接","2023-06-07","台账","填报","半年",null,230]
[{"$nulls":4},"RQSSYH","燃气设施隐患","RQ_JC_RQSSYH","点","excel表格、半年，巡检、隐患，提供表 瞿乐依，巡检系统","已对接","2023-06-07","台账","填报","半年","阀门隐患已办信息：缺少必给字段：标识码，隐患等级，所属机构，上报人单位",219]
[{"$nulls":4},"AQJCTJ","安全检查统计表","RQ_JG_AQJCTJ","-","手工数据","已对接",{"$nulls":5},168]
[{"$nulls":4},"LHJCJL","联合检查记录","RQ_JG_LHJCJL","-","是纸质扫描件，无法提供电子档","已对接"]
[{"$nulls":4},"ZGJL","整改记录","RQ_JG_ZGJL","-",null,"已对接",{"$nulls":5},2]
[{"$nulls":4},"XJXCJL","巡检巡查信息","RQ_JG_XJXCJL",null,null,"已对接","2023-08-28",null,"线下",null,null,1]
[{"$nulls":4},"RQFXTJ","燃气风险统计信息","RQ_JG_RQFXTJ",null,null,"已对接","2023-08-28",{"$nulls":4},1]
[{"$nulls":4},"FXPG","风险评估信息","RQ_JG_FXPG",null,null,"已对接","2023-08-28",{"$nulls":4},1]
[{"$nulls":4},"_LJGWTJ","老旧管网统计表","RQ_JG_LJGWTJ",null,null,"已对接","2023-09-28",{"$nulls":4},1]
[{"$nulls":4},"XJXCDSFSGWT","巡检养护第三方施工问题属性结构表","RQ_JG_XJXCDSFSGWT",null,null,"已对接","2023-09-28",{"$nulls":4},362]
[{"$nulls":4},"DSFSGZX","第三方施工专项","RQ_JG_DSFSGZX","面","巡检系统，一个月数据","已对接","2023-08-28",null,"线下"]
["供水设施","基础数据","GS","JS","GX","管线","GS_JS_GX  GS_JS_GX_ATT","线",null,"已对接","2023-06-06","系统","线下","年"]
[{"$nulls":4},"GD","管点","GS_JS_GD","点",null,"已对接","2023-06-06","系统","线下","年"]
[{"$nulls":4},"CZ","厂站","GS_JS_CZ","面",null,"已对接","2023-07-04","台账","填报（水厂、增压泵、二次供水基础信息）","年","部分必给字段内容缺少如使用状态，水源名称，水源类型，取水规模，应急水源名称，应急水源类型，应急取水规模",16]
[{"$nulls":4},"JCD","监测点","GS_JS_JCD","点",null,"已对接","2023-07-04","台账","填报（水厂、增压泵、二次供水监测点信息）","年","标识码，暂由系统生成。",1681]
[{"$nulls":4},"GSYHSL","供水用户数量","GS_JS_GSYHSL",null,null,"已对接","2023-07-04","台账","填报（供水服务用户信息）",null,null,1]
[{"$nulls":4},"GSLXX","供水量信息","GS_JS_GSLXX",null,null,"已对接","2023-07-04","台账","填报（供水量信息）",null,"未给出供水量数据",5]
[{"$nulls":5},"设施改造数据",null,null,null,"已对接","2023-07-04","台账","填报（设施改造数据）"]
[null,"监测数据",null,"JC","JCSB","监测设备","GS_JC_JCSB","-",null,"已对接","2023-07-04","台账","填报（水厂、增压泵、二次供水设备信息）","年","缺少标识码，暂由系统生成。",1701]
[{"$nulls":4},"JCXYZ","监测项阈值","GS_JC_JCXYZ","-","压力流量水质没有报警阈值数据，按照国标保证出厂水达标。","已对接","2023-07-28","物联网平台","接口","天",null,16]
[{"$nulls":4},"SSJC","实时监测","GS_JC_SSJC","-","无数据","实时数据",null,"物联网平台","接口","天"]
[{"$nulls":4},"SPJK","视频监控","GS_JC_SPJK","点","无网络环境、水务集团无视频平台","视频数据"]
[{"$nulls":4},"JCBJ","监测报警","GS_JC_JCBJ","-","压力流量水质没有报警阈值数据，按照国标保证出厂水达标。","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"BJFX","报警分析","GS_JC_BJFX","-","压力流量水质没有报警阈值数据，按照国标保证出厂水达标。","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"BJCZ","报警处置","GS_JC_BJCZ","-","压力流量水质没有报警阈值数据，按照国标保证出厂水达标。","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"JCYJ","监测预警","GS_JC_JCYJ","-","压力流量水质没有报警阈值数据，按照国标保证出厂水达标。","已对接，无法提供","2023-07-28"]
[null,"监管数据",null,"JG","JHXM","计划项目","GS_JG_JHXM","面","监管中心这边没有需求","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"JSXM","建设项目","GS_JG_JSXM","面","监管中心这边没有需求","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"GWFXHCZXX","管网风险&处置信息","GS_JG_GWFXHCZXX",null,null,"已对接","2023-09-28",{"$nulls":4},3]
[{"$nulls":4},"LJGWGZLSQK","老旧管网改造落实情况","GS_JG_LJGWGZLSQK",null,null,"已对接","2023-09-28",{"$nulls":4},1]
[{"$nulls":4},"WXD","维修点","GS_JG_WXD","点","与突发事件抢修、停水影响区域合并，暂无数据","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"TSYXQY","停水影响区域","GS_JG_TSYXQY","面","与突发事件抢修、维修点合并，暂无数据","已对接，无法提供","2023-07-28"]
[{"$nulls":4},"RCWHWX","日常维护维修","GS_JG_RCWHWX","-","有数据对接","已对接","2023-06-15",null,null,null,"缺少标识码、处置结果、处置日期、处置人员、联系电话、养护单位、设施权属单位、",13]
[{"$nulls":4},"TFSJQX","突发事件抢修","GS_JG_TFSJQX","-","与停水影响区域、维修点合并，暂无数据","已对接","2023-06-15",null,null,null,"缺失必给项标识码、相应级别、现场照片、附件",1]
[{"$nulls":5},"巡检记录",null,null,null,"已对接","2023-09-28",{"$nulls":4},3]
[{"$nulls":4},"GDJC","管道检测","GS_JC_GDJC","点","有数据对接，已提供数据","已对接","2023-08-01","台账","填报","年","缺少标识码、描述",2]
[{"$nulls":4},"XJXCDSFSGWT","巡检养护第三方施工问题属性结构表","RQ_JG_XJXCDSFSGWT",null,null,"已对接","2023-09-28",{"$nulls":4},3]
[{"$nulls":4},"DSFSGZX","第三方施工专项","GS_JG_DSFSGZX","面","不涉及","已对接，无法提供","2023-07-28"]
["排水设施","基础数据","PS","JS","GX","管线","PS_JS_GX  PS_JS_GX_ATT","线",null,"已对接","2023-06-15","系统","库表","年","管线 缺少必给\n字段： 标识码,埋设类型,要素代码",1535]
[{"$nulls":4},"GD","管点","PS_JS_GD","点",null,"已对接","2023-06-15","系统","库表","年","管点 缺少必给字段：管类代码，要素代码，特征点，附属物，井室代码，旋转角，权属单位，探测单位，探测日期",1191]
[{"$nulls":4},"PK","排口","PS_JS_PK","点",null,"已对接","2023-07-07","系统","库表","年","排口 缺少必给字段：  地表高程，顶部高程，排口尺寸，是否有拍门",38]
[{"$nulls":4},"CZ","厂站","PS_JS_CZ","面","50个污水厂、33个污水主力泵站","已对接","2023-06-29","系统","库表","每月5日","厂站 缺少必给字段：污泥处理设计规模",56]
[{"$nulls":4},"PSFLZDBZD X","排水防涝重点保障对象","PS_JS_PSFLZDBZDX","点",null,"已对接","2023-09-28",{"$nulls":4},16]
[{"$nulls":4},"YLD","易涝点","PS_JS_YLD","点/面",null,"已对接","2023-09-28",{"$nulls":4},16]
[{"$nulls":4},"FLYJZY","防涝应急资源","PS_JS_FLYJZY","点",null,"已对接"]
[{"$nulls":4},"TXSS","调蓄设施","PS_JS_TXSS",null,"无","待对接"]
[{"$nulls":4},"XXTD","行泄通道","PS_JS_XXTD",null,"无","待对接"]
[{"$nulls":4},"PSH","重点排水户","PS_JS_PSH",null,null,"已对接","2023-09-28",{"$nulls":4},2]
[{"$nulls":4},"JLSS","截流设施","PS_JS_JLSS",null,null,"已对接","2023-09-28",{"$nulls":4},14]
[{"$nulls":4},"ZYHD","主要河道","PS_JS_ZYHD",null,null,"已对接","2023-09-28",{"$nulls":4},47]
[{"$nulls":4},"JCD","监测点","PS_JS_JCD","点",null,"已对接","2023-07-07","系统","库表","每月5日","监测点 缺少必给字段：标识码",3]
[null,"监测数据",null,"JC","JCSB","监测设备","PS_JC_JCSB","-",null,"已对接","2023-07-07","系统","库表","每月5日","监测设备 缺少必给字段：标识码",3]
[{"$nulls":4},"JCXYZ","监测项阈值","PS_JC_JCXYZ","-",null,"已对接","2023-09-28",{"$nulls":4},3]
[{"$nulls":4},"SSJC","实时监测","PS_JC_SSJC","-",null,"已对接","2023-07-07","系统","库表","小时",null,158336]
[{"$nulls":4},"SPJK","视频监控","PS_JC_SPJK","点",null,"已对接","2023-09-28",{"$nulls":4},5]
[{"$nulls":4},"YLDJSSJ","易涝点积水事件","PS_JC_YLDJSSJ",null,null,"已对接","2023-09-28",{"$nulls":4},16]
[{"$nulls":4},"JCBJ","监测报警","PS_JC_JCBJ","-","暂无法提供","已对接，暂无数据","2023-08-02"]
[{"$nulls":4},"BJFX","报警分析","PS_JC_BJFX","-","暂无法提供","已对接，暂无数据","2023-08-02"]
[{"$nulls":4},"BJCZ","报警处置","PS_JC_BJCZ","-","暂无法提供","已对接，暂无数据","2023-08-02"]
[{"$nulls":4},"JCYJ","监测预警","PS_JC_JCYJ","-","暂无法提供","已对接，暂无数据","2023-08-02"]
[null,"监管数据",null,"JG","JHXM","计划项目","PS_JG_JHXM","面","暂无法提供","无法提供"]
[{"$nulls":4},"JSXM","建设项目","PS_JG_JSXM","面","暂无法提供","无法提供"]
[{"$nulls":4},"QXQXD","抢修抢险点","PS_JG_QXQXD","点",null,"已对接","2023-08-31",{"$nulls":4},2]
[{"$nulls":4},"QXQXQY","抢修抢险区域","PS_JG_QXQXQY","面",null,"已对接","2023-08-31",{"$nulls":4},2]
[{"$nulls":4},"RCWHWX","日常维护维修","PS_JG_RCWHWX","-",null,"已对接","2023-08-31",{"$nulls":4},2]
[{"$nulls":4},"TFSJQX","突发事件抢修","PS_JG_TFSJQX","-",null,"已对接","2023-08-31",null,null,null,"缺失必给项附件",162]
[{"$nulls":4},"YHJL","养护记录","PS_JG_YHJL","-",null,"已对接","2023-08-31",{"$nulls":4},2]
[{"$nulls":4},"XJJL","巡检记录","PS_JG_XJJL","-",null,"已对接","2023-08-31",null,null,null,"缺失必给项附件",108]
[{"$nulls":4},"JCJQXJC","检查井缺陷检测","PS_JG_JCJQXJC","点",null,"待对接","下周三"]
[{"$nulls":4},"YSFXGK","雨水风险管控","PS_JG_YSFXGK",null,null,"已对接","2023-09-28",{"$nulls":4},16]
[{"$nulls":4},"XJXCDSFSGWT","巡检养护第三方施工问题","PS_JG_XJXCDSFSGWT",null,null,"已对接","2023-08-31",null,null,null,"缺失必给项巡检养护标识码",3]
[{"$nulls":4},"LJGWGZJD","老旧管网改造进度相关结构表","PS_JG_LJGWGZJD",null,null,"已对接","2023-09-28",{"$nulls":4},2]
[{"$nulls":4},"GDQXJC","管道缺陷检测","PS_JC_GDQXJC","点",null,"已对接","2023-06-15","系统","库表","每月5日","管道缺陷检测 缺少必给\n字段：行政区划代码，检测人，联系电话，检测方法，检测方向，封堵情况，影像文件，填报单位，填报日期",10]
[{"$nulls":4},"DSFSGZX","第三方施工专项","PS_JG_DSFSGZX","面",null,"已对接","2023-08-31",{"$nulls":4},2]
["道路设施","基础数据","DL","JS","CSDL","城市道路","DL_JS_CSDL","面",null,"已对接","2023-07-10","台账","文档",null,"缺少行政区划代码、道路等级、管理分类、养护等级、道路长度、道路面积、管理单位、养护单位、灯杆类型、光源类型、空间信息",197]
[{"$nulls":4},"DLFSSS","道路附属设施","DL_JS_DLFSSS",null,null,"已对接","2023-09-20",{"$nulls":4},197]
[{"$nulls":4},"SD","隧道","DL_JS_SD","面",null,"已对接","2023-07-10","台账","文档",null,null,5]
[null,"监测数据",null,"JC","SPJK","视频监控","DL_JC_SPJK","点","公安有视频设备信息","已对接","2023-09-20"]
[null,"监管数据",null,"JG","JHXM","计划项目","DL_JG_JHXM","面"]
[{"$nulls":4},"JSXM","建设项目","DL_JG_JSXM","面"]
[{"$nulls":4},"RCWHWX","日常维护维修","DL_JG_RCWHWX","-","平台建设后有数据"]
[{"$nulls":4},"TFSJQX","突发事件抢修","DL_JG_TFSJQX","-"]
[{"$nulls":4},"YHJL","养护记录","DL_JG_YHJL","-"]
[{"$nulls":4},"XJJL","巡检记录","DL_JG_XJJL","-"]
[{"$nulls":4},"YHWX","道路养护维修","DL_JG_YHWX",null,null,"已对接","2023-09-20",{"$nulls":4},198]
[{"$nulls":4},"DLTXFX","道路塌陷风险","DL_JC_DLTXFX","面","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},190]
[{"$nulls":4},"DLTXYH","道路塌陷隐患","DL_JC_DLTXYH","面","目前没有数据，后面系统建设完成会有。","已对接","2023-09-20"]
[{"$nulls":4},"DLTXSG","道路塌陷事故","DL_JC_DLTXSG","点","业务上没有数据","已对接","2023-09-20"]
[{"$nulls":4},"DQJC","定期检测","DL_JG_DQJC","-"]
[{"$nulls":4},"JCBHXX","道路检查病害信息","DL_JG_JCBHXX",null,"平台建设后有数据","已对接","2023-09-20",{"$nulls":4},198]
[{"$nulls":4},"XJXCDSFSGWT","巡检养护第三方施工问题属性结构表","DL_JG_XJXCDSFSGWT",null,"业务上没有数据","已对接","2023-09-20"]
[{"$nulls":4},"DSFSGZX","第三方施工专项","DL_JG_DSFSGZX","面","业务上没有数据","已对接","2023-09-20"]
["桥梁设施","基础数据","QL","JS","QL","桥梁","QL_JS_QL","面",null,"已对接","2023-07-10","台账","文档",null,null,624]
[{"$nulls":4},"JCD","监测点","QL_JS_JCD","点","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},349]
[null,"监测数据",null,"JC","JCSB","监测设备","QL_JC_JCSB","-","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},349]
[{"$nulls":4},"JCXYZ","监测项阈值","QL_JC_JCXYZ","-","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},645]
[{"$nulls":4},"SSJC","实时监测","QL_JC_SSJC","-"]
[{"$nulls":4},"SPJK","视频监控","QL_JC_SPJK","点"]
[{"$nulls":4},"JCBJ","监测报警","QL_JC_JCBJ","-"]
[{"$nulls":4},"BJFX","报警分析","QL_JC_BJFX","-"]
[{"$nulls":4},"BJCZ","报警处置","QL_JC_BJCZ","-"]
[{"$nulls":4},"JCYJ","监测预警","QL_JC_JCYJ","-"]
[{"$nulls":4},"SJFXBG","数据分析报告","QL_JC_SJFXBG","-"]
[null,"监管数据",null,"JG","JHXM","计划项目","QL_JG_JHXM","面","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},43]
[{"$nulls":4},"JSXM","建设项目","QL_JG_JSXM","面","有数据，手工录入","已对接","2023-09-20",{"$nulls":4},43]
[{"$nulls":4},"RCWHWX","日常维护维修","QL_JG_RCWHWX","-"]
[{"$nulls":4},"TFSJQX","突发事件抢修","QL_JG_TFSJQX","-"]
[{"$nulls":4},"YHJL","养护记录","QL_JG_YHJL","-"]
[{"$nulls":4},"XJJL","巡检记录","QL_JG_XJJL","-"]
[{"$nulls":4},"fxpg","桥梁风险评估信息","ql_jg_fxpg",null,"有数据，手工录入","已对接","2023-09-20",{"$nulls":4},65]
[{"$nulls":4},"DQJC","定期检测","QL_JG_DQJC","-"]
["综合管线","基础数据","ZH","JS","GX","管线","ZH_JS_GX","线","已对接燃气，供水部分数据","已对接","2023-06-09"]
[{"$nulls":4},"GD","管点","ZH_JS_GD","点","已对接燃气，供水部分数据","已对接","2023-06-09"]
[null,"监管数据",null,"JG","JHXM","计划项目","ZH_JG_JHXM","面",null,"待对接"]
[{"$nulls":4},"JSXM","建设项目","ZH_JG_JSXM","面",null,"待对接"]
[{"$nulls":4},"GXGTJL","管线供图记录","ZH_JG_GXGTJL",null,null,"已对接","2023-09-22",{"$nulls":4},2]
[{"$nulls":4},"FXJL","放线记录","ZH_JG_FXJL",null,null,"已对接","2023-09-22",{"$nulls":4},3]
[{"$nulls":4},"YXJL","验线记录","ZH_JG_YXJL",null,null,"已对接","2023-09-22",{"$nulls":4},3]
[{"$nulls":4},"JGCGHJJL","竣工成果汇交记录","ZH_JG_JGCGHJJL",null,null,"已对接","2023-09-22",{"$nulls":4},3]
[{"$nulls":4},"JHFXYH","交互风险隐患","ZH_JG_JHFXYH","点",null,"待对接"]
[{"$nulls":4},"GHPHGL","规划批后管理","ZH_JG_GHPHGL","面",null,"已对接","2023-09-22",{"$nulls":4},3]
[{"$nulls":4},"DSFSGZX","第三方施工专项","ZH_JG_DSFSGZX","面",null,"待对接"]
["第三方施 工","监管数据","SG","JG","DSFSGXMXX","第三方施工项目信息","SG_JG_DSFSGXMXX","面","住建局先提供部分离线数据","已对接","2023-06-19","台账","填报",null,"项目信息：必给字段缺失：标识码，所在街道，施工深度",1271]
[{"$nulls":4},"DSFSGSQGL","第三方施工事前管理","SG_JG_DSFSGSQGL","面","住建局","已对接","2023-06-19"]
[{"$nulls":4},"DSFSGPHSJ","第三方施工破坏事件","SG_JG_DSFSGPHSJ","点","待业务系统建成后可提供","已对接","2023-06-19"]
[{"$nulls":4},"DSFSGPHCZ JG","第三方施工破坏处置结果","SG_JG_DSFSGPHCZ JG","-","待业务系统建成后可提供","已对接","2023-06-19"]
[{"$nulls":4},"DSFSGLHCJ","第三方施工联合惩戒","SG_JG_DSFSGLHCJ","-","待业务系统建成后可提供","已对接","2023-06-19"]
[{"$nulls":4},"DXDAALK","第三方施工典型档案案例库","SG_JG_DXDAALK",null,"待业务系统建成后可提供","已对接","2023-09-20"]
[{"$nulls":4},"JXBAXX","第三方施工机械备案信息","SG_JG_JXBAXX",null,"待业务系统建成后可提供","已对接","2023-09-20"]
[{"$nulls":4},"QSDWQR","权属单位确认信息","SG_JG_QSDWQR",{"$nulls":8},8]
[{"$nulls":4},"SPJK","视频监控","SG_JC_SPJK",null,null,"已对接","2023-09-20",{"$nulls":4},1]
[{"$nulls":4},"SFJDFB","四方交底记录附表","SG_JG_SFJDFB",null,null,"已对接","2023-09-20",{"$nulls":4},4]
[{"$nulls":4},"SFJDECFH","现场交底管线二次复核记录","SG_JG_SFJDECFH",null,null,"已对接","2023-09-20",{"$nulls":4},1]
[{"$nulls":4},"SFJDBHFA","现场交底保护方案","SG_JG_ SFJDBHFA",null,null,"已对接","2023-09-20",{"$nulls":4},2]
[{"$nulls":4},"SFJDPZJHJL","四方交底旁站监护记录","SG_JG_SFJDPZJHJL",null,null,"已对接","2023-09-20",{"$nulls":4},5]
[{"$nulls":4},"SFJDPZJHJLMX","四方交底旁站监护记录明细","SG_JG_SFJDPZJHJLMX",null,null,"已对接","2023-09-20",{"$nulls":4},5]
[null,"监测数据",null,"JC","JCSB","监测设备","SG_JC_JCSB",null,null,"已对接","2023-09-20",{"$nulls":4},1]
[{"$nulls":4},"JCSS","监测设施","SG_JC_JCSS"]
[{"$nulls":4},"JCD","监测点","SG_JS_JCD",null,"待业务系统建成后可提供","已对接","2023-09-20"]
[{"$nulls":4},"JCXYZ","监测项阈值","SG_JC_JCXYZ",null,"待业务系统建成后可提供","已对接","2023-09-20"]
["注： 第三方施工项目信息范围为四方交底红线范围。",{"$nulls":8},"待对接"]
["综合应用","基础数据","ZY","JS","bncs","避难场所","zy_js_bncs",null,null,"已对接","2023-09-26",{"$nulls":4},2]
[{"$nulls":4},"yjzj","应急专家","zy_js_yjzj",null,null,"待对接"]
[{"$nulls":4},"ck","仓库信息","zy_js_ck",null,null,"待对接"]
[{"$nulls":4},"yjwz","应急物资","zy_js_yjwz",null,null,"已对接","2023-09-26",{"$nulls":4},2]
[{"$nulls":4},"jydw","救援队伍","zy_js_jydw",null,null,"待对接"]
[{"$nulls":4},"ylwsjg","医疗卫生机构","zy_js_ylwsjg",null,null,"已对接","2023-09-26",{"$nulls":4},2]
[{"$nulls":4},"zdwxy","重大危险源","zy_js_zdwxy",null,null,"待对接"]
[{"$nulls":4},"yjya","应急预案","zy_js_yjya",null,null,"待对接"]

{"sheet":"燃气分类","index":1,"n_rows":484,"n_cols":13,"rows_kept":484,"cut":false,"hidden":false,"merged":[[0,0,0,1],[2,0,398,0],[2,1,118,1],[119,1,220,1],[221,1,398,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[11,5,12,5],[27,5,28,5],[0,6,1,6],[11,6,12,6],[27,6,28,6],[0,7,1,7],[11,7,12,7],[27,7,28,7],[0,8,1,8],[0,9,1,9],[11,9,12,9],[27,9,28,9],[92,9,94,9],[292,9,293,9],[320,9,322,9],[0,10,1,10],[11,10,12,10],[27,10,28,10],[0,11,1,11],[70,12,88,12],[89,12,109,12],[110,12,118,12],[119,12,133,12],[272,12,285,12],[286,12,301,12],[317,12,331,12]]}
["数据分类",null,"中文表名","表名","要素类型","中文名","字段名","数据类型","长度","值域及说明","约束条件段 （M 为必填项、O 为选填项、C 为条件必填字段）","备注"]
["大类","一级"]
["燃气设施","基础数据","管线","RQ_JS_GX","线","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"管线","RQ_JS_GX","线","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"管线","RQ_JS_GX","线","管类代码","GLDM","字符型",8,"管线类型代码(如“RQ”)","M"]
[null,null,"管线","RQ_JS_GX","线","起点点号","QDDH","字符型",14,"-","M"]
[null,null,"管线","RQ_JS_GX","线","终点点号","ZDDH","字符型",14,"-","M"]
[null,null,"管线","RQ_JS_GX","线","起点高程","QDGC","浮点型",6.2,"单位：米","M"]
[null,null,"管线","RQ_JS_GX","线","终点高程","ZDGC","浮点型",6.2,"单位：米","M"]
[null,null,"管线","RQ_JS_GX","线","起点埋深","QDMS","浮点型",6.2,"起点埋深/架空高度，单位：米","M"]
[null,null,"管线","RQ_JS_GX","线","终点埋深","ZDMS","浮点型",6.2,"终点埋深/架空高度，单位：米","M"]
[null,null,"管线","RQ_JS_GX","线","埋设类型","MSLX","整型",null,"0(直埋)/1(矩形管沟)/2(拱形管 沟 )/3( 管 块 )/4( 管 埋 )/5( 架 空)/6(井内连线)/7(顶管)","M"]
[null,null,"管线","RQ_JS_GX","线",null,null,null,"-"]
[null,null,"管线","RQ_JS_GX","线","材质","CZ","字符型",8,"-","M"]
[null,null,"管线","RQ_JS_GX","线","管径","GJ","字符型",15,"断面尺寸(宽 X 高)或者管径","M"]
[null,null,"管线","RQ_JS_GX","线","压力","YL","字符型",4,"燃气管道压力，排水是否有压","M"]
[null,null,"管线","RQ_JS_GX","线","要素代码","YSDM","字符型",10,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
[null,null,"管线","RQ_JS_GX","线","所在道路","SZDL","字符型",50,"-","O"]
[null,null,"管线","RQ_JS_GX","线","权属单位","QSDW","字符型",100,"单位名称","O"]
[null,null,"管线","RQ_JS_GX","线","建设年代","JSND","字符型",10,"如：“1991”","O"]
[null,null,"管线","RQ_JS_GX","线","探测单位","TCDW","字符型",100,"单位名称","O"]
[null,null,"管线","RQ_JS_GX","线","探测日期","TCRQ","日期型","-","-","O"]
[null,null,"管线","RQ_JS_GX","线","使用状态","SYZT","整型","-","1(待投用)/2(投用中)/3(检修中) /4(废弃)","O"]
[null,null,"管线","RQ_JS_GX","线","数据来源","SJLY","字符型",255,"探测/竣测/图解/整合/权属单位 提供","O"]
[null,null,"管线","RQ_JS_GX","线","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"通用表标识码","TYBBSM","字符型",32,"关联管线通用表标识码","M"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"管道级别","GDJB","整型",null,"1(高压 A)/2(高压 B)/3(次高压 A)/4(次高压 B)/5(中压 A)/6(中压 B)/7(低压)","M"]
[null,null,"管线明细","RQ_JS_GX_ATT",{"$nulls":4},"-"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"管线名称","GXMC","字符型",32,"权属单位对该段管线的命名","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"当前介质","DQJZ","字符型",8,"当前管道内充满或者主要输送功 能的介质， 例如燃气管道通气前介 质为氮气","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"保护材质","BHCZ","字符型",15,"-","M"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"设计压力","SJYL","字符型",10,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"风险等级","FXDJ","字符型",32,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"运行压力","YXYL","字符型",10,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"通气日期","TQRQ","日期型","-","-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"建设单位","JSDW","字符型",100,"单位名称","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"生产厂家","SCCJ","字符型",100,"管道生产厂家名称","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"防腐形式","FFXS","字符型",12,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"腐蚀情况","FSQK","字符型",12,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"接口方式","JKFS","字符型",12,"-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"路面性质","LMXZ","整型","-","1(水泥)/2(柏油)/3(土路)/4(弹 石 )/5( 绿 化 地 )/6( 人 行 道 板)/7(农田)","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"最近改造时间","ZJGZSJ","日期型","-","-","O"]
[null,null,"管线明细","RQ_JS_GX_ATT",null,"备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"管点","RQ_JS_GD","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"管点","RQ_JS_GD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"管点","RQ_JS_GD","点","管类代码","GLDM","字符型",8,"管点类型代码(如“RQ” )","M"]
[null,null,"管点","RQ_JS_GD","点","探测点号","TCDH","字符型",16,"外业点号，测区内唯一","M"]
[null,null,"管点","RQ_JS_GD","点","要素代码","YSDM","字符型",10,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
[null,null,"管点","RQ_JS_GD","点","地面高程","DMGC","浮点型",7.3,"单位：米","M"]
[null,null,"管点","RQ_JS_GD","点","特征点","TZD","字符型",15,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
[null,null,"管点","RQ_JS_GD","点","附属物","FSW","字符型",15,"如调压箱、阀门等， 参照 DGJ32/TJ 187《江苏省城市地下管线数据标 准》","M"]
[null,null,"管点","RQ_JS_GD","点","所在道路","SZDL","字符型",50,"-","M"]
[null,null,"管点","RQ_JS_GD","点","井室代码","JSDM","整型","-","填写 3 位井室代码","M"]
[null,null,"管点","RQ_JS_GD","点","旋转角","XZJ","浮点型",8.3,"按平面直角坐标系弧度表示","M"]
[null,null,"管点","RQ_JS_GD","点","井深","JS","浮点型",6.2,"当探测点号为检修井时， 单位： 米","O"]
[null,null,"管点","RQ_JS_GD","点","井盖形状","JGXZ","字符型",10,"圆形/矩形","O"]
[null,null,"管点","RQ_JS_GD","点","井盖材质","JGCZ","字符型",10,"-","O"]
[null,null,"管点","RQ_JS_GD","点","井盖直径","JGZJ","浮点型",5,"单位：米","O"]
[null,null,"管点","RQ_JS_GD","点","井盖长","JGC","浮点型",5,"管线的主线方向井盖长， 单位： 米","O"]
[null,null,"管点","RQ_JS_GD","点","井盖宽","JGK","浮点型",5,"垂直管线的主线方向井盖宽度， 单 位：米","O"]
[null,null,"管点","RQ_JS_GD","点","检修井材质","JXJCZ","字符型",10,"水泥/砖","O"]
[null,null,"管点","RQ_JS_GD","点","井脖深","JBS","浮点型",5.2,"井盖向下的垂直段的距离，单位： 米","O"]
[null,null,"管点","RQ_JS_GD","点","井室直径","JSZJ","浮点型",5,"井室是柱体时填写，单位：毫米","O"]
[null,null,"管点","RQ_JS_GD","点","建设年代","JSND","字符型",10,"如：“1991”","O"]
[null,null,"管点","RQ_JS_GD","点","权属单位","QSDW","字符型",100,"单位名称","M"]
[null,null,"管点","RQ_JS_GD","点","探测单位","TCDW","字符型",100,"单位名称","M"]
[null,null,"管点","RQ_JS_GD","点","探测日期","TCRQ","日期型","-","-","M"]
[null,null,"管点","RQ_JS_GD","点","数据来源","SJLY","字符型",255,"探测/竣测/图解/整合/权属单位 提供","O"]
[null,null,"管点","RQ_JS_GD","点","备注","BZ","字符型",255,"非正常埋设的需要备注","O"]
[null,null,"场站","RQ_JS_CZ","面","标识码","BSM","字符型",32,"自动生成，唯一","M","有","1.华润车用气加气站：缺少必给字段：BSM,XZQHDM,CQNL,SJCQL,GZNL\n2.新区储配站信息：缺少必给字段：标识码\n"]
[null,null,"场站","RQ_JS_CZ","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M","无"]
[null,null,"场站","RQ_JS_CZ","面","场站类型","CZLX","字符型",40,"气化站、门站、储配站、加气站、 调压站、瓶装供应站等","M","有"]
[null,null,"场站","RQ_JS_CZ","面","使用状态","SYZT","整型","-","1(待投用 )/2(投用中 )/3( 检 修 中)/4(废弃)","O","调压站投用中"]
[null,null,"场站","RQ_JS_CZ","面","名称","MC","字符型",50,"-","M","有"]
[null,null,"场站","RQ_JS_CZ","面","储气能力","CQNL","字符型",50,"-","M","无"]
[null,null,"场站","RQ_JS_CZ","面","实际储气量","SJCQL","字符型",20,"-","M","无"]
[null,null,"场站","RQ_JS_CZ","面","灌装能力","GZNL","字符型",50,"-","M"]
[null,null,"场站","RQ_JS_CZ","面","年供气量","NGQL","浮点型",10.2,"单位：万立方米","M"]
[null,null,"场站","RQ_JS_CZ","面","小时供应能力","XSGYNL","浮点型",10.2,"单位： 万立方米； 场站类型为门站、 调压站、气化站、加气站时填写","C"]
[null,null,"场站","RQ_JS_CZ","面","重瓶数","ZPS","整型","-","-","O"]
[null,null,"场站","RQ_JS_CZ","面","压力","YL","浮点型",6.2,"单位： MPa；当场站类型为气化站、 门站、储配站、加气站、调压站时 填写，取场站整体运行数据","C","无"]
[null,null,"场站","RQ_JS_CZ","面","流量","LL","浮点型",10.2,"单位： m3/h；当场站类型为门站、调 压站时填写，取场站整体运行数据","C","无"]
[null,null,"场站","RQ_JS_CZ","面","液位","YW","浮点型",10.2,"单位： mm ；当场站类型为储配站、 LNG 站时填写，取场站整体运行数 据","C","无"]
[null,null,"场站","RQ_JS_CZ","面","温度","WD","浮点型",6.2,"单位： ℃； 当场站类型为门站、储 配站、加气站、调压站、气化站时 填写，取场站整体运行数据","C","无"]
[null,null,"场站","RQ_JS_CZ","面","竣工日期","JGRQ","日期型","-","-","O","无"]
[null,null,"场站","RQ_JS_CZ","面","地址","DZ","字符型",255,"-","O","无"]
[null,null,"场站","RQ_JS_CZ","面","建设单位","JSDW","字符型",100,"单位名称","O","无"]
[null,null,"场站","RQ_JS_CZ","面","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","标识码","BSM","字符型",32,"自动生成，唯一","M",null,"1.燃气用户：缺少必给字段：标识码，启用日期，气源种类，液化气瓶种类，液化气存瓶数，供气单位，是否重点用气场所，报警器，是否有切断装置"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","用户类型","YHLX","整型","-","1(居民)/2(非居民)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)",{"$nulls":4},"当用户类型为非居民时填写； 1(餐 饮业)/2(工业)/3(住宿业)/4(商 贸 服 务 业 )/5( 教 育 )/6( 医 疗)/7(社会保障)/8(机关事业单 位)"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","非居民用户类型","FJMYHLX","整型",null,null,"C"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)",null,null,null,"-"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","用户信息","YHXX","字符型",20,"-","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","详细地址","XXDZ","字符型",255,"-","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","所在街道和社区","SZJDHSQ","字符型",50,"-","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","启用日期","QYRQ","日期型","-","-","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","用气范围","YQFW","字符型",255,"-","O"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","气源种类","QYZL","整型","-","1(天然气)/2(液化石油气)/3(其 它)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","液化气瓶种类","YHQPZL","整型","-","1(YSP12)/2(YSP23.5)/3(YSP35.5 )/4(YSP118)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","液化气存瓶数","YHQCPS","整型","-","单位：瓶","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","用气规模","YQGM","浮点型",10.2,"单位：立方米/年或公斤/年","O"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","供气单位","GQDW","字符型",100,"单位名称","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","设备设施情况","SBSSQK","字符型",255,"-","O"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","是否重点用气场所","SFZDYQCS","布尔型","-","0(否)/1(是)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","报警器","BJQ","整型","-","1(家用报警器)/2(商用报警器)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","是否有切断装置","SFYQDZZ","布尔型","-","0(否)/1(是)","M"]
[null,null,"燃气用户","RQ_JS_RQYH","- (居民用 户) /点(非 居民用户)","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"监测点","RQ_JS_JCD","点","标识码","BSM","字符型",32,"自动生成，唯一","M","无","缺少标识码"]
[null,null,"监测点","RQ_JS_JCD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M","无"]
[null,null,"监测点","RQ_JS_JCD","点","点位名称","DWMC","字符型",64,"-","M","有"]
[null,null,"监测点","RQ_JS_JCD","点","设施名称","SSMC","字符型",64,"基础设施名称","O","无"]
[null,null,"监测点","RQ_JS_JCD","点","设施编码","SSBM","字符型",17,"被监测设施编码","M","无"]
[null,null,"监测点","RQ_JS_JCD","点","监测位置","JCWZ","字符型",200,"-","O","无"]
[null,null,"监测点","RQ_JS_JCD","点","高程","GC","浮点型",7.3,"单位：米","O","无"]
[null,null,"监测点","RQ_JS_JCD","点","高程基准","GCJZ","字符型",32,"-","O","无"]
[null,null,"监测点","RQ_JS_JCD","点","备注","BZ","字符型",255,"相关事项说明","O","无"]
[null,"监测数据","监测设备","RQ_JC_JCSB","-","标识码","BSM","字符型",32,"自动生成，唯一","M","无","缺少点位标识码、设备类型、设备名称、检测指标、采集频率、上传频率、设备状态"]
[null,null,"监测设备","RQ_JC_JCSB","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","设备名称","SBMC","字符型",50,"-","M","有"]
[null,null,"监测设备","RQ_JC_JCSB","-","设备型号","SBXH","字符型",32,"-","O","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M","有"]
[null,null,"监测设备","RQ_JC_JCSB","-","采集频率","CJPL","字符型",32,"采集间隔时间，单位：分钟","M","有"]
[null,null,"监测设备","RQ_JC_JCSB","-","上传频率","SCPL","字符型",32,"上传间隔时间，单位：分钟","M","有"]
[null,null,"监测设备","RQ_JC_JCSB","-","设备状态","SBZT","整型","-","1( 未 使 用 )/2( 正 常 )/3( 试 运 行)/4(故障)/5(维修)/6(报废)","M","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","厂商名称","CSMC","字符型",50,"-","O","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","相对高度","XDGD","浮点型",7.3,"如液位计相对井口高度","O","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","安装时间","AZSJ","日期型","-","-","O","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","安装维护单位","AZWHDW","字符型",100,"单位名称","O","无"]
[null,null,"监测设备","RQ_JC_JCSB","-","供电方式","GDFS","字符型",32,"-","O","有-电池"]
[null,null,"监测设备","RQ_JC_JCSB","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M","无"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M","无"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M","无"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M","有"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","报警阈值","BJYZ","浮点型",10.3,"-","M","有"]
[null,null,"监测项阈值","RQ_JC_JCXYZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"实时监测","RQ_JC_SSJC","-","标识码","BSM","字符型",32,"自动生成，唯一","M","无"]
[null,null,"实时监测","RQ_JC_SSJC","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M","无"]
[null,null,"实时监测","RQ_JC_SSJC","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M","无"]
[null,null,"实时监测","RQ_JC_SSJC","-","监测值","JCZ","浮点型",18.2,"监测特征值","M","有"]
[null,null,"实时监测","RQ_JC_SSJC","-","监测采集时间","JCCJSJ","时间日期型","-","-","M","无"]
[null,null,"实时监测","RQ_JC_SSJC","-","监测上报时间","JCSBSJ","时间日期型","-","-","M","有"]
[null,null,"实时监测","RQ_JC_SSJC","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"视频监控","RQ_JC_SPJK","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","设备名称","SBMC","字符型",50,"视频设备名称","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","安装地址","AZDZ","字符型",255,"-","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","监控对象","JKDX","字符型",255,"-","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","设备型号","SBXH","字符型",255,"-","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","生产厂家","SCCJ","字符型",100,"厂家名称","O"]
[null,null,"视频监控","RQ_JC_SPJK","点","产权单位","CQDW","字符型",100,"单位名称","M"]
[null,null,"视频监控","RQ_JC_SPJK","点","视频地址","SPDZ","字符型",255,"可以直接播放的视频流 URL 地址， 通常由视频联网平台提供","O"]
[null,null,"视频监控","RQ_JC_SPJK","点","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"监测报警","RQ_JC_JCBJ","-","标识码","BSM","字符型",32,"自动生成，唯一","M","无"]
[null,null,"监测报警","RQ_JC_JCBJ","-","报警名称","BJMC","字符型",50,"-","M","有"]
[null,null,"监测报警","RQ_JC_JCBJ","-","报警编号","BJBH","字符型",64,"程序自动生成，唯一","M","无"]
[null,null,"监测报警","RQ_JC_JCBJ","-","点位标识码","DWBSM","字符型",64,"关联监测点标识码","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","监测报警指标","JCBJZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","当前报警级别","DQBJJB","字符型",16,"一级/二级/三级/四级；城市内涝 场景非必填","C"]
[null,null,"监测报警","RQ_JC_JCBJ","-","初次报警时间","CCBJSJ","时间日期型","-","-","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","初次报警值","CCBJZ","浮点型",18.2,"初次触发报警的监测值","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","当前报警时间","DQBJSJ","时间日期型","-","-","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","当前报警值","DQBJZ","浮点型",18.2,"当前触发报警的监测值","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","累计报警频次","LJBJPC","整型","-","本次报警在报警解除之间所产生 的报警次数","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","报警是否解除","BJSFJC","布尔型","-","0(否)/1(是)","M"]
[null,null,"监测报警","RQ_JC_JCBJ","-","报警解除时间","BJJCSJ","时间日期型","-","当报警确认解除时， 填写报警解除 时间","C"]
[null,null,"监测报警","RQ_JC_JCBJ","-","报警解除说明","BJJCSM","字符型",255,"当报警确认解除时， 填写报警解除 说明","C"]
[null,null,"监测报警","RQ_JC_JCBJ","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"报警分析","RQ_JC_BJFX","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","报警编号","BJBH","字符型",64,"见监测报警属性表","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","报警点位位置","BJDWWZ","字符型",255,"-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","现场排查人员","XCPCRY","字符型",32,"-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","现场排查人员手机","XCPCRYSJ","字符型",15,"-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","到达现场时间","DDXCSJ","时间日期型","-","-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","现场状况描述","XCZKMS","变长字符型","-","-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","值守人员","ZSRY","字符型",32,"系统值守人员","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","值守人员手机","ZSRYSJ","字符型",15,"-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","值守人员单位","ZSRYDW","字符型",100,"单位名称","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","值守人员分析简述","ZSRYFXJS","字符型",500,"-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","现场人员分析报告","XCRYFXBG","二进制型","-","-","O"]
[null,null,"报警分析","RQ_JC_BJFX","-","值守人员分析时间","ZSRYFXSJ","时间日期型","-","-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","分析内容","FXNR","变长字符型","-","-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","现场图片视频文件","XCTPSPWJ","二进制型","-","现场图片、视频文件","O"]
[null,null,"报警分析","RQ_JC_BJFX","-","更新时间","GXSJ","时间日期型","-","-","M"]
[null,null,"报警分析","RQ_JC_BJFX","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"报警处置","RQ_JC_BJCZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","报警编号","BJBH","字符型",64,"关联监测报警表","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","处置时间","CZSJ","时间日期型","-","-","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","处置内容","CZNR","变长字符型","-","-","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","处置报告","CZBG","二进制型","-","-","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","记录人员","JLRY","字符型",32,"-","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","更新时间","GXSJ","时间日期型","-","-","M"]
[null,null,"报警处置","RQ_JC_BJCZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"监测预警","RQ_JC_JCYJ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警名称","YJMC","字符型",50,"-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警设施名称","YJSSMC","字符型",50,"-","O"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警设施编号","YJSSBH","字符型",64,"-","O"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警类型","YJLX","整型","-",null,"M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警地址","YJDZ","字符型",255,"-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警级别","YJJB","整型","-","1(一级)/2(二级)/3(三级)/4(四级)","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警状态","YJZT","整型","-","1(发布)/2(处置)/3(解除)","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警生成时间","YJSCSJ","时间日期型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警上报时间","YJSBSJ","时间日期型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警简述","YJJS","变长字符型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","预警报告","YJBG","二进制型","-","-","O"]
[null,null,"监测预警","RQ_JC_JCYJ","-","研判分析","YPFX","变长字符型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","分析报告","FXBG","二进制型","-","-","O"]
[null,null,"监测预警","RQ_JC_JCYJ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)/3(误报)","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","处置人","CZR","字符型",32,"-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","处置时间","CZSJ","时间日期型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","处置建议","CZJY","变长字符型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","处置报告","CZBG","二进制型","-","-","M"]
[null,null,"监测预警","RQ_JC_JCYJ","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,"监管数据","计划项目","RQ_JG_JHXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","项目名称","XMMC","字符型",255,"-","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","项目内容","XMNR","字符型",255,"-","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","计划年度","JHND","整型","-","如：“2022”","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","项目建设周期","XMJSZQ","整型","-","单位：月","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
[null,null,"计划项目","RQ_JG_JHXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目名称","XMMC","字符型",255,"针对道路是指最新一次改造拓宽 项目","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目代码","XMDM","字符型",50,"固定资产投资审批、核准、备案范 围内的项目引用项目代码","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目编码","XMBM","字符型",32,"非固定资产投资审批、核准、备案 范围内的项目引用项目编码","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目内容","XMNR","字符型",255,"-","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","详细地址","XXDZ","字符型",255,"-","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","立项许可信息","LXXKXX","字符型",255,"立项批复文号","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","规划许可信息","GHXKXX","字符型",255,"建设工程规划许可证号","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","施工许可信息","SGXKXX","字符型",255,"建设工程施工许可证号","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","竣工验收信息","JGYSXX","字符型",255,"-","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","建设单位","JSDW","字符型",100,"单位名称","M"]
[null,null,"建设项目","RQ_JG_JSXM","面","设计单位","SJDW","字符型",100,"单位名称","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","施工单位","SGDW","字符型",100,"单位名称","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","监理单位","JLDW","字符型",100,"单位名称","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","实际开始时间","SJKSSJ","日期型","-","-","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","实际结束时间","SJJSSJ","日期型","-","-","O"]
[null,null,"建设项目","RQ_JG_JSXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","名称","MC","字符型",50,"抢修抢险区域的常用名称","M"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","地址","DZ","字符型",255,"具体位置描述","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","类型","LX","字符型",100,"抢修抢险区域的所属设施类型","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","调查日期","DCRQ","日期型","-","现场调查日期","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","区域情况描述","QYQKMS","字符型",255,"抢修抢险重点区域情况描述","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","填报单位","TBDW","字符型",100,"单位名称","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","填报日期","TBRQ","日期型","-","数据填报日期","O"]
[null,null,"抢修抢险点","RQ_JG_QXQXD","点","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","名称","MC","字符型",50,"抢修抢险区域的常用名称","M"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","地址","DZ","字符型",255,"具体位置描述","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","类型","LX","字符型",100,"抢修抢险区域的所属设施类型","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","调查日期","DCRQ","日期型","-","现场调查日期","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","区域情况描述","QYQKMS","字符型",255,"抢修抢险重点区域情况描述","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","填报单位","TBDW","字符型",100,"单位名称","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","填报日期","TBRQ","日期型","-","数据填报日期","O"]
[null,null,"抢修抢险区域","RQ_JG_QXQXQY","面","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","标识码","BSM","字符型",32,"自动生成，唯一","M",null,"1.维修记录查询：缺少必给字段：标识码，检测方法"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","维护维修内容","WHWXNR","字符型",255,"-","M"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","设备设施","SBSS","字符型",255,"关联设备设施的标识码， 存在多个 设备设施用英文分号“;”分隔","M"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","处理结果","CLJG","字符型",255,"-","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","处理日期","CLRQ","日期型","-","-","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","处理人员","CLRY","字符型",32,"-","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","联系电话","LXDH","字符型",16,"-","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","养护单位","YHDW","字符型",100,"单位名称","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","设施权属单位","SSQSDW","字符型",100,"单位名称","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","检测方法","JCFF","字符型",255,"-","M"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","检测结论","JCJL","字符型",255,"-","M"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","附件","FJ","二进制型","-","-","O"]
[null,null,"日常维护维修","RQ_JG_RCWHWX","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","标识码","BSM","字符型",32,"自动生成，唯一","M",null,"燃气工单抢修信息：缺少必给字段：标识码，行政区划代码，事件名称，响应级别，现场照片，附件"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","事件名称","SJMC","字符型",50,"-","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","事件说明","SJSM","字符型",255,"-","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","地址","DZ","字符型",255,"-","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","关联基础设施","GLJCSS","字符型",32,"燃气/供水/排水/道路/桥梁，存在多 个设备设施用英文分号“;”分隔","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-",{"$nulls":4},"1(一级)/2(二级)/3(三级)/4(四级)； 参照《江苏省突发事件总体应急预 案》中应急响应分级的规定"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","响应级别","XYJB","整型","-",null,"M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","现场照片","XCZP","二进制型","-","-","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","抢修内容","QXNR","字符型",255,"抢修内容及处理方法","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","处理结果","CLJG","字符型",255,"-","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","处理日期","CLRQ","日期型","-","-","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","处理人员","CLRY","字符型",32,"-","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","处理单位","CLDW","字符型",100,"单位名称","O"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","附件","FJ","二进制型","-","-","M"]
[null,null,"突发事件抢修","RQ_JG_TFSJQX","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","巡检对象","XJDX","整型","-","燃 气 、 排 水 设 施 填 写 ； 1( 管 道)/2(场站)/3(用户)/4(其它)","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查单元","JCDY","字符型",255,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查项目","JCXM","字符型",255,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查方法","JCFF","字符型",255,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查内容","JCNR","字符型",255,"-","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查结果","JCJG","字符型",255,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","存在隐患","CZYH","字符型",255,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查日期","JCRQ","时间日期型","-","-","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","检查人员","JCRY","字符型",32,"-","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","设施权属单位","SSQSDW","字符型",100,"单位名称","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","主管单位","ZGDW","字符型",100,"单位名称","O"]
[null,null,"巡检记录","RQ_JG_XJJL","-","附件","FJ","二进制型","-","-","M"]
[null,null,"巡检记录","RQ_JG_XJJL","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","标识码","BSM","字符型",32,"自动生成，唯一","M",null,"阀门隐患已办信息：缺少必给字段：标识码，隐患等级，所属机构，上报人单位"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","隐患描述","YHMS","字符型",255,"-","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点",{"$nulls":4},"1(第三方施工)/2(不满足规范要求 的交叉穿越)/3(违章占压)/4(管网 间距不足)/5(管网老化)/6(管网腐 蚀)/7(液化气瓶隐患)/8(燃气场站 隐患)/9(地质灾害)/10(其它)"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","隐患类型","YHLX","整型",null,null,"M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点",null,null,null,"-"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","隐患等级","YHDJ","字符型",8,"A(重大)/B(一般)","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","隐患点地址","YHDDZ","字符型",255,"-","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","所属机构","SSJG","字符型",64,"-","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","整改状态","ZGZT","整型","-","1(未整改)/2(整改中)/3(已整改)","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","上报人","SBR","字符型",32,"-","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","上报人单位","SBRDW","字符型",100,"单位名称","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","上报时间","SBSJ","日期型","-","-","M"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","整改负责人","ZGFZR","字符型",32,"开始整改时填写","C"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","整改负责人联系 电话","ZGFZRLXDH","字符型",16,"开始整改时填写","C"]
[null,null,"燃气设施隐患","RQ_JC_RQSSYH","点","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查对象","JCDX","字符型",255,"参照 DB32/T 4064《江苏省城镇燃 气安全检查标准》","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","类型","LX","字符型",16,"参照 DB32/T 4064《江苏省城镇燃 气安全检查标准》， 检查项目按 A、 B 两类评定","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查单元","JCDY","字符型",255,"参照 DB32/T 4064《江苏省城镇燃 气安全检查标准》","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查项目","JCXM","字符型",255,"参照 DB32/T 4064《江苏省城镇燃 气安全检查标准》","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查方法","JCFF","字符型",255,"-","O"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查内容","JCNR","字符型",255,"-","O"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查结果","JCJG","字符型",255,"-","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","存在隐患","CZYH","字符型",255,"-","O"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查日期","JCRQ","日期型","-","-","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查人员","JCRY","字符型",32,"-","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","检查单位","JCDW","字符型",100,"单位名称","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","设施权属单位","SSQSDW","字符型",100,"单位名称","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","主管单位","ZGDW","字符型",100,"单位名称","M"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","附件","FJ","二进制型","-","-","O"]
[null,null,"安全专项检查记录","RQ_JG_AQZXJCJL","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","牵头部门","QTBM","字符型",100,"单位名称","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","参检部门","CJBM","字符型",100,"参与检查部门单位名称","O"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","检查日期","JCRQ","日期型","-","-","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","检查项目","JCXM","字符型",255,"-","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","检查内容","JCNR","字符型",255,"-","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","检查结果","JCJG","字符型",255,"-","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","责任单位","ZRDW","字符型",100,"-","C"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","检查人员","JCRY","字符型",32,"-","C"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","现场照片","XCZP","二进制型","-","-","M"]
[null,null,"联合检查记录","RQ_JG_LHJCJL","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改计划名称","ZGJHMC","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改内容","ZGNR","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改位置","ZGWZ","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改图片","ZGTP","二进制型","-","-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","关联设备设施","GLSBSS","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改日期","ZGRQ","日期型","-","-","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改进度","ZGJD","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改结果","ZGJG","字符型",255,"-","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","负责人信息","FZRXX","字符型",255,"-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","整改单位","ZGDW","字符型",100,"单位名称","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","设施权属单位","SSQSDW","字符型",100,"单位名称","M"]
[null,null,"整改记录","RQ_JG_ZGJL","-","行业主管单位","HYZGDW","字符型",100,"单位名称","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","附件","FJ","二进制型","-","-","O"]
[null,null,"整改记录","RQ_JG_ZGJL","-","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","项目名称","XMMC","字符型",255,"-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","项目内容","XMNR","字符型",255,"-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","所在街道","SZJD","字符型",255,"-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","施工项目地址","XXDZ","字符型",255,"-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","计划开始时间","JHKSSJ","日期型","-","-","O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","计划结束时间","JHJSSJ","日期型","-","-","O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","实际开始时间","SJKSSJ","日期型","-","-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","实际结束时间","SJJSSJ","日期型","-","-","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","施工深度","SGSD","浮点型",6.2,"第三方施工开挖最大深度","M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","建设单位","JSDW","字符型",255,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","建设单位负责人","JSDWFZR","字符型",16,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","建设单位负责人联 系电话","JSDWFZRLXDH","字符型",16,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","施工单位","SGDW","字符型",255,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","施工单位负责人","SGDWFZR","字符型",16,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","施工单位负责人联 系电话","SGDWFZRLXDH","字符型",16,null,"M"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","监理单位","JLDW","字符型",255,null,"O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","监理单位负责人","JLDWFZR","字符型",255,null,"O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","监理单位负责人联 系电话","JLDWFZRLXDH","字符型",255,null,"O"]
[null,null,"第三方施工专项","RQ_JG_DSFSGZX","面","备注","BZ","字符型",255,"相关事项说明","O"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"标识码","bsm","字符型",32,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"燃气管网总长度","rqgwzcd","浮点型",12.2,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"低风险长度","dfxcd","浮点型",12.2,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"一般风险长度","ybfxcd","浮点型",12.2,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"较大风险长度","jdfxcd","浮点型",12.2,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"重大风险长度","zdfxcd","浮点型",12.2,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"备注","bz","字符型",255,null,"O"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
[null,null,"燃气风险统计信息表","rq_jg_rqfxtj",null,"同步时间","tbsj","日期型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"标识码","bsm","字符型",32,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"管线id","gxid","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"所属区域","ssqy","字符型",255,null,"O"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"责任单位","zrdw","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单元","pgdy","字符型",100,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"关联管段编号","glgdbh","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单元管道长度","pgdygdcd","浮点型",20,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"风险描述","fxms","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"风险等级","fxdj","整型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"管控状态","gkzt","整型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"风险类型","fxlx","整型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估时间","pgsj","日期型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单位","pgdw","字符型",50,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"地址","dz","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"批次编号","pcbh","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单元名称","pgdymc","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单元位置","pgdywz","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"评估单元唯一标识","pgdywybs","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"可能性等级","knxdj","整型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"后果等级","hgdj","整型",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"管控措施","gkcs","字符型",255,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"空间信息","kjxx","geometry",null,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"更新时间","gxsj","日期型",null,null,"O"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"备注","bz","字符型",255,null,"O"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
[null,null,"风险评估信息表","rq_jg_fxpg",null,"同步时间","tbsj","日期型",null,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"标识码","bsm","字符型",255,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"行政区划代码","xzqhdm","字符型",255,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"填报时间","tibsj","日期型",null,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"计划改造总长","jhgzzc","浮点型",10,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"已改造","ygz","浮点型",10,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"改造中","gzz","浮点型",10,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"未改造","wgz","浮点型",10,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"现有老旧管网总长","xyljgwzc","浮点型",10,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
[null,null,"老旧管网统计表","rq_jg_ljgwtj",null,"同步时间","tbsj","日期型",null,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"标识码","bsm","字符型",32,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"巡检养护标识码","xjyhbsm","字符型",32,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"是否涉及工程机械","sfsjgcjx","布尔型",null,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题分类","wtfl","整型",null,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题描述","wtms","字符型",255,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"检查地址","jcdz","字符型",255,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题上报单位","wtsbdw","字符型",100,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题上报人","wtsbr","字符型",16,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题上报时间","wtsbsj","日期型",null,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题处置单位","wtczdw","字符型",100,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题处置负责人","wtczfzr","字符型",32,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题处置负责人联系电话","wtczfzrlxdh","字符型",16,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题处置时间","wtczsj","日期型",null,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"问题处置简述","wtczjs","字符型",255,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"处置状态","czzt","整型",null,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"处置附件","czfj","二进制型",null,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"现场图片","xctp","二进制型",null,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"备注","bz","字符型",255,null,"O"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"同步时间","tbsj","日期型",null,null,"M"]
[null,null,"巡检养护第三方施工问题属性结构表","rq_jg_xjxcdsfsgwt",null,"空间信息","kjxx","geometry",null,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"标识码","bsm","字符型",32,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"计划内容","jhnr","字符型",255,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"计划开始时间","jhkssj","日期型",null,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"计划结束时间","jhjssj","日期型",null,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"计划数","jhs","整型",32,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"完成数","wcs","整型",32,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"完成率","wcl","浮点型",12.2,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"备注","bz","字符型",255,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
[null,null,"巡检巡查信息表","rq_jg_xjxcjl",null,"同步时间","tbsj","日期型",null,null,"M"]

{"sheet":"供水分类","index":2,"n_rows":334,"n_cols":10,"rows_kept":334,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[2,9,23,9],[24,9,26,9],[27,9,29,9],[37,9,45,9],[46,9,60,9],[200,9,213,9],[214,9,229,9],[230,9,238,9]]}
["中文表名","表名","要素类型","字段中文名","字段名","数据类型","长度","值域及说明","约束条件","备注"]
[]
["厂站","GS_JS_CZ",null,"标识码","BSM","字符型",32,"自动生成，唯一","M","部分必给字段内容缺少如使用状态，水源名称，水源类型，取水规模，应急水源名称，应急水源类型，应急取水规模"]
["厂站","GS_JS_CZ",null,"行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["厂站","GS_JS_CZ",null,"厂站类型","CZLX","字符型",40,"原水厂、自来水厂、增压站、二次 供水泵房等","M"]
["厂站","GS_JS_CZ",null,"使用状态","SYZT","整型","-","1(待投用 )/2(投用中 )/3( 检 修 中)/4(关停)/5(废弃)","M"]
["厂站","GS_JS_CZ",null,"厂站名称","CZMC","字符型",50,"-","M"]
["厂站","GS_JS_CZ",null,"水源名称","SYMC","字符型",50,"-","M"]
["厂站","GS_JS_CZ",null,"水源类型","SYLX","字符型",20,"地表水(长江、太湖、其它湖库、 淮河流域、沂沭泗流域) 、地下水","M"]
["厂站","GS_JS_CZ",null,"取水规模","QSGM","字符型",50,"单位：万立方米/日","M"]
["厂站","GS_JS_CZ",null,"应急水源名称","YJSYMC","字符型",50,"-","M"]
["厂站","GS_JS_CZ",null,"应急水源类型","YJSYLX","字符型",40,"地表水(长江、太湖、其它湖库、 淮河流域、沂沭泗流域) 、地下水","M"]
["厂站","GS_JS_CZ",null,"应急取水规模","YJQSGM","字符型",50,"单位：万立方米/日","M"]
["厂站","GS_JS_CZ",null,"应急取水天数","YJQSTS","整型","-","单位：日","M"]
["厂站","GS_JS_CZ",null,"供水规模","GSGM","字符型",50,"单位：万立方米/日","O"]
["厂站","GS_JS_CZ",null,"供水人口","GSRK","浮点型",8.2,"水厂属性，单位：万人","M"]
["厂站","GS_JS_CZ",null,"供水区域","GSQY","字符型",50,"水厂属性， 供水覆盖范围描述， 供 水区域面积(平方公里)","O"]
["厂站","GS_JS_CZ",null,"处理工艺","CLGY","字符型",50,"-","O"]
["厂站","GS_JS_CZ",null,"投产日期","TCRQ","日期型","-","-","O"]
["厂站","GS_JS_CZ",null,"增压站类型","ZYZLX","字符型",50,"-","O"]
["厂站","GS_JS_CZ",null,"竣工日期","JGRQ","日期型","-","-","O"]
["厂站","GS_JS_CZ",null,"地址","DZ","字符型",255,"-","O"]
["厂站","GS_JS_CZ",null,"建设单位","JSDW","字符型",100,"单位名称","O"]
["厂站","GS_JS_CZ",null,"备注","BZ","字符型",255,"相关事项说明","O"]
["供水服务用户数",null,null,"年份","nf"]
["供水服务用户数",null,null,"居民用户数量","jmyhsl"]
["供水服务用户数",null,null,"非居民用户数量","fjmyhsl"]
["城市供水量信息",null,null,"年月","ny"]
["城市供水量信息",null,null,"月度城市供水量","ydcsgsl"]
["城市供水量信息",null,null,"备注","bz"]
["设施改造数据",null,null,"上报时间"]
["设施改造数据",null,null,"年份（例：2023）"]
["设施改造数据",null,null,"全市当年计划改造供水老旧管网总长"]
["设施改造数据",null,null,"已改造长度"]
["设施改造数据",null,null,"改造中长度"]
["设施改造数据",null,null,"未改造长度"]
["监测点","GS_JS_JCD","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测点","GS_JS_JCD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M","标识码，暂由系统生成。"]
["监测点","GS_JS_JCD","点","点位名称","DWMC","字符型",64,"-","M"]
["监测点","GS_JS_JCD","点","设施名称","SSMC","字符型",64,"基础设施名称","O"]
["监测点","GS_JS_JCD","点","设施编码","SSBM","字符型",17,"被监测设施编码","M"]
["监测点","GS_JS_JCD","点","监测位置","JCWZ","字符型",200,"-","O"]
["监测点","GS_JS_JCD","点","高程","GC","浮点型",7.3,"单位：米","O"]
["监测点","GS_JS_JCD","点","高程基准","GCJZ","字符型",32,"-","O"]
["监测点","GS_JS_JCD","点","备注","BZ","字符型",255,"相关事项说明","O"]
["监测设备","GS_JC_JCSB","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测设备","GS_JC_JCSB","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M","标识码，暂由系统生成。"]
["监测设备","GS_JC_JCSB","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测设备","GS_JC_JCSB","-","设备名称","SBMC","字符型",50,"-","M"]
["监测设备","GS_JC_JCSB","-","设备型号","SBXH","字符型",32,"-","O"]
["监测设备","GS_JC_JCSB","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测设备","GS_JC_JCSB","-","采集频率","CJPL","字符型",32,"采集间隔时间，单位：分钟","M"]
["监测设备","GS_JC_JCSB","-","上传频率","SCPL","字符型",32,"上传间隔时间，单位：分钟","M"]
["监测设备","GS_JC_JCSB","-","设备状态","SBZT","整型","-","1( 未 使 用 )/2( 正 常 )/3( 试 运 行)/4(故障)/5(维修)/6(报废)","M"]
["监测设备","GS_JC_JCSB","-","厂商名称","CSMC","字符型",50,"-","O"]
["监测设备","GS_JC_JCSB","-","相对高度","XDGD","浮点型",7.3,"如液位计相对井口高度","O"]
["监测设备","GS_JC_JCSB","-","安装时间","AZSJ","日期型","-","-","O"]
["监测设备","GS_JC_JCSB","-","安装维护单位","AZWHDW","字符型",100,"单位名称","O"]
["监测设备","GS_JC_JCSB","-","供电方式","GDFS","字符型",32,"-","O"]
["监测设备","GS_JC_JCSB","-","备注","BZ","字符型",255,"相关事项说明","O"]
["监测项阈值","GS_JC_JCXYZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测项阈值","GS_JC_JCXYZ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M"]
["监测项阈值","GS_JC_JCXYZ","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测项阈值","GS_JC_JCXYZ","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测项阈值","GS_JC_JCXYZ","-","报警阈值","BJYZ","浮点型",10.3,"-","M"]
["监测项阈值","GS_JC_JCXYZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["实时监测","GS_JC_SSJC","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["实时监测","GS_JC_SSJC","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M"]
["实时监测","GS_JC_SSJC","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["实时监测","GS_JC_SSJC","-","监测值","JCZ","浮点型",18.2,"监测特征值","M"]
["实时监测","GS_JC_SSJC","-","监测采集时间","JCCJSJ","时间日期型","-","-","M"]
["实时监测","GS_JC_SSJC","-","监测上报时间","JCSBSJ","时间日期型","-","-","M"]
["实时监测","GS_JC_SSJC","-","备注","BZ","字符型",255,"相关事项说明","O"]
["视频监控  ","GS_JC_SPJK ","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["视频监控  ","GS_JC_SPJK ","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["视频监控  ","GS_JC_SPJK ","点","设备名称","SBMC","字符型",50,"视频设备名称","M"]
["视频监控  ","GS_JC_SPJK ","点","安装地址","AZDZ","字符型",255,"-","M"]
["视频监控  ","GS_JC_SPJK ","点","监控对象","JKDX","字符型",255,"-","M"]
["视频监控  ","GS_JC_SPJK ","点","设备型号","SBXH","字符型",255,"-","M"]
["视频监控  ","GS_JC_SPJK ","点","生产厂家","SCCJ","字符型",100,"厂家名称","O"]
["视频监控  ","GS_JC_SPJK ","点","产权单位","CQDW","字符型",100,"单位名称","M"]
["视频监控  ","GS_JC_SPJK ","点","视频地址","SPDZ","字符型",255,"可以直接播放的视频流 URL 地址， 通常由视频联网平台提供","O"]
["视频监控  ","GS_JC_SPJK ","点","备注","BZ","字符型",255,"相关事项说明","O"]
["监测报警  ","GS_JC_JCBJ ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测报警  ","GS_JC_JCBJ ","-","报警名称","BJMC","字符型",50,"-","M"]
["监测报警  ","GS_JC_JCBJ ","-","报警编号","BJBH","字符型",64,"程序自动生成，唯一","M"]
["监测报警  ","GS_JC_JCBJ ","-","点位标识码","DWBSM","字符型",64,"关联监测点标识码","M"]
["监测报警  ","GS_JC_JCBJ ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M"]
["监测报警  ","GS_JC_JCBJ ","-","监测报警指标","JCBJZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测报警  ","GS_JC_JCBJ ","-","当前报警级别","DQBJJB","字符型",16,"一级/二级/三级/四级；城市内涝 场景非必填","C"]
["监测报警  ","GS_JC_JCBJ ","-","初次报警时间","CCBJSJ","时间日期型","-","-","M"]
["监测报警  ","GS_JC_JCBJ ","-","初次报警值","CCBJZ","浮点型",18.2,"初次触发报警的监测值","M"]
["监测报警  ","GS_JC_JCBJ ","-","当前报警时间","DQBJSJ","时间日期型","-","-","M"]
["监测报警  ","GS_JC_JCBJ ","-","当前报警值","DQBJZ","浮点型",18.2,"当前触发报警的监测值","M"]
["监测报警  ","GS_JC_JCBJ ","-","累计报警频次","LJBJPC","整型","-","本次报警在报警解除之间所产生 的报警次数","M"]
["监测报警  ","GS_JC_JCBJ ","-","报警是否解除","BJSFJC","布尔型","-","0(否)/1(是)","M"]
["监测报警  ","GS_JC_JCBJ ","-","报警解除时间","BJJCSJ","时间日期型","-","当报警确认解除时， 填写报警解除 时间","C"]
["监测报警  ","GS_JC_JCBJ ","-","报警解除说明","BJJCSM","字符型",255,"当报警确认解除时， 填写报警解除 说明","C"]
["监测报警  ","GS_JC_JCBJ ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["报警分析","GS_JC_BJFX","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["报警分析","GS_JC_BJFX","-","报警编号","BJBH","字符型",64,"见监测报警属性表","M"]
["报警分析","GS_JC_BJFX","-","报警点位位置","BJDWWZ","字符型",255,"-","M"]
["报警分析","GS_JC_BJFX","-","现场排查人员","XCPCRY","字符型",32,"-","M"]
["报警分析","GS_JC_BJFX","-","现场排查人员手机","XCPCRYSJ","字符型",15,"-","M"]
["报警分析","GS_JC_BJFX","-","到达现场时间","DDXCSJ","时间日期型","-","-","M"]
["报警分析","GS_JC_BJFX","-","现场状况描述","XCZKMS","变长字符型","-","-","M"]
["报警分析","GS_JC_BJFX","-","值守人员","ZSRY","字符型",32,"系统值守人员","M"]
["报警分析","GS_JC_BJFX","-","值守人员手机","ZSRYSJ","字符型",15,"-","M"]
["报警分析","GS_JC_BJFX","-","值守人员单位","ZSRYDW","字符型",100,"单位名称","M"]
["报警分析","GS_JC_BJFX","-","值守人员分析简述","ZSRYFXJS","字符型",500,"-","M"]
["报警分析","GS_JC_BJFX","-","现场人员分析报告","XCRYFXBG","二进制型","-","-","O"]
["报警分析","GS_JC_BJFX","-","值守人员分析时间","ZSRYFXSJ","时间日期型","-","-","M"]
["报警分析","GS_JC_BJFX","-","分析内容","FXNR","变长字符型","-","-","M"]
["报警分析","GS_JC_BJFX","-","现场图片视频文件","XCTPSPWJ","二进制型","-","现场图片、视频文件","O"]
["报警分析","GS_JC_BJFX","-","更新时间","GXSJ","时间日期型","-","-","M"]
["报警分析","GS_JC_BJFX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["报警处置","GS_JC_BJCZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["报警处置","GS_JC_BJCZ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
["报警处置","GS_JC_BJCZ","-","报警编号","BJBH","字符型",64,"关联监测报警表","M"]
["报警处置","GS_JC_BJCZ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)","M"]
["报警处置","GS_JC_BJCZ","-","处置时间","CZSJ","时间日期型","-","-","M"]
["报警处置","GS_JC_BJCZ","-","处置内容","CZNR","变长字符型","-","-","M"]
["报警处置","GS_JC_BJCZ","-","处置报告","CZBG","二进制型","-","-","M"]
["报警处置","GS_JC_BJCZ","-","记录人员","JLRY","字符型",32,"-","M"]
["报警处置","GS_JC_BJCZ","-","更新时间","GXSJ","时间日期型","-","-","M"]
["报警处置","GS_JC_BJCZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["监测预警","GS_JC_JCYJ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测预警","GS_JC_JCYJ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
["监测预警","GS_JC_JCYJ","-","预警名称","YJMC","字符型",50,"-","M"]
["监测预警","GS_JC_JCYJ","-","预警设施名称","YJSSMC","字符型",50,"-","O"]
["监测预警","GS_JC_JCYJ","-","预警设施编号","YJSSBH","字符型",64,"-","O"]
["监测预警","GS_JC_JCYJ","-",{"$nulls":4},"1(燃气泄漏)/2(燃气爆炸)/3(管网 爆管)/4(泄漏)/5(路面塌陷)/6(暴 雨洪涝)/7(排水管网淤积)/8(合流 制溢流)/9(检查井冒溢) /10(结构 损伤)/11(极端天气)/12(车辆超载 )/13(其它)"]
["监测预警","GS_JC_JCYJ","-"]
["监测预警","GS_JC_JCYJ","-","预警类型","YJLX","整型","-",null,"M"]
["监测预警","GS_JC_JCYJ","-","预警地址","YJDZ","字符型",255,"-","M"]
["监测预警","GS_JC_JCYJ","-","预警级别","YJJB","整型","-","1(一级)/2(二级)/3(三级)/4(四级)","M"]
["监测预警","GS_JC_JCYJ","-","预警状态","YJZT","整型","-","1(发布)/2(处置)/3(解除)","M"]
["监测预警","GS_JC_JCYJ","-","预警生成时间","YJSCSJ","时间日期型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","预警上报时间","YJSBSJ","时间日期型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","预警简述","YJJS","变长字符型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","预警报告","YJBG","二进制型","-","-","O"]
["监测预警","GS_JC_JCYJ","-","研判分析","YPFX","变长字符型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","分析报告","FXBG","二进制型","-","-","O"]
["监测预警","GS_JC_JCYJ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)/3(误报)","M"]
["监测预警","GS_JC_JCYJ","-","处置人","CZR","字符型",32,"-","M"]
["监测预警","GS_JC_JCYJ","-","处置时间","CZSJ","时间日期型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","处置建议","CZJY","变长字符型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","处置报告","CZBG","二进制型","-","-","M"]
["监测预警","GS_JC_JCYJ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["计划项目","GS_JG_JHXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["计划项目","GS_JG_JHXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["计划项目","GS_JG_JHXM","面","项目名称","XMMC","字符型",255,"-","M"]
["计划项目","GS_JG_JHXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
["计划项目","GS_JG_JHXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
["计划项目","GS_JG_JHXM","面","项目内容","XMNR","字符型",255,"-","M"]
["计划项目","GS_JG_JHXM","面","计划年度","JHND","整型","-","如：“2022”","M"]
["计划项目","GS_JG_JHXM","面","项目建设周期","XMJSZQ","整型","-","单位：月","M"]
["计划项目","GS_JG_JHXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
["计划项目","GS_JG_JHXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
["建设项目","GS_JG_JSXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["建设项目","GS_JG_JSXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["建设项目","GS_JG_JSXM","面","项目名称","XMMC","字符型",255,"针对道路是指最新一次改造拓宽 项目","M"]
["建设项目","GS_JG_JSXM","面","项目代码","XMDM","字符型",50,"固定资产投资审批、核准、备案范 围内的项目引用项目代码","O"]
["建设项目","GS_JG_JSXM","面","项目编码","XMBM","字符型",32,"非固定资产投资审批、核准、备案 范围内的项目引用项目编码","O"]
["建设项目","GS_JG_JSXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
["建设项目","GS_JG_JSXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
["建设项目","GS_JG_JSXM","面","项目内容","XMNR","字符型",255,"-","M"]
["建设项目","GS_JG_JSXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
["建设项目","GS_JG_JSXM","面","详细地址","XXDZ","字符型",255,"-","M"]
["建设项目","GS_JG_JSXM","面","立项许可信息","LXXKXX","字符型",255,"立项批复文号","O"]
["建设项目","GS_JG_JSXM","面","规划许可信息","GHXKXX","字符型",255,"建设工程规划许可证号","O"]
["建设项目","GS_JG_JSXM","面","施工许可信息","SGXKXX","字符型",255,"建设工程施工许可证号","O"]
["建设项目","GS_JG_JSXM","面","竣工验收信息","JGYSXX","字符型",255,"-","O"]
["建设项目","GS_JG_JSXM","面","建设单位","JSDW","字符型",100,"单位名称","M"]
["建设项目","GS_JG_JSXM","面","设计单位","SJDW","字符型",100,"单位名称","O"]
["建设项目","GS_JG_JSXM","面","施工单位","SGDW","字符型",100,"单位名称","O"]
["建设项目","GS_JG_JSXM","面","监理单位","JLDW","字符型",100,"单位名称","O"]
["建设项目","GS_JG_JSXM","面","实际开始时间","SJKSSJ","日期型","-","-","O"]
["建设项目","GS_JG_JSXM","面","实际结束时间","SJJSSJ","日期型","-","-","O"]
["建设项目","GS_JG_JSXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
["维修点","GS_JG_WXD","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["维修点","GS_JG_WXD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["维修点","GS_JG_WXD","点","名称","MC","字符型",50,"维修点/停水影响区域的常用名称","M"]
["维修点","GS_JG_WXD","点","地址","DZ","字符型",255,"具体位置描述","O"]
["维修点","GS_JG_WXD","点","类型","LX","字符型",100,"维修点/停水影响区域的所属设施 类型","O"]
["维修点","GS_JG_WXD","点","调查日期","DCRQ","日期型","-","现场调查日期","O"]
["维修点","GS_JG_WXD","点","区域情况描述","QYQKMS","字符型",255,"维修点/停水影响区域情况描述","O"]
["维修点","GS_JG_WXD","点","填报单位","TBDW","字符型",100,"单位名称","O"]
["维修点","GS_JG_WXD","点","填报日期","TBRQ","日期型","-","数据填报日期","O"]
["维修点","GS_JG_WXD","点","备注","BZ","字符型",255,"相关事项说明","O"]
["停水影响区域","GS_JG_TSYXQY","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["停水影响区域","GS_JG_TSYXQY","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["停水影响区域","GS_JG_TSYXQY","面","名称","MC","字符型",50,"维修点/停水影响区域的常用名称","M"]
["停水影响区域","GS_JG_TSYXQY","面","地址","DZ","字符型",255,"具体位置描述","O"]
["停水影响区域","GS_JG_TSYXQY","面","类型","LX","字符型",100,"维修点/停水影响区域的所属设施 类型","O"]
["停水影响区域","GS_JG_TSYXQY","面","调查日期","DCRQ","日期型","-","现场调查日期","O"]
["停水影响区域","GS_JG_TSYXQY","面","区域情况描述","QYQKMS","字符型",255,"维修点/停水影响区域情况描述","O"]
["停水影响区域","GS_JG_TSYXQY","面","填报单位","TBDW","字符型",100,"单位名称","O"]
["停水影响区域","GS_JG_TSYXQY","面","填报日期","TBRQ","日期型","-","数据填报日期","O"]
["停水影响区域","GS_JG_TSYXQY","面","备注","BZ","字符型",255,"相关事项说明","O"]
["日常维护维修","GS_JG_RCWHWX","-","标识码","BSM","字符型",32,"自动生成，唯一","M","缺少标识码、处置结果、处置日期、处置人员、联系电话、养护单位、设施权属单位、"]
["日常维护维修","GS_JG_RCWHWX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["日常维护维修","GS_JG_RCWHWX","-","维护维修内容","WHWXNR","字符型",255,"-","M"]
["日常维护维修","GS_JG_RCWHWX","-","设备设施","SBSS","字符型",255,"关联设备设施的标识码， 存在多个 设备设施用英文分号“;”分隔","M"]
["日常维护维修","GS_JG_RCWHWX","-","处理结果","CLJG","字符型",255,"-","O"]
["日常维护维修","GS_JG_RCWHWX","-","处理日期","CLRQ","日期型","-","-","O"]
["日常维护维修","GS_JG_RCWHWX","-","处理人员","CLRY","字符型",32,"-","O"]
["日常维护维修","GS_JG_RCWHWX","-","联系电话","LXDH","字符型",16,"-","O"]
["日常维护维修","GS_JG_RCWHWX","-","养护单位","YHDW","字符型",100,"单位名称","O"]
["日常维护维修","GS_JG_RCWHWX","-","设施权属单位","SSQSDW","字符型",100,"单位名称","O"]
["日常维护维修","GS_JG_RCWHWX","-","检测方法","JCFF","字符型",255,"-","M"]
["日常维护维修","GS_JG_RCWHWX","-","检测结论","JCJL","字符型",255,"-","M"]
["日常维护维修","GS_JG_RCWHWX","-","附件","FJ","二进制型","-","-","O"]
["日常维护维修","GS_JG_RCWHWX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["突发事件抢修","GS_JG_TFSJQX","-","标识码","BSM","字符型",32,"自动生成，唯一","M","缺失必给项标识码、相应级别、现场照片、附件"]
["突发事件抢修","GS_JG_TFSJQX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["突发事件抢修","GS_JG_TFSJQX","-","事件名称","SJMC","字符型",50,"-","M"]
["突发事件抢修","GS_JG_TFSJQX","-","事件说明","SJSM","字符型",255,"-","O"]
["突发事件抢修","GS_JG_TFSJQX","-","地址","DZ","字符型",255,"-","O"]
["突发事件抢修","GS_JG_TFSJQX","-","关联基础设施","GLJCSS","字符型",32,"燃气/供水/排水/道路/桥梁，存在多 个设备设施用英文分号“;”分隔","M"]
["突发事件抢修","GS_JG_TFSJQX","-",{"$nulls":4},"1(一级)/2(二级)/3(三级)/4(四级)； 参照《江苏省突发事件总体应急预 案》中应急响应分级的规定"]
["突发事件抢修","GS_JG_TFSJQX","-","响应级别","XYJB","整型","-",null,"M"]
["突发事件抢修","GS_JG_TFSJQX","-","现场照片","XCZP","二进制型","-","-","M"]
["突发事件抢修","GS_JG_TFSJQX","-","抢修内容","QXNR","字符型",255,"抢修内容及处理方法","M"]
["突发事件抢修","GS_JG_TFSJQX","-","处理结果","CLJG","字符型",255,"-","O"]
["突发事件抢修","GS_JG_TFSJQX","-","处理日期","CLRQ","日期型","-","-","O"]
["突发事件抢修","GS_JG_TFSJQX","-","处理人员","CLRY","字符型",32,"-","O"]
["突发事件抢修","GS_JG_TFSJQX","-","处理单位","CLDW","字符型",100,"单位名称","O"]
["突发事件抢修","GS_JG_TFSJQX","-","附件","FJ","二进制型","-","-","M"]
["突发事件抢修","GS_JG_TFSJQX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["管道检测","GS_JC_GDJC","点","标识码","BSM","字符型",32,"自动生成，唯一","M","缺少标识码、描述"]
["管道检测","GS_JC_GDJC","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["管道检测","GS_JC_GDJC","点","设施编码","SSBM","字符型",17,"与被检测管道的编码一致","M"]
["管道检测","GS_JC_GDJC","点","管道材质","GDCZ","字符型",6,"-","M"]
["管道检测","GS_JC_GDJC","点","管径","GJ","字符型",255,"-","M"]
["管道检测","GS_JC_GDJC","点","检测日期","JCRQ","日期型","-","-","M"]
["管道检测","GS_JC_GDJC","点","描述","MS","字符型",255,"-","M"]
["管道检测","GS_JC_GDJC","点","照片","ZP","二进制型","-","-","O"]
["管道检测","GS_JC_GDJC","点","备注","BZ","字符型",255,"相关事项说明","O"]
["第三方施工专项","GS_JG_DSFSGZX","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","项目名称","XMMC","字符型",255,"-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","项目内容","XMNR","字符型",255,"-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","所在街道","SZJD","字符型",255,"-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","施工项目地址","XXDZ","字符型",255,"-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","计划开始时间","JHKSSJ","日期型","-","-","O"]
["第三方施工专项","GS_JG_DSFSGZX","面","计划结束时间","JHJSSJ","日期型","-","-","O"]
["第三方施工专项","GS_JG_DSFSGZX","面","实际开始时间","SJKSSJ","日期型","-","-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","实际结束时间","SJJSSJ","日期型","-","-","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","施工深度","SGSD","浮点型",6.2,"第三方施工开挖最大深度","M"]
["第三方施工专项","GS_JG_DSFSGZX","面","建设单位","JSDW","字符型",255,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","建设单位负责人","JSDWFZR","字符型",16,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","建设单位负责人联 系电话","JSDWFZRLXDH","字符型",16,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","施工单位","SGDW","字符型",255,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","施工单位负责人","SGDWFZR","字符型",16,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","施工单位负责人联 系电话","SGDWFZRLXDH","字符型",16,null,"M"]
["第三方施工专项","GS_JG_DSFSGZX","面","监理单位","JLDW","字符型",255,null,"O"]
["第三方施工专项","GS_JG_DSFSGZX","面","监理单位负责人","JLDWFZR","字符型",255,null,"O"]
["第三方施工专项","GS_JG_DSFSGZX","面","监理单位负责人联 系电话","JLDWFZRLXDH","字符型",255,null,"O"]
["第三方施工专项","GS_JG_DSFSGZX","面","备注","BZ","字符型",255,"相关事项说明","O"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"标识码","bsm","字符型",32,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"风险编号","fxbh","字符型",64,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"风险等级","fxdj","整型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"详细地址","xxdz","字符型",200,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估单位","pgdw","字符型",100,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估时间","pgsj","日期型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"管控状态","gkzt","整型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"管控措施","gkcs","字符型",500,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"风险描述","fxms","字符型",1000,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"备注","bz","字符型",255,null,"O"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"同步时间","tbsj","日期型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"权属单位","qsdw","字符型",64,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"数据成果批次编号","sjcgpcbh","字符型",64,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估单元名称","pgdymc","字符型",100,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估单元唯一标识","pgdywybs","字符型",64,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"关联管段编号","glgdbh","字符型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估单元位置","pgdywz","字符型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"评估单元管道长度","pgdygdcd","浮点型",11.3,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"可能性等级","knxdj","整型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"后果等级","hgdj","整型",null,null,"M"]
["管网风险&处置信息属性结构表","gs_jg_gwfxhczxx",null,"空间信息","kjxx","geometry",null,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"标识码","bsm","字符型",32,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"老旧管网总长","ljgwzc","整型",null,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"当年计划改造老旧管网总长","dnjhgzljgwzc","整型",null,null,"O"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"老旧管网已改造长度","ljgwygzcd","整型",null,null,"O"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"老旧管网改造中长度","ljgwgzzcd","整型",null,null,"O"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"老旧管网未改造长度","ljgwwgzcd","整型",null,null,"O"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"年份","nf","整型",null,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"备注","bz","字符型",255,null,"O"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["老旧管网改造落实情况属性结构表","gs_jg_ljgwgzlsqk",null,"同步时间","tbsj","日期型",null,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"标识码","bsm","字符型",32,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"巡检养护标识码","xjyhbsm","字符型",32,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"是否涉及工程机械","sfsjgcjx","布尔型",null,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题分类","wtfl","整型",null,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题描述","wtms","字符型",255,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"检查地址","jcdz","字符型",255,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题上报单位","wtsbdw","字符型",100,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题上报人","wtsbr","字符型",16,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题上报时间","wtsbsj","日期型",null,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题处置单位","wtczdw","字符型",100,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题处置负责人","wtczfzr","字符型",32,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题处置负责人联系电话","wtczfzrlxdh","字符型",16,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题处置时间","wtczsj","日期型",null,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"问题处置简述","wtczjs","字符型",255,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"处置状态","czzt","整型",null,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"处置附件","czfj","二进制型",null,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"现场图片","xctp","二进制型",null,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"备注","bz","字符型",255,null,"O"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"空间信息","kjxx","geometry",null,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["巡检养护第三方施工问题属性结构表","gs_jg_xjxcdsfsgwt",null,"同步时间","tbsj","日期型",null,null,"M"]
["巡检记录","GS_JG_XJJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["巡检记录","GS_JG_XJJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["巡检记录","GS_JG_XJJL","-","巡检对象","XJDX","整型","-","燃 气 、 排 水 设 施 填 写 ； 1( 管 道)/2(场站)/3(用户)/4(其它)","M"]
["巡检记录","GS_JG_XJJL","-","检查单元","JCDY","字符型",255,"-","O"]
["巡检记录","GS_JG_XJJL","-","检查项目","JCXM","字符型",255,"-","O"]
["巡检记录","GS_JG_XJJL","-","检查方法","JCFF","字符型",255,"-","O"]
["巡检记录","GS_JG_XJJL","-","检查内容","JCNR","字符型",255,"-","M"]
["巡检记录","GS_JG_XJJL","-","检查结果","JCJG","字符型",255,"-","O"]
["巡检记录","GS_JG_XJJL","-","存在隐患","CZYH","字符型",255,"-","O"]
["巡检记录","GS_JG_XJJL","-","检查日期","JCRQ","时间日期型","-","-","M"]
["巡检记录","GS_JG_XJJL","-","检查人员","JCRY","字符型",32,"-","O"]
["巡检记录","GS_JG_XJJL","-","设施权属单位","SSQSDW","字符型",100,"单位名称","M"]
["巡检记录","GS_JG_XJJL","-","主管单位","ZGDW","字符型",100,"单位名称","O"]
["巡检记录","GS_JG_XJJL","-","附件","FJ","二进制型","-","-","M"]
["巡检记录","GS_JG_XJJL","-","备注","BZ","字符型",255,"相关事项说明","O"]

{"sheet":"排水分类","index":3,"n_rows":547,"n_cols":10,"rows_kept":547,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[29,3,30,3],[359,3,360,3],[0,4,1,4],[29,4,30,4],[0,5,1,5],[29,5,30,5],[359,5,360,5],[0,6,1,6],[29,6,30,6],[0,7,1,7],[317,7,318,7],[359,7,360,7],[0,8,1,8],[29,8,30,8],[0,9,1,9],[2,9,23,9],[33,9,58,9],[59,9,71,9],[72,9,96,9],[135,9,143,9],[144,9,158,9],[165,9,171,9],[366,9,391,9]]}
["中文表名","表名","要素类型","中文名","字段名","数据类型","长度","值域及说明","约束条件","备注"]
[]
["管线","PS_JS_GX","线","标识码","BSM","字符型",32,"自动生成，唯一","M","管线 缺少必给\n字段： 标识码,埋设类型,要素代码"]
["管线","PS_JS_GX","线","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["管线","PS_JS_GX","线","管类代码","GLDM","字符型",8,"管线类型代码(如“RQ”)","M"]
["管线","PS_JS_GX","线","起点点号","QDDH","字符型",14,"-","M"]
["管线","PS_JS_GX","线","终点点号","ZDDH","字符型",14,"-","M"]
["管线","PS_JS_GX","线","起点高程","QDGC","浮点型",6.2,"单位：米","M"]
["管线","PS_JS_GX","线","终点高程","ZDGC","浮点型",6.2,"单位：米","M"]
["管线","PS_JS_GX","线","起点埋深","QDMS","浮点型",6.2,"起点埋深/架空高度，单位：米","M"]
["管线","PS_JS_GX","线","终点埋深","ZDMS","浮点型",6.2,"终点埋深/架空高度，单位：米","M"]
["管线","PS_JS_GX","线","埋设类型","MSLX","整型",null,"0(直埋)/1(矩形管沟)/2(拱形管 沟 )/3( 管 块 )/4( 管 埋 )/5( 架 空)/6(井内连线)/7(顶管)","M"]
["管线","PS_JS_GX","线","材质","CZ","字符型",8,"-","M"]
["管线","PS_JS_GX","线","管径","GJ","字符型",15,"断面尺寸(宽 X 高)或者管径","M"]
["管线","PS_JS_GX","线","压力","YL","字符型",4,"燃气管道压力，排水是否有压","M"]
["管线","PS_JS_GX","线","要素代码","YSDM","字符型",10,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
["管线","PS_JS_GX","线","所在道路","SZDL","字符型",50,"-","O"]
["管线","PS_JS_GX","线","权属单位","QSDW","字符型",100,"单位名称","O"]
["管线","PS_JS_GX","线","建设年代","JSND","字符型",10,"如：“1991”","O"]
["管线","PS_JS_GX","线","探测单位","TCDW","字符型",100,"单位名称","O"]
["管线","PS_JS_GX","线","探测日期","TCRQ","日期型","-","-","O"]
["管线","PS_JS_GX","线","使用状态","SYZT","整型","-","1(待投用)/2(投用中)/3(检修中) /4(废弃)","O"]
["管线","PS_JS_GX","线","数据来源","SJLY","字符型",255,"探测/竣测/图解/整合/权属单位 提供","O"]
["管线","PS_JS_GX","线","备注","BZ","字符型",255,"相关事项说明","O"]
["管线明细","PS_JS_GX_ATT",null,"标识码","BSM","字符型",32,"自动生成，唯一","M"]
["管线明细","PS_JS_GX_ATT",null,"通用表标识码","TYBBSM","字符型",32,"关联管线通用表标识码","M"]
["管线明细","PS_JS_GX_ATT",null,"类別","LB","整型","-","1(雨水)/2(污水)3(合流)","M"]
["管线明细","PS_JS_GX_ATT",null,"管道级别","GDJB","字符型",10,"主干管/次干管/支管","M"]
["管线明细","PS_JS_GX_ATT",null,"流向","LX","整型","-","0(起点到终点)/1(终点到起点)","M"]
["管线明细","PS_JS_GX_ATT",null,"是否有压","SFYY","布尔型","-","当类别为污水时填写：","C"]
["管线明细","PS_JS_GX_ATT",{"$nulls":5},"0(否)/1(是)"]
["管线明细","PS_JS_GX_ATT",null,"管道异常","GDYC","字符型",255,"记录管道内异常情况，如穿缆等","O"]
["管线明细","PS_JS_GX_ATT",null,"备注","BZ","字符型",255,"相关事项说明","O"]
["管点","PS_JS_GD","点","标识码","BSM","字符型",32,"自动生成，唯一","M","管点 缺少必给字段：管类代码，要素代码，特征点，附属物，井室代码，旋转角，权属单位，探测单位，探测日期"]
["管点","PS_JS_GD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["管点","PS_JS_GD","点","管类代码","GLDM","字符型",8,"管点类型代码(如“RQ” )","M"]
["管点","PS_JS_GD","点","探测点号","TCDH","字符型",16,"外业点号，测区内唯一","M"]
["管点","PS_JS_GD","点","要素代码","YSDM","字符型",10,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
["管点","PS_JS_GD","点","地面高程","DMGC","浮点型",7.3,"单位：米","M"]
["管点","PS_JS_GD","点","特征点","TZD","字符型",15,"参照 DGJ32/TJ 187《江苏省城市地 下管线数据标准》","M"]
["管点","PS_JS_GD","点","附属物","FSW","字符型",15,"如调压箱、阀门等， 参照 DGJ32/TJ 187《江苏省城市地下管线数据标 准》","M"]
["管点","PS_JS_GD","点","所在道路","SZDL","字符型",50,"-","M"]
["管点","PS_JS_GD","点","井室代码","JSDM","整型","-","填写 3 位井室代码","M"]
["管点","PS_JS_GD","点","旋转角","XZJ","浮点型",8.3,"按平面直角坐标系弧度表示","M"]
["管点","PS_JS_GD","点","井深","JS","浮点型",6.2,"当探测点号为检修井时， 单位： 米","O"]
["管点","PS_JS_GD","点","井盖形状","JGXZ","字符型",10,"圆形/矩形","O"]
["管点","PS_JS_GD","点","井盖材质","JGCZ","字符型",10,"-","O"]
["管点","PS_JS_GD","点","井盖直径","JGZJ","浮点型",5,"单位：米","O"]
["管点","PS_JS_GD","点","井盖长","JGC","浮点型",5,"管线的主线方向井盖长， 单位： 米","O"]
["管点","PS_JS_GD","点","井盖宽","JGK","浮点型",5,"垂直管线的主线方向井盖宽度， 单 位：米","O"]
["管点","PS_JS_GD","点","检修井材质","JXJCZ","字符型",10,"水泥/砖","O"]
["管点","PS_JS_GD","点","井脖深","JBS","浮点型",5.2,"井盖向下的垂直段的距离，单位： 米","O"]
["管点","PS_JS_GD","点","井室直径","JSZJ","浮点型",5,"井室是柱体时填写，单位：毫米","O"]
["管点","PS_JS_GD","点","建设年代","JSND","字符型",10,"如：“1991”","O"]
["管点","PS_JS_GD","点","权属单位","QSDW","字符型",100,"单位名称","M"]
["管点","PS_JS_GD","点","探测单位","TCDW","字符型",100,"单位名称","M"]
["管点","PS_JS_GD","点","探测日期","TCRQ","日期型","-","-","M"]
["管点","PS_JS_GD","点","数据来源","SJLY","字符型",255,"探测/竣测/图解/整合/权属单位 提供","O"]
["管点","PS_JS_GD","点","备注","BZ","字符型",255,"非正常埋设的需要备注","O"]
["排口","PS_JS_PK","点","标识码","BSM","字符型",32,"自动生成，唯一","M","排口 缺少必给字段：  地表高程，顶部高程，排口尺寸，是否有拍门"]
["排口","PS_JS_PK","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["排口","PS_JS_PK","点","名称","MC","字符型",50,"-","M"]
["排口","PS_JS_PK","点","地址","DZ","字符型",255,"-","M"]
["排口","PS_JS_PK","点","类别","LB","整型","-","1(雨水)/2(污水)/3(合流)","M"]
["排口","PS_JS_PK","点","地表高程","DBGC","浮点型",6.2,"单位：米","M"]
["排口","PS_JS_PK","点","顶部高程","DBGC","浮点型",6.2,"单位：米","M"]
["排口","PS_JS_PK","点","排口尺寸","PKCC","字符型",20,"断面尺寸(宽 X 高) 或者管径， 单 位：毫米","M"]
["排口","PS_JS_PK","点","是否有拍门","SFYPM","布尔型","-","0(否)/1(是)","M"]
["排口","PS_JS_PK","点","出流形式","CLXS","整型","-","1( 自 由 出 流 )/2( 常 水 位 淹 没)/3(潮汐影响)","O"]
["排口","PS_JS_PK","点","河道常水位","HDCSW","浮点型",6.2,"排入河道的常水位，单位：米","O"]
["排口","PS_JS_PK","点","排口照片","PKZP","二进制型","-","-","O"]
["排口","PS_JS_PK","点","备注","BZ","字符型",255,"相关事项说明","O"]
["厂站","PS_JS_CZ","面","标识码","BSM","字符型",32,"自动生成，唯一","M","厂站 缺少必给字段：污泥处理设计规模"]
["厂站","PS_JS_CZ","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["厂站","PS_JS_CZ","面","名称","MC","字符型",50,"-","M"]
["厂站","PS_JS_CZ","面","地址","DZ","字符型",255,"-","O"]
["厂站","PS_JS_CZ","面","厂站类型","CZLX","字符型",40,"污水处理厂、雨水泵站、污水泵站 等","M"]
["厂站","PS_JS_CZ","面","使用状态","SYZT","整型","-","1(待投用)/2(投用中)/3(检修 中)/4(废弃)","O"]
["厂站","PS_JS_CZ","面","探测单位","TCDW","字符型",100,"单位名称","O"]
["厂站","PS_JS_CZ","面","探测日期","TCRQ","日期型","-","-","O"]
["厂站","PS_JS_CZ","面","数据来源","SJLY","字符型",255,"探测/竣测/图解/整合/权属单位 提供","O"]
["厂站","PS_JS_CZ","面","竣工日期","JGRQ","日期型","-","-","O"]
["厂站","PS_JS_CZ","面","污水处理级别","WSCLJB","整型","-","1(一级)/2(二级)/3(三级)","O"]
["厂站","PS_JS_CZ","面","年耗电量","NHDL","浮点型",10.2,"单位：万千瓦时","O"]
["厂站","PS_JS_CZ","面","污水处理设计规模","WSCLSJGM","浮点型",10.2,"污水处理厂设计处理能力，单位： 万立方米/天","M"]
["厂站","PS_JS_CZ","面","污水运行负荷率","WSYXFHL","浮点型",4.2,"百分比例，填年均值","M"]
["厂站","PS_JS_CZ","面","雨水处理设计规模","YSCLSJGM","浮点型",10.2,"初期雨水设计处理规模， 单位： 万 立方米/天","O"]
["厂站","PS_JS_CZ","面","污泥处理设计规模","WNCLSJGM","浮点型",10.2,"污水处理厂污泥设计处理能力， 单 位：万吨/天","M"]
["厂站","PS_JS_CZ","面","污泥运行负荷率","WNYXFHL","浮点型",4.2,"百分比例，填年均值","O"]
["厂站","PS_JS_CZ","面","污泥处置方式","WNCZFS","字符型",100,"1( 填 埋 )/2( 焚 烧 )/3( 土 地 利 用)/4(建材利用)/5(堆肥)/6(其 它)，并注明污泥处理方式","O"]
["厂站","PS_JS_CZ","面","污泥处置单位","WNCZDW","字符型",100,"-","O"]
["厂站","PS_JS_CZ","面","泵站水泵台数","BZSBTS","整型","-","水泵的台数","O"]
["厂站","PS_JS_CZ","面","泵站总功率","BZZGL","浮点型",6.2,"单位：千瓦","O"]
["厂站","PS_JS_CZ","面","泵站总流量","BZZLL","浮点型",6.2,"单位：立方米/秒","O"]
["厂站","PS_JS_CZ","面","泵站照片","BZZP","二进制型","-","-","O"]
["厂站","PS_JS_CZ","面","建设单位","JSDW","字符型",100,"单位名称","O"]
["厂站","PS_JS_CZ","面","备注","BZ","字符型",255,"相关事项说明","O"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","名称","MC","字符型",50,"重点保障对象名称","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","地址","DZ","字符型",255,"具体位置描述","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","类别","LB","字符型",100,"下穿立交、涵洞、隧道、医院、学 校等","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","调查日期","DCRQ","日期型","-","-","O"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","对象情况描述","DXQKMS","字符型",255,"重点保障对象情况描述","M"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","填报单位","TBDW","字符型",100,"单位名称","O"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","填报日期","TBRQ","日期型","-","-","O"]
["排水防涝重点保 障对象","PS_JS_PSFLZDBZDX","点","备注","BZ","字符型",255,"相关事项说明","O"]
["易涝点","PS_JS_YLD","点/面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["易涝点","PS_JS_YLD","点/面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["易涝点","PS_JS_YLD","点/面","名称","MC","字符型",50,"易涝点的常用名称","M"]
["易涝点","PS_JS_YLD","点/面","风险等级","FXDJ","字符型",32,"-","O"]
["易涝点","PS_JS_YLD","点/面","地址","DZ","字符型",255,"具体位置描述","M"]
["易涝点","PS_JS_YLD","点/面","调查降雨量","DCJYL","浮点型",5.2,"单位：毫米","O"]
["易涝点","PS_JS_YLD","点/面","调查降雨持续时间","DCJYLCXSJ","整型",5,"单位：分钟","O"]
["易涝点","PS_JS_YLD","点/面","调查最大内涝水深","DCZDNLSS","浮点型",4.2,"单位：米","O"]
["易涝点","PS_JS_YLD","点/面","调查最大淹水面积","DCZDYSMJ","浮点型",10.2,"道路积水超过 15 厘米的路段面积， 单位：平方米","O"]
["易涝点","PS_JS_YLD","点/面","调查内涝持续时间","DCNLCXSJ","整型",5,"单位：分钟","O"]
["易涝点","PS_JS_YLD","点/面","内涝主要原因","NLZYYY","字符型",100,"引起该区域内涝的主要原因","M"]
["易涝点","PS_JS_YLD","点/面","调查日期","DCRQ","日期型","-","-","O"]
["易涝点","PS_JS_YLD","点/面","区域情况描述","QYQKMS","字符型",255,"内涝情况描述","M"]
["易涝点","PS_JS_YLD","点/面","填报单位","TBDW","字符型",100,"单位名称","M"]
["易涝点","PS_JS_YLD","点/面","填报日期","TBRQ","日期型","-","-","M"]
["易涝点","PS_JS_YLD","点/面","备注","BZ","字符型",255,"相关事项说明","O"]
["防涝应急资源","PS_JS_FLYJZY","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["防涝应急资源","PS_JS_FLYJZY","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["防涝应急资源","PS_JS_FLYJZY","点","仓库名称","CKMC","字符型",50,"-","M"]
["防涝应急资源","PS_JS_FLYJZY","点","仓库类型","CKLX","字符型",50,"-","M"]
["防涝应急资源","PS_JS_FLYJZY","点","应急联系人","YJLXR","字符型",32,"-","M"]
["防涝应急资源","PS_JS_FLYJZY","点","联系电话","LXDH","字符型",16,"-","M"]
["防涝应急资源","PS_JS_FLYJZY","点","地址","DZ","字符型",255,"具体位置描述","M"]
["防涝应急资源","PS_JS_FLYJZY","点","资源种类","ZYZL","字符型",32,"防涝应急资源种类","M"]
["防涝应急资源","PS_JS_FLYJZY","点","资源数量","ZYSL","整型","-","防涝应急资源数量","M"]
["防涝应急资源","PS_JS_FLYJZY","点","填报单位","TBDW","字符型",100,"单位名称","O"]
["防涝应急资源","PS_JS_FLYJZY","点","填报日期","TBRQ","日期型","-","数据填报日期","O"]
["防涝应急资源","PS_JS_FLYJZY","点","备注","BZ","字符型",255,"相关事项说明","O"]
["监测点","PS_JS_JCD","点","标识码","BSM","字符型",32,"自动生成，唯一","M","监测点 缺少必给字段：标识码"]
["监测点","PS_JS_JCD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["监测点","PS_JS_JCD","点","点位名称","DWMC","字符型",64,"-","M"]
["监测点","PS_JS_JCD","点","设施名称","SSMC","字符型",64,"基础设施名称","O"]
["监测点","PS_JS_JCD","点","设施编码","SSBM","字符型",17,"被监测设施编码","M"]
["监测点","PS_JS_JCD","点","监测位置","JCWZ","字符型",200,"-","O"]
["监测点","PS_JS_JCD","点","高程","GC","浮点型",7.3,"单位：米","O"]
["监测点","PS_JS_JCD","点","高程基准","GCJZ","字符型",32,"-","O"]
["监测点","PS_JS_JCD","点","备注","BZ","字符型",255,"相关事项说明","O"]
["监测设备","PS_JC_JCSB","-","标识码","BSM","字符型",32,"自动生成，唯一","M","监测设备 缺少必给字段：标识码"]
["监测设备","PS_JC_JCSB","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M"]
["监测设备","PS_JC_JCSB","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测设备","PS_JC_JCSB","-","设备名称","SBMC","字符型",50,"-","M"]
["监测设备","PS_JC_JCSB","-","设备型号","SBXH","字符型",32,"-","O"]
["监测设备","PS_JC_JCSB","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测设备","PS_JC_JCSB","-","采集频率","CJPL","字符型",32,"采集间隔时间，单位：分钟","M"]
["监测设备","PS_JC_JCSB","-","上传频率","SCPL","字符型",32,"上传间隔时间，单位：分钟","M"]
["监测设备","PS_JC_JCSB","-","设备状态","SBZT","整型","-","1( 未 使 用 )/2( 正 常 )/3( 试 运 行)/4(故障)/5(维修)/6(报废)","M"]
["监测设备","PS_JC_JCSB","-","厂商名称","CSMC","字符型",50,"-","O"]
["监测设备","PS_JC_JCSB","-","相对高度","XDGD","浮点型",7.3,"如液位计相对井口高度","O"]
["监测设备","PS_JC_JCSB","-","安装时间","AZSJ","日期型","-","-","O"]
["监测设备","PS_JC_JCSB","-","安装维护单位","AZWHDW","字符型",100,"单位名称","O"]
["监测设备","PS_JC_JCSB","-","供电方式","GDFS","字符型",32,"-","O"]
["监测设备","PS_JC_JCSB","-","备注","BZ","字符型",255,"相关事项说明","O"]
["监测项阈值","PS_JC_JCXYZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测项阈值","PS_JC_JCXYZ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M"]
["监测项阈值","PS_JC_JCXYZ","-","设备类型","SBLX","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测项阈值","PS_JC_JCXYZ","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测项阈值","PS_JC_JCXYZ","-","报警阈值","BJYZ","浮点型",10.3,"-","M"]
["监测项阈值","PS_JC_JCXYZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["实时监测","PS_JC_SSJC","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["实时监测","PS_JC_SSJC","-","点位标识码","DWBSM","字符型",32,"关联监测点标识码","M"]
["实时监测","PS_JC_SSJC","-","监测指标","JCZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["实时监测","PS_JC_SSJC","-","监测值","JCZ","浮点型",18.2,"监测特征值","M"]
["实时监测","PS_JC_SSJC","-","监测采集时间","JCCJSJ","时间日期型","-","-","M"]
["实时监测","PS_JC_SSJC","-","监测上报时间","JCSBSJ","时间日期型","-","-","M"]
["实时监测","PS_JC_SSJC","-","备注","BZ","字符型",255,"相关事项说明","O"]
["视频监控","PS_JC_SPJK","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["视频监控","PS_JC_SPJK","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["视频监控","PS_JC_SPJK","点","设备名称","SBMC","字符型",50,"视频设备名称","M"]
["视频监控","PS_JC_SPJK","点","安装地址","AZDZ","字符型",255,"-","M"]
["视频监控","PS_JC_SPJK","点","监控对象","JKDX","字符型",255,"-","M"]
["视频监控","PS_JC_SPJK","点","设备型号","SBXH","字符型",255,"-","M"]
["视频监控","PS_JC_SPJK","点","生产厂家","SCCJ","字符型",100,"厂家名称","O"]
["视频监控","PS_JC_SPJK","点","产权单位","CQDW","字符型",100,"单位名称","M"]
["视频监控","PS_JC_SPJK","点","视频地址","SPDZ","字符型",255,"可以直接播放的视频流 URL 地址， 通常由视频联网平台提供","O"]
["视频监控","PS_JC_SPJK","点","备注","BZ","字符型",255,"相关事项说明","O"]
["监测报警","PS_JC_JCBJ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测报警","PS_JC_JCBJ","-","报警名称","BJMC","字符型",50,"-","M"]
["监测报警","PS_JC_JCBJ","-","报警编号","BJBH","字符型",64,"程序自动生成，唯一","M"]
["监测报警","PS_JC_JCBJ","-","点位标识码","DWBSM","字符型",64,"关联监测点标识码","M"]
["监测报警","PS_JC_JCBJ","-","设备标识码","SBBSM","字符型",64,"关联监测设备标识码","M"]
["监测报警","PS_JC_JCBJ","-","监测报警指标","JCBJZB","字符型",32,"见附录B表B.1监测设备及指标字典","M"]
["监测报警","PS_JC_JCBJ","-","当前报警级别","DQBJJB","字符型",16,"一级/二级/三级/四级；城市内涝 场景非必填","C"]
["监测报警","PS_JC_JCBJ","-","初次报警时间","CCBJSJ","时间日期型","-","-","M"]
["监测报警","PS_JC_JCBJ","-","初次报警值","CCBJZ","浮点型",18.2,"初次触发报警的监测值","M"]
["监测报警","PS_JC_JCBJ","-","当前报警时间","DQBJSJ","时间日期型","-","-","M"]
["监测报警","PS_JC_JCBJ","-","当前报警值","DQBJZ","浮点型",18.2,"当前触发报警的监测值","M"]
["监测报警","PS_JC_JCBJ","-","累计报警频次","LJBJPC","整型","-","本次报警在报警解除之间所产生 的报警次数","M"]
["监测报警","PS_JC_JCBJ","-","报警是否解除","BJSFJC","布尔型","-","0(否)/1(是)","M"]
["监测报警","PS_JC_JCBJ","-","报警解除时间","BJJCSJ","时间日期型","-","当报警确认解除时， 填写报警解除 时间","C"]
["监测报警","PS_JC_JCBJ","-","报警解除说明","BJJCSM","字符型",255,"当报警确认解除时， 填写报警解除 说明","C"]
["监测报警","PS_JC_JCBJ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["报警分析","PS_JC_BJFX","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["报警分析","PS_JC_BJFX","-","报警编号","BJBH","字符型",64,"见监测报警属性表","M"]
["报警分析","PS_JC_BJFX","-","报警点位位置","BJDWWZ","字符型",255,"-","M"]
["报警分析","PS_JC_BJFX","-","现场排查人员","XCPCRY","字符型",32,"-","M"]
["报警分析","PS_JC_BJFX","-","现场排查人员手机","XCPCRYSJ","字符型",15,"-","M"]
["报警分析","PS_JC_BJFX","-","到达现场时间","DDXCSJ","时间日期型","-","-","M"]
["报警分析","PS_JC_BJFX","-","现场状况描述","XCZKMS","变长字符型","-","-","M"]
["报警分析","PS_JC_BJFX","-","值守人员","ZSRY","字符型",32,"系统值守人员","M"]
["报警分析","PS_JC_BJFX","-","值守人员手机","ZSRYSJ","字符型",15,"-","M"]
["报警分析","PS_JC_BJFX","-","值守人员单位","ZSRYDW","字符型",100,"单位名称","M"]
["报警分析","PS_JC_BJFX","-","值守人员分析简述","ZSRYFXJS","字符型",500,"-","M"]
["报警分析","PS_JC_BJFX","-","现场人员分析报告","XCRYFXBG","二进制型","-","-","O"]
["报警分析","PS_JC_BJFX","-","值守人员分析时间","ZSRYFXSJ","时间日期型","-","-","M"]
["报警分析","PS_JC_BJFX","-","分析内容","FXNR","变长字符型","-","-","M"]
["报警分析","PS_JC_BJFX","-","现场图片视频文件","XCTPSPWJ","二进制型","-","现场图片、视频文件","O"]
["报警分析","PS_JC_BJFX","-","更新时间","GXSJ","时间日期型","-","-","M"]
["报警分析","PS_JC_BJFX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["报警处置","PS_JC_BJCZ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["报警处置","PS_JC_BJCZ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
["报警处置","PS_JC_BJCZ","-","报警编号","BJBH","字符型",64,"关联监测报警表","M"]
["报警处置","PS_JC_BJCZ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)","M"]
["报警处置","PS_JC_BJCZ","-","处置时间","CZSJ","时间日期型","-","-","M"]
["报警处置","PS_JC_BJCZ","-","处置内容","CZNR","变长字符型","-","-","M"]
["报警处置","PS_JC_BJCZ","-","处置报告","CZBG","二进制型","-","-","M"]
["报警处置","PS_JC_BJCZ","-","记录人员","JLRY","字符型",32,"-","M"]
["报警处置","PS_JC_BJCZ","-","更新时间","GXSJ","时间日期型","-","-","M"]
["报警处置","PS_JC_BJCZ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["监测预警","PS_JC_JCYJ","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["监测预警","PS_JC_JCYJ","-","行政区划代码","XZQHDM","字符型",6,"见附录A表A.1行政区划代码表","M"]
["监测预警","PS_JC_JCYJ","-","预警名称","YJMC","字符型",50,"-","M"]
["监测预警","PS_JC_JCYJ","-","预警设施名称","YJSSMC","字符型",50,"-","O"]
["监测预警","PS_JC_JCYJ","-","预警设施编号","YJSSBH","字符型",64,"-","O"]
["监测预警","PS_JC_JCYJ","-","预警类型","YJLX","整型","-","1(燃气泄漏)/2(燃气爆炸)/3(管网 爆管)/4(泄漏)/5(路面塌陷)/6(暴 雨洪涝)/7(排水管网淤积)/8(合流 制溢流)/9(检查井冒溢) /10(结构 损伤)/11(极端天气)/12(车辆超载 )/13(其它)","M"]
["监测预警","PS_JC_JCYJ","-","预警地址","YJDZ","字符型",255,"-","M"]
["监测预警","PS_JC_JCYJ","-","预警级别","YJJB","整型","-","1(一级)/2(二级)/3(三级)/4(四级)","M"]
["监测预警","PS_JC_JCYJ","-","预警状态","YJZT","整型","-","1(发布)/2(处置)/3(解除)","M"]
["监测预警","PS_JC_JCYJ","-","预警生成时间","YJSCSJ","时间日期型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","预警上报时间","YJSBSJ","时间日期型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","预警简述","YJJS","变长字符型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","预警报告","YJBG","二进制型","-","-","O"]
["监测预警","PS_JC_JCYJ","-","研判分析","YPFX","变长字符型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","分析报告","FXBG","二进制型","-","-","O"]
["监测预警","PS_JC_JCYJ","-","处置状态","CZZT","整型","-","1(处置中)/2(处置完成)/3(误报)","M"]
["监测预警","PS_JC_JCYJ","-","处置人","CZR","字符型",32,"-","M"]
["监测预警","PS_JC_JCYJ","-","处置时间","CZSJ","时间日期型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","处置建议","CZJY","变长字符型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","处置报告","CZBG","二进制型","-","-","M"]
["监测预警","PS_JC_JCYJ","-","备注","BZ","字符型",255,"相关事项说明","O"]
["计划项目","PS_JG_JHXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["计划项目","PS_JG_JHXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["计划项目","PS_JG_JHXM","面","项目名称","XMMC","字符型",255,"-","M"]
["计划项目","PS_JG_JHXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
["计划项目","PS_JG_JHXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
["计划项目","PS_JG_JHXM","面","项目内容","XMNR","字符型",255,"-","M"]
["计划项目","PS_JG_JHXM","面","计划年度","JHND","整型","-","如：“2022”","M"]
["计划项目","PS_JG_JHXM","面","项目建设周期","XMJSZQ","整型","-","单位：月","M"]
["计划项目","PS_JG_JHXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
["计划项目","PS_JG_JHXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
["建设项目","PS_JG_JSXM","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["建设项目","PS_JG_JSXM","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["建设项目","PS_JG_JSXM","面","项目名称","XMMC","字符型",255,"针对道路是指最新一次改造拓宽 项目","M"]
["建设项目","PS_JG_JSXM","面","项目代码","XMDM","字符型",50,"固定资产投资审批、核准、备案范 围内的项目引用项目代码","O"]
["建设项目","PS_JG_JSXM","面","项目编码","XMBM","字符型",32,"非固定资产投资审批、核准、备案 范围内的项目引用项目编码","O"]
["建设项目","PS_JG_JSXM","面","项目类型","XMLX","字符型",8,"新建/改建/扩建","M"]
["建设项目","PS_JG_JSXM","面","主管单位","ZGDW","字符型",100,"单位名称","M"]
["建设项目","PS_JG_JSXM","面","项目内容","XMNR","字符型",255,"-","M"]
["建设项目","PS_JG_JSXM","面","项目投资额","XMTZE","浮点型",10.3,"单位：万元","M"]
["建设项目","PS_JG_JSXM","面","详细地址","XXDZ","字符型",255,"-","M"]
["建设项目","PS_JG_JSXM","面","立项许可信息","LXXKXX","字符型",255,"立项批复文号","O"]
["建设项目","PS_JG_JSXM","面","规划许可信息","GHXKXX","字符型",255,"建设工程规划许可证号","O"]
["建设项目","PS_JG_JSXM","面","施工许可信息","SGXKXX","字符型",255,"建设工程施工许可证号","O"]
["建设项目","PS_JG_JSXM","面","竣工验收信息","JGYSXX","字符型",255,"-","O"]
["建设项目","PS_JG_JSXM","面","建设单位","JSDW","字符型",100,"单位名称","M"]
["建设项目","PS_JG_JSXM","面","设计单位","SJDW","字符型",100,"单位名称","O"]
["建设项目","PS_JG_JSXM","面","施工单位","SGDW","字符型",100,"单位名称","O"]
["建设项目","PS_JG_JSXM","面","监理单位","JLDW","字符型",100,"单位名称","O"]
["建设项目","PS_JG_JSXM","面","实际开始时间","SJKSSJ","日期型","-","-","O"]
["建设项目","PS_JG_JSXM","面","实际结束时间","SJJSSJ","日期型","-","-","O"]
["建设项目","PS_JG_JSXM","面","备注","BZ","字符型",255,"相关事项说明","O"]
["抢修抢险点","PS_JG_QXQXD","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["抢修抢险点","PS_JG_QXQXD","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["抢修抢险点","PS_JG_QXQXD","点","名称","MC","字符型",50,"抢修抢险区域的常用名称","M"]
["抢修抢险点","PS_JG_QXQXD","点","地址","DZ","字符型",255,"具体位置描述","O"]
["抢修抢险点","PS_JG_QXQXD","点","类型","LX","字符型",100,"抢修抢险区域的所属设施类型","O"]
["抢修抢险点","PS_JG_QXQXD","点","调查日期","DCRQ","日期型","-","现场调查日期","O"]
["抢修抢险点","PS_JG_QXQXD","点","区域情况描述","QYQKMS","字符型",255,"抢修抢险重点区域情况描述","O"]
["抢修抢险点","PS_JG_QXQXD","点","填报单位","TBDW","字符型",100,"单位名称","O"]
["抢修抢险点","PS_JG_QXQXD","点","填报日期","TBRQ","日期型","-","数据填报日期","O"]
["抢修抢险点","PS_JG_QXQXD","点","备注","BZ","字符型",255,"相关事项说明","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["抢修抢险区域","PS_JG_QXQXQY","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["抢修抢险区域","PS_JG_QXQXQY","面","名称","MC","字符型",50,"抢修抢险区域的常用名称","M"]
["抢修抢险区域","PS_JG_QXQXQY","面","地址","DZ","字符型",255,"具体位置描述","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","类型","LX","字符型",100,"抢修抢险区域的所属设施类型","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","调查日期","DCRQ","日期型","-","现场调查日期","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","区域情况描述","QYQKMS","字符型",255,"抢修抢险重点区域情况描述","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","填报单位","TBDW","字符型",100,"单位名称","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","填报日期","TBRQ","日期型","-","数据填报日期","O"]
["抢修抢险区域","PS_JG_QXQXQY","面","备注","BZ","字符型",255,"相关事项说明","O"]
["日常维护维修","PS_JG_RCWHWX","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["日常维护维修","PS_JG_RCWHWX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["日常维护维修","PS_JG_RCWHWX","-","维护维修内容","WHWXNR","字符型",255,"-","M"]
["日常维护维修","PS_JG_RCWHWX","-","设备设施","SBSS","字符型",255,"关联设备设施的标识码， 存在多个 设备设施用英文分号“;”分隔","M"]
["日常维护维修","PS_JG_RCWHWX","-","处理结果","CLJG","字符型",255,"-","O"]
["日常维护维修","PS_JG_RCWHWX","-","处理日期","CLRQ","日期型","-","-","O"]
["日常维护维修","PS_JG_RCWHWX","-","处理人员","CLRY","字符型",32,"-","O"]
["日常维护维修","PS_JG_RCWHWX","-","联系电话","LXDH","字符型",16,"-","O"]
["日常维护维修","PS_JG_RCWHWX","-","养护单位","YHDW","字符型",100,"单位名称","O"]
["日常维护维修","PS_JG_RCWHWX","-","设施权属单位","SSQSDW","字符型",100,"单位名称","O"]
["日常维护维修","PS_JG_RCWHWX","-","检测方法","JCFF","字符型",255,"-","M"]
["日常维护维修","PS_JG_RCWHWX","-","检测结论","JCJL","字符型",255,"-","M"]
["日常维护维修","PS_JG_RCWHWX","-","附件","FJ","二进制型","-","-","O"]
["日常维护维修","PS_JG_RCWHWX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["突发事件抢修","PS_JG_TFSJQX","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["突发事件抢修","PS_JG_TFSJQX","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["突发事件抢修","PS_JG_TFSJQX","-","事件名称","SJMC","字符型",50,"-","M"]
["突发事件抢修","PS_JG_TFSJQX","-","事件说明","SJSM","字符型",255,"-","O"]
["突发事件抢修","PS_JG_TFSJQX","-","地址","DZ","字符型",255,"-","O"]
["突发事件抢修","PS_JG_TFSJQX","-","关联基础设施","GLJCSS","字符型",32,"燃气/供水/排水/道路/桥梁，存在多 个设备设施用英文分号“;”分隔","M"]
["突发事件抢修","PS_JG_TFSJQX","-",{"$nulls":4},"1(一级)/2(二级)/3(三级)/4(四级)； 参照《江苏省突发事件总体应急预 案》中应急响应分级的规定"]
["突发事件抢修","PS_JG_TFSJQX","-","响应级别","XYJB","整型","-",null,"M"]
["突发事件抢修","PS_JG_TFSJQX","-","现场照片","XCZP","二进制型","-","-","M"]
["突发事件抢修","PS_JG_TFSJQX","-","抢修内容","QXNR","字符型",255,"抢修内容及处理方法","M"]
["突发事件抢修","PS_JG_TFSJQX","-","处理结果","CLJG","字符型",255,"-","O"]
["突发事件抢修","PS_JG_TFSJQX","-","处理日期","CLRQ","日期型","-","-","O"]
["突发事件抢修","PS_JG_TFSJQX","-","处理人员","CLRY","字符型",32,"-","O"]
["突发事件抢修","PS_JG_TFSJQX","-","处理单位","CLDW","字符型",100,"单位名称","O"]
["突发事件抢修","PS_JG_TFSJQX","-","附件","FJ","二进制型","-","-","M"]
["突发事件抢修","PS_JG_TFSJQX","-","备注","BZ","字符型",255,"相关事项说明","O"]
["养护记录","PS_JG_YHJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["养护记录","PS_JG_YHJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["养护记录","PS_JG_YHJL","-","养护对象","YHDX","字符型",255,"-","M"]
["养护记录","PS_JG_YHJL","-","养护日期","YHRQ","日期型","-","-","M"]
["养护记录","PS_JG_YHJL","-","养护内容","YHNR","字符型",255,"-","O"]
["养护记录","PS_JG_YHJL","-","作业人员","ZYRY","字符型",32,"-","M"]
["养护记录","PS_JG_YHJL","-","附件","FJ","二进制型","-","-","O"]
["养护记录","PS_JG_YHJL","-","备注","BZ","字符型",255,"相关事项说明","O"]
["巡检记录","PS_JG_XJJL","-","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["巡检记录","PS_JG_XJJL","-","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["巡检记录","PS_JG_XJJL","-","巡检对象","XJDX","整型","-","燃 气 、 排 水 设 施 填 写 ； 1( 管 道)/2(场站)/3(用户)/4(其它)","M"]
["巡检记录","PS_JG_XJJL","-","检查单元","JCDY","字符型",255,"-","O"]
["巡检记录","PS_JG_XJJL","-","检查项目","JCXM","字符型",255,"-","O"]
["巡检记录","PS_JG_XJJL","-","检查方法","JCFF","字符型",255,"-","O"]
["巡检记录","PS_JG_XJJL","-","检查内容","JCNR","字符型",255,"-","M"]
["巡检记录","PS_JG_XJJL","-","检查结果","JCJG","字符型",255,"-","O"]
["巡检记录","PS_JG_XJJL","-","存在隐患","CZYH","字符型",255,"-","O"]
["巡检记录","PS_JG_XJJL","-","检查日期","JCRQ","时间日期型","-","-","M"]
["巡检记录","PS_JG_XJJL","-","检查人员","JCRY","字符型",32,"-","O"]
["巡检记录","PS_JG_XJJL","-","设施权属单位","SSQSDW","字符型",100,"单位名称","M"]
["巡检记录","PS_JG_XJJL","-","主管单位","ZGDW","字符型",100,"单位名称","O"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","设施编码","SSBM","字符型",17,"与被检测检查井的编码一致","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","检测时间","JCSJ","时间日期型","-","-","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","所在道路","SZDL","字符型",50]
["检查井缺陷检测","PS_JG_JCJQXJC","点","检测单位","JCDW","字符型",100,"单位名称","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","检测人","JCR","字符型",32,"-","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","联系电话","LXDH","字符型",16,"检测单位联系电话","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","检查井材质","JCJCZ","整型","-","1(水泥)/2(砖)","O"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","井盖形状","JGCZ","字符型",10,"-","O"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","井盖材质","JGCZ","字符型",10,"-","O"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","缺陷描述",null,"字符型",null,"检查井情况缺陷描述，参照 CJJ 181 《城镇排水管道检测与评估技术规 程》"]
["检查井缺陷检测","PS_JG_JCJQXJC","点",null,"QXMS",null,255,null,"M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","建设年代","JSND","字符型",10,"如：“1991”","O"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","影像文件","YXWJ","二进制型","-","检测影像文件","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","填报单位","TBDW","字符型",100,"单位名称","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","填报日期","TBRQ","日期型","-","-","M"]
["检查井缺陷检测","PS_JG_JCJQXJC","点","备注","BZ","字符型",100,"相关事项说明","O"]
["管道缺陷检测","PS_JC_GDQXJC","点","标识码","BSM","字符型",32,"自动生成，唯一","M","管道缺陷检测 缺少必给\n字段：行政区划代码，检测人，联系电话，检测方法，检测方向，封堵情况，影像文件，填报单位，填报日期"]
["管道缺陷检测","PS_JC_GDQXJC","点","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","设施编码","SSBM","字符型",17,"与被检测管道的编码一致","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","检测时间","JCSJ","时间日期型","-","-","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","检测单位","JCDW","字符型",100,"单位名称","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","检测人","JCR","字符型",32,"-","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","联系电话","LXDH","字符型",16,"检测单位联系电话","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","检测方法","JCFF","整型","-","1(CCTV)/2(声纳)/3(潜望镜)/4(其 它)","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","检测方向","JCFX","整型","-","1(与流向一致)/2(与流向不一致)","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","封堵情况","FDQK","字符型",100,"说明封堵情况","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","淤泥厚度","YNHD","浮点型",5.3,"单位：毫米","O"]
["管道缺陷检测","PS_JC_GDQXJC","点","功能性缺陷类型","GNXQXLX","整型","-","0(无缺陷)/1(沉积)/2(结垢)/3(障 碍物)4(残墙、坝根)/5(树根)/6(浮 渣)/7(封堵)/8(其它)","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","功能性缺陷长度","GNXQXCD","浮点型",7.3,"功能性缺陷的长度，单位：米","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","功能性缺陷位置","GNXQXWZ","字符型",100,"功能性缺陷具体地址描述","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","功能性缺陷等级","GNXQXDJ","整型","-","1(轻微缺陷)/2(中等缺陷)/3(严重 缺陷)/4(重大缺陷)，参照 CJJ 181 《城镇排水管道检测与评估技术规 程》","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","结构性缺陷类型","JGXQXLX","整型",null,"0(无缺陷)/1(破裂)/2(变形)/3(腐 蚀 )/4( 错 口 )/5( 起 伏 )/6( 脱 节)/7(接口材料脱落)/8(支管暗 接)/9(异物穿入)/10(渗漏)/11(其 它)","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","结构性缺陷长度","JGXQXCD","浮点型",7.3,"结构性缺陷的长度，单位：米","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","结构性缺陷位置","JGXQXWZ","字符型",100,"结构性缺路且体地址描述","C"]
["管道缺陷检测","PS_JC_GDQXJC","点","结构性缺陷等级","JGXQXDJ","整型",null,"1(轻微缺陷)/2(中等缺陷)/3(严重缺 陷)/4(重大缺陷)，参照CJJ 181《城镇 排水管道检测与评估技术规程》","c"]
["管道缺陷检测","PS_JC_GDQXJC","点","修复指数 RI","XFZSRI","浮点型",4.2,"-","O"]
["管道缺陷检测","PS_JC_GDQXJC","点","养护指数 MI","YHZSMI","浮点型",4.2,"-","O"]
["管道缺陷检测","PS_JC_GDQXJC","点","缺陷描述","QXMS","字符型",255,"管道情况缺陷描述","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","影像文件","YXWJ","二进制型","-","检测影像文件","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","填报单位","TBDW","字符型",100,"单位名称","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","填报日期","TBRQ","日期型","-","-","M"]
["管道缺陷检测","PS_JC_GDQXJC","点","备注","BZ","字符型",100,"相关事项说明","O"]
["第三方施工专项","PS_JG_DSFSGZX","面","标识码","BSM","字符型",32,"自动生成，唯一","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","行政区划代码","XZQHDM","字符型",6,"见附录 A 表 A.1 行政区划代码表","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","项目名称","XMMC","字符型",255,"-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","项目内容","XMNR","字符型",255,"-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","所在街道","SZJD","字符型",255,"-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","施工项目地址","XXDZ","字符型",255,"-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","计划开始时间","JHKSSJ","日期型","-","-","O"]
["第三方施工专项","PS_JG_DSFSGZX","面","计划结束时间","JHJSSJ","日期型","-","-","O"]
["第三方施工专项","PS_JG_DSFSGZX","面","实际开始时间","SJKSSJ","日期型","-","-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","实际结束时间","SJJSSJ","日期型","-","-","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","施工深度","SGSD","浮点型",6.2,"第三方施工开挖最大深度","M"]
["第三方施工专项","PS_JG_DSFSGZX","面","建设单位","JSDW","字符型",255,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","建设单位负责人","JSDWFZR","字符型",16,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","建设单位负责人联 系电话","JSDWFZRLXDH","字符型",16,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","施工单位","SGDW","字符型",255,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","施工单位负责人","SGDWFZR","字符型",16,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","施工单位负责人联 系电话","SGDWFZRLXDH","字符型",16,null,"M"]
["第三方施工专项","PS_JG_DSFSGZX","面","监理单位","JLDW","字符型",255,null,"O"]
["第三方施工专项","PS_JG_DSFSGZX","面","监理单位负责人","JLDWFZR","字符型",255,null,"O"]
["第三方施工专项","PS_JG_DSFSGZX","面","监理单位负责人联 系电话","JLDWFZRLXDH","字符型",255,null,"O"]
["第三方施工专项","PS_JG_DSFSGZX","面","备注","BZ","字符型",255,"相关事项说明","O"]
["调蓄设施属性结构表","ps_js_txss",null,"标识码","bsm","字符型",32,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"调蓄设施编码","txssbm","字符型",32,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"类别","lb","整型",null,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"权属单位","qsdw","字符型",30,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"所属排水系统","sspsxt","字符型",32,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"调蓄设施名称","txssmc","字符型",30,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"最高水位","zgsw","浮点型",8.2,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"最低水位","zdsw","浮点型",8.2,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"调蓄设施容积","txssrj","浮点型",10.2,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"调蓄设施类型","txsslx","整型",null,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"调蓄设施材质","txsscz","整型",null,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"建设时间","jssj","日期型",null,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"备注","bz","字符型",255,null,"O"]
["调蓄设施属性结构表","ps_js_txss",null,"空间信息","kjxx","geometry",null,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["调蓄设施属性结构表","ps_js_txss",null,"同步时间","tbsj","日期型",null,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"标识码","bsm","字符型",32,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"行泄通道编码","xxtdbm","字符型",32,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"地表雨水行泄通道类型","dbysxxtdlx","整型",null,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"路面等级与面层类型","lmdjymclx","整型",null,null,"O"]
["行泄通道属性结构表","ps_js_xxtd",null,"地表雨水行泄通道糙率","dbysxxtdcl","浮点型",9.4,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"数据来源","sjly","字符型",50,null,"O"]
["行泄通道属性结构表","ps_js_xxtd",null,"数据获取日期","sjhqrq","日期型",null,null,"O"]
["行泄通道属性结构表","ps_js_xxtd",null,"填报单位","tbdw","字符型",30,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"填报日期","tbrq","日期型",null,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"道路名称","dlmc","字符型",255,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"地址","dz","字符型",255,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"长度","cd","浮点型",10.3,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"面积","mj","浮点型",12.2,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"备注","bz","字符型",255,null,"O"]
["行泄通道属性结构表","ps_js_xxtd",null,"空间信息","kjxx","geometry",null,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["行泄通道属性结构表","ps_js_xxtd",null,"同步时间","tbsj","日期型",null,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"标识码","bsm","字符型",32,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"河道编码","hdbm","字符型",32,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"河流名称","hlmc","字符型",20,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"河段长度","hdcd","浮点型",11.3,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"起点桩号编码","qdzhbm","字符型",17,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"终点桩号编码","zdzhbm","字符型",17,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"起点河底标高","qdhdbg","浮点型",10.3,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"终点河底标高","zdhdbg","浮点型",10.3,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"常水位","csw","浮点型",8.2,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"警戒水位","jjsw","浮点型",8.2,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"备注","bz","字符型",255,null,"O"]
["主要河道属性结构表","ps_js_zyhd",null,"空间信息","kjxx","geometry",null,null,"O"]
["主要河道属性结构表","ps_js_zyhd",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["主要河道属性结构表","ps_js_zyhd",null,"同步时间","tbsj","日期型",null,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"标识码","bsm","字符型",64,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"所属排水系统","sspsxt","字符型",32,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"排水户名称","pshmc","字符型",50,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"排水户地址","pshdz","字符型",255,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"接入检查井编码","jrjcjbm","字符型",32,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"组织机构代码","zzjgdm","字符型",32,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"法人代表","frdb","字符型",16,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"联系电话","lxdh","字符型",16,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"主管单位","zgdw","字符型",32,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"排水户类型","pshlx","字符型",200,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"是否为重点排水户","sfwzdpsh","布尔型",null,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"主要生产工艺","zyscgy","字符型",200,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"排水许可证编号","psxkzbh","字符型",16,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"许可证颁发日期","xkzbfrq","日期型",null,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"用户总量","yhzl","浮点型",12.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"自备水量","zbsl","浮点型",12.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"总排水量","zpsl","浮点型",12.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"生产污水量","scwsl","浮点型",12.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"生活污水量","shwsl","浮点型",12.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"第一类污染物名称","dylwrwmc","字符型",50,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"第二类污染物名称","delwrwmc","字符型",50,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"污水处理方式","wsclfs","整型",null,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"污水处理规模","wsclgm","浮点型",14.2,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"技术资料文件","jszlwj","字符型",null,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"数据来源","sjly","字符型",64,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"数据获取日期","sjhqrq","日期型",null,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"填报单位","tbdw","字符型",100,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"填报日期","tbrq","日期型",null,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"备注","bz","字符型",255,null,"O"]
["重点排水户属性结构表","ps_js_psh",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"同步时间","tbsj","日期型",null,null,"M"]
["重点排水户属性结构表","ps_js_psh",null,"空间信息","kjxx","geometry",null,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"标识码","bsm","字符型",64,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"所属排水系统","sspsxt","字符型",32,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"截流设施类型","jlsslx","整型",null,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"截流设施连接管渠编码","jlssljgqbm","字符型",32,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"技术资料文件","jszlwj","字符型",null,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"数据来源","sjly","字符型",64,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"数据获取日期","sjhqrq","日期型",null,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"填报单位","tbdw","字符型",30,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"填报日期","tbrq","日期型",null,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"截流内部设施编码","jlnbssbm","字符型",32,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"截流量","jll","浮点型",6.2,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"截流曲线","jlqx","整型",null,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"设施状态","sszt","整型",null,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"备注","bz","字符型",255,null,"O"]
["截流设施属性结构表","ps_js_jlss",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"同步时间","tbsj","日期型",null,null,"M"]
["截流设施属性结构表","ps_js_jlss",null,"空间信息","kjxx","geometry",null,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"标识码","bsm","字符型",32,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"易涝点编码","yldbm","字符型",32,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"积淹深度","jysd","浮点型",6.2,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"积淹范围","jyfw","字符型",255,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"退水时长","tssc","整型",null,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"积水时间","jssj","日期型",null,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"影响人数","yxrs","整型",null,null,"O"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"填报单位","tbdw","字符型",100,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"填报日期","tbrq","日期型",null,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"备注","bz","字符型",255,null,"O"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["易涝点积水事件信息属性结构表","ps_jc_yldjssj",null,"同步时间","tbsj","日期型",null,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"标识码","bsm","字符型",32,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"行政区划代码","xzqhdm","字符型",6,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"年份","nf","字符型",64,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"风险名称","fxmc","字符型",64,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"风险等级","fxdj","字符型",64,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"风险来源","fxly","字符型",255,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"风险内容","fxnr","字符型",255,null,"O"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"面积","mj","浮点型",12.2,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"管控措施","gkcs","字符型",255,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"是否管控","sfgk","布尔型",null,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"原始库主键标志","yskzjbz","字符型",64,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"数据同步状态","sjtbzt","字符型",16,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"同步时间","tbsj","日期型",null,null,"M"]
["雨水风险管控属性结构表","ps_jg_ysfxgk",null,"空间信息","kjxx","geometry",null,null,"M"]

{"sheet":"第三方分类","index":4,"n_rows":281,"n_cols":7,"rows_kept":281,"cut":false,"hidden":false,"merged":[]}
["表名","表注释","字段序号","字段名","字段注释","字段类型","非空"]
["sg_jc_jcsb","表7监测设备属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",2,"dwbsm","点位标识码","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",3,"jcssid","监测设施编号","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",4,"xmbh","项目编号","varchar(32)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",5,"jcssqsqy","监测设施权属企业","varchar(100)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",6,"sblx","设备类型","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",7,"sbmc","设备名称","varchar(50)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",8,"sbxh","设备型号","varchar(32)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",9,"jczb","监测指标","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",10,"cjpl","采集频率","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",11,"scpl","上传频率","varchar(32)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",12,"sbzt","设备状态","int4","M"]
["sg_jc_jcsb","表7监测设备属性结构表",13,"csmc","厂商名称","varchar(50)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",14,"xdgd","相对高度","numeric(10,3)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",15,"azsj","安装时间","date","O"]
["sg_jc_jcsb","表7监测设备属性结构表",16,"azwhdw","安装维护单位","varchar(100)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",17,"gdfs","供电方式","varchar(32)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",18,"bz","备注","varchar(255)","O"]
["sg_jc_jcsb","表7监测设备属性结构表",19,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",20,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jc_jcsb","表7监测设备属性结构表",21,"tbsj","同步时间","timestamp","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",2,"sbbsm","设备标识码","varchar(64)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",3,"sblx","设备类型","varchar(32)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",4,"jczb","监测指标","varchar(32)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",5,"bjyz","报警阈值","numeric(13,3)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",6,"bz","备注","varchar(255)","O"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",7,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",8,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jc_jcxyz","表8监测项阈值属性结构表",9,"tbsj","同步时间","timestamp","M"]
["sg_jc_spjk","表9视频监控属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jc_spjk","表9视频监控属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jc_spjk","表9视频监控属性结构表",3,"sbmc","设备名称","varchar(50)","M"]
["sg_jc_spjk","表9视频监控属性结构表",4,"azdz","安装地址","varchar(255)","M"]
["sg_jc_spjk","表9视频监控属性结构表",5,"jkdx","监控对象","varchar(255)","M"]
["sg_jc_spjk","表9视频监控属性结构表",6,"sbxh","设备型号","varchar(255)","M"]
["sg_jc_spjk","表9视频监控属性结构表",7,"sccj","生产厂家","varchar(100)","O"]
["sg_jc_spjk","表9视频监控属性结构表",8,"cqdw","产权单位","varchar(100)","M"]
["sg_jc_spjk","表9视频监控属性结构表",9,"spdz","视频地址","varchar(255)","O"]
["sg_jc_spjk","表9视频监控属性结构表",10,"bz","备注","varchar(255)","O"]
["sg_jc_spjk","表9视频监控属性结构表",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["sg_jc_spjk","表9视频监控属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jc_spjk","表9视频监控属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jc_spjk","表9视频监控属性结构表",14,"tbsj","同步时间","timestamp","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",3,"xmbm","项目编码","varchar(32)","O"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",4,"sjbm","事件编码","varchar(32)","O"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",5,"sjms","事件描述","varchar(255)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",6,"cjsj","惩戒时间","varchar(100)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",7,"bcjdw","被惩戒单位","varchar(100)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",8,"cjjg","惩戒结果","varchar(255)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",9,"fbdw","发布单位","varchar(100)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",10,"fbsj","发布时间","date","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",11,"fj","附件","bytea","O"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",12,"bz","备注","varchar(255)","O"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",13,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",14,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dsfsglhcj","表5第三方施工联合惩戒属性结构表",15,"tbsj","同步时间","timestamp","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",3,"xmbm","项目编码","varchar(32)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",4,"dsfphsjbsm","第三方破坏事件标识码","varchar(64)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",5,"sbsj","上报时间","date","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",6,"yhmc","隐患名称","varchar(64)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",7,"yhddz","隐患点地址","varchar(255)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",8,"yhms","隐患描述","varchar(255)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",9,"yhxczp","隐患现场照片","bytea","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",10,"sbr","上报人","varchar(32)","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",11,"sbrlxdh","上报人联系电话","varchar(16)","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",12,"yhczdw","隐患处置单位","varchar(100)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",13,"czfzr","处置负责人","varchar(32)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",14,"czfzrlxdh","处置负责人联系电话","varchar(16)","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",15,"yhslsj","隐患受理时间","date","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",16,"yhczzt","隐患处置状态","int4","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",17,"yhczjs","隐患处置简述","varchar(255)","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",18,"yhczbg","隐患处置报告","bytea","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",19,"czwcsj","处置完成时间","date","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",20,"bz","备注","varchar(255)","O"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",21,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",22,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dsfsgphczjg","表4第三方施工破坏处置结果属性结构表",23,"tbsj","同步时间","timestamp","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",3,"sjmc","事件名称","varchar(255)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",4,"xmbm","项目编码","varchar(32)","O"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",5,"sjxz","事件性质","int4","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",6,"fssj","发生时间","date","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",7,"fsdd","发生地点","varchar(255)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",8,"sgdw","施工单位","varchar(100)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",9,"sfycz","是否已处置","bool","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",10,"gxqsdw","管线权属单位","varchar(100)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",11,"phsjms","破坏事件描述","varchar(255)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",12,"czwcsj","处置完成时间","date","O"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",13,"bz","备注","varchar(255)","O"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",14,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",15,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",16,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dsfsgphsj","表3第三方施工破坏事件属性结构表",17,"tbsj","同步时间","timestamp","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",3,"xmbm","项目编码","varchar(32)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",4,"xmdm","项目代码","varchar(32)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",5,"gxqsdw","管线权属单位","varchar(255)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",6,"gxlx","管线类型","varchar(100)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",7,"gxqsdwclr","处理人","varchar(255)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",8,"gxdwfzrlxdh","处理人联系电话","varchar(100)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",9,"wts","委托书","bytea","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",10,"hxdzwj","红线电子文件","bytea","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",11,"gxt","管线图","bytea","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",12,"sfygx","是否有管线","bool","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",13,"xcjddz","现场交底地址","varchar(100)","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",14,"xcjdrq","现场交底日期","varchar(100)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",15,"sfwcjd","是否完成交底","bool","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",16,"dtrq","动土日期","date","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",17,"bz","备注","varchar(255)","O"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",18,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",19,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",20,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dsfsgsqgl","表2 第三方施工事前管理属性结构表",21,"tbsj","同步时间","timestamp","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",3,"xmdm","项目代码","varchar(32)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",4,"sgzt","施工状态","varchar(16)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",5,"sgxkxx","施工许可信息","varchar(255)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",6,"dlwjspzt","道路挖掘审批状态","varchar(16)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",7,"xmmc","项目名称","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",8,"dkm","地块名","varchar(255)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",9,"xmlx","项目类型","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",10,"szjd","所在街道","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",11,"sgxmdz","施工项目地址","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",12,"jhkssj","计划开始时间","date","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",13,"jhjssj","计划结束时间","date","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",14,"sjkssj","实际开始时间","date","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",15,"sjjssj","实际结束时间","date","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",16,"sgsd","施工深度","numeric(8,2)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",17,"jsdw","建设单位","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",18,"jsdwfzr","建设单位负责人","varchar(32)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",19,"jsdwfzrlxdh","建设单位负责人联\n系电话","varchar(16)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",20,"sgdw","施工单位","varchar(255)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",21,"sgdwfzr","施工单位负责人","varchar(32)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",22,"sgdwfzrlxdh","施工单位负责人联\n系电话","varchar(16)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",23,"jldw","监理单位","varchar(255)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",24,"jldwfzr","监理单位负责人","varchar(32)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",25,"jldwfzrlxdh","监理单位负责人联\n系电话","varchar(16)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",26,"bz","备注","varchar(255)","O"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",27,"hxfw","红线范围","geometry(Geometry,4490)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",28,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",29,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",30,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dsfsgxmxx","表1 第三方施工项目信息属性结构表",31,"tbsj","同步时间","timestamp","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",3,"xmbm","项目编码","varchar(64)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",4,"sjbsm","事件标识码","varchar(32)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",5,"sjmc","事件名称","varchar(255)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",6,"sjms","事件描述","varchar(255)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",7,"sjlx","事件类型","int4","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",8,"sjjb","事件级别","varchar","O"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",9,"schy","所处行业","int4","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",10,"sjnf","事件年份","date","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",11,"hyjy","行业建议","varchar","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",12,"hyfx","行业分析","varchar","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",13,"cjjg","惩戒结果","varchar(1024)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",14,"fj","附件","bytea","O"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",15,"bz","备注","varchar(255)","O"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",16,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",17,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_dxdaalk","表17 第三方施工典型档案案例库属性结构表",18,"tbsj","同步时间","timestamp","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",2,"xmbm","项目编码","varchar(64)","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",3,"jcssid","监测设施编号","varchar(32)","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",4,"babh","备案编号","varchar(32)","O"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",5,"bar","备案人","varchar(32)","O"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",6,"basj","备案时间","varchar(100)","O"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",7,"bazt","备案状态","varchar(16)","O"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",8,"bz","备注","varchar(255)","O"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",9,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",10,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_jxbaxx","表15 第三方施工机械备案信息属性结构表",11,"tbsj","同步时间","timestamp","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",3,"sqglbsm","事前管理标识码","varchar(64)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",4,"sfygx","是否有管线","bool","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",5,"gxqsdw","管线权属单位","varchar(255)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",6,"gxqsdwclr","管线权属单位处理人","varchar(255)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",7,"gxdwclrlxdh","管线权属单位处理人联系电话","varchar(100)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",8,"gxqsdwclrclyj","管线权属单位处理人处理意见","varchar(255)","O"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",9,"gxtzwj","管线图纸文件","bytea","O"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",10,"gxfxsm","管线风险说明","varchar(255)","O"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",11,"bz","备注","varchar(255)","O"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_qsdwqr","表16 权属单位确认信息属性结构表",14,"tbsj","同步时间","timestamp","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",2,"sqglbsm","事前管理标识码","varchar(64)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",3,"gxbhfags","管线保护方案概述","varchar(255)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",4,"gxbhfawj","管线保护方案文件","bytea","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",5,"jsdwbhfaqrr","建设单位保护方案确认人","varchar(16)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",6,"jsdwbhfaqrsj","建设单位保护方案确认时间","timestamp","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",7,"sgdwbhfaqrr","施工单位保护方案确认人","varchar(16)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",8,"sgdwbhfaqrsj","施工单位保护方案确认时间","timestamp","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",9,"jldwbhfaqrr","监理单位保护方案确认人","varchar(16)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",10,"jldwbhfaqrsj","监理单位保护方案确认时间","timestamp","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",11,"bz","备注","varchar(255)","O"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_sfjdbhfa","表12现场交底保护方案属性结构表",14,"tbsj","同步时间","timestamp","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",2,"sqglbsm","事前管理标识码","varchar(64)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",3,"ecfhsj","二次复核时间","timestamp","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",4,"fhdw","复核单位","varchar(255)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",5,"fhry","复核人员","varchar(32)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",6,"fhrlxdh","复核人员联系电话","varchar(16)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",7,"fhzl","复核资料","bytea","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",8,"fhsm","复核说明","varchar(255)","O"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",9,"jsdwfhqrr","建设单位复核确认人","varchar(32)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",10,"jsdwfhqrsj","建设单位复核确认时间","timestamp","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",11,"sgdwfhqrr","施工单位复核确认人","varchar(32)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",12,"sgdwfhqrsj","施工单位复核确认时间","timestamp","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",13,"jldwfhqrr","监理单位复核确认人","varchar(32)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",14,"jldwfhqrsj","监理单位复核确认时间","timestamp","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",15,"bz","备注","varchar(255)","O"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",16,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",17,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_sfjdecfh","表11现场交底管线二次复核记录属性结构表",18,"tbsj","同步时间","timestamp","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",2,"sqglbsm","事前管理标识码","varchar(64)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",3,"gxjdcl","管线交底材料","bytea","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",4,"xcjdtpsp","现场交底照片\\视频","bytea","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",5,"jdqrd","现场签署的交底确认单","bytea","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",6,"qsdwqrr","权属单位确认人","varchar(16)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",7,"qsdwqrsj","权属单位确认时间","timestamp","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",8,"jsdwqrr","建设单位确认人","varchar(16)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",9,"jsdwqrsj","建设单位确认时间","timestamp","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",10,"sgdwqrr","施工单位确认人","varchar(16)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",11,"sgdwqrsj","施工单位确认时间","timestamp","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",12,"jldwqrr","监理单位确认人","varchar(16)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",13,"jldwqrsj","监理单位确认时间","timestamp","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",14,"bz","备注","varchar(255)","O"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",15,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",16,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_sfjdfb","表10四方交底记录附表属性结构表",17,"tbsj","同步时间","timestamp","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",2,"sqglbsm","事前管理标识码","varchar(64)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",3,"pzjhbh","旁站监护编号","varchar(32)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",4,"xmbm","项目编码","varchar(32)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",5,"sfjdid","四方交底编号","varchar(32)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",6,"gxqsdw","管线权属单位","varchar(255)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",7,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",8,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_sfjdpzjhjl","表13四方交底旁站监护记录属性结构表",9,"tbsj","同步时间","timestamp","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",2,"pzjhbh","旁站监护编号","varchar(32)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",3,"xcjhrq","现场监护日期","timestamp","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",4,"jhkssj","监护开始时间","timestamp","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",5,"jhjssj","监护结束时间","timestamp","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",6,"jhry","监护人员","varchar(16)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",7,"jhyrlxfs","监护人员联系方式","varchar(255)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",8,"sfwg","是否发现违规行为","bool","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",9,"wglx","违规行为类型","varchar(32)","O"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",10,"sftgzg","是否停工整改","bool","O"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",11,"zggzs","整改告知书","bytea","O"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",12,"bz","备注","varchar(255)","O"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",13,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",14,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_jg_sfjdpzjhjlmx","表14四方交底旁站监护记录明细属性结构表",15,"tbsj","同步时间","timestamp","M"]
["sg_js_jcd","表6监测点属性结构表",1,"bsm","标识码","varchar(32)","M"]
["sg_js_jcd","表6监测点属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["sg_js_jcd","表6监测点属性结构表",3,"dwmc","点位名称","varchar(64)","M"]
["sg_js_jcd","表6监测点属性结构表",4,"ssmc","设施名称","varchar(64)","O"]
["sg_js_jcd","表6监测点属性结构表",5,"ssbm","设施编码","varchar(17)","M"]
["sg_js_jcd","表6监测点属性结构表",6,"jcwz","监测位置","varchar(200)","O"]
["sg_js_jcd","表6监测点属性结构表",7,"gc","高程","numeric(10,3)","O"]
["sg_js_jcd","表6监测点属性结构表",8,"gcjz","高程基准","varchar(32)","O"]
["sg_js_jcd","表6监测点属性结构表",9,"bz","备注","varchar(255)","O"]
["sg_js_jcd","表6监测点属性结构表",10,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["sg_js_jcd","表6监测点属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["sg_js_jcd","表6监测点属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["sg_js_jcd","表6监测点属性结构表",13,"tbsj","同步时间","timestamp","M"]

{"sheet":"桥梁分类","index":5,"n_rows":160,"n_cols":7,"rows_kept":160,"cut":false,"hidden":false,"merged":[]}
["表名","表注释","字段序号","字段名","字段注释","字段类型","非空"]
["ql_jc_jcsb","监测设备属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",2,"dwbsm","点位标识码","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",3,"sblx","设备类型","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",4,"sbmc","设备名称","varchar(50)","M"]
["ql_jc_jcsb","监测设备属性结构表",5,"sbxh","设备型号","varchar(32)","O"]
["ql_jc_jcsb","监测设备属性结构表",6,"jczb","监测指标","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",7,"cjpl","采集频率","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",8,"scpl","上传频率","varchar(32)","M"]
["ql_jc_jcsb","监测设备属性结构表",9,"sbzt","设备状态","int4","M"]
["ql_jc_jcsb","监测设备属性结构表",10,"csmc","厂商名称","varchar(50)","O"]
["ql_jc_jcsb","监测设备属性结构表",11,"xdgd","相对高度","numeric(10,3)","O"]
["ql_jc_jcsb","监测设备属性结构表",12,"azsj","安装时间","date","O"]
["ql_jc_jcsb","监测设备属性结构表",13,"azwhdw","安装维护单位","varchar(100)","O"]
["ql_jc_jcsb","监测设备属性结构表",14,"gdfs","供电方式","varchar(32)","O"]
["ql_jc_jcsb","监测设备属性结构表",15,"bz","备注","varchar(255)","O"]
["ql_jc_jcsb","监测设备属性结构表",16,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jc_jcsb","监测设备属性结构表",17,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jc_jcsb","监测设备属性结构表",18,"tbsj","同步时间","timestamp","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",2,"sbbsm","设备标识码","varchar(64)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",3,"sblx","设备类型","varchar(32)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",4,"jczb","监测指标","varchar(32)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",5,"bjyz","报警阈值","numeric(13,3)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",6,"bz","备注","varchar(255)","O"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",7,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",8,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jc_jcxyz","桥梁监测项阈值属性结构表",9,"tbsj","同步时间","timestamp","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",3,"sbmc","设备名称","varchar(50)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",4,"azdz","安装地址","varchar(255)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",5,"jkdx","监控对象","varchar(255)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",6,"sbxh","设备型号","varchar(255)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",7,"sccj","生产厂家","varchar(100)","O"]
["ql_jc_spjk","桥梁视频监控属性结构表",8,"cqdw","产权单位","varchar(100)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",9,"spdz","视频地址","varchar(255)","O"]
["ql_jc_spjk","桥梁视频监控属性结构表",10,"bz","备注","varchar(255)","O"]
["ql_jc_spjk","桥梁视频监控属性结构表",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jc_spjk","桥梁视频监控属性结构表",14,"tbsj","同步时间","timestamp","M"]
["ql_jg_fxpg","桥梁风险评估信息表",1,"bsm","标识码","varchar(32)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",3,"qlmc","桥梁名称","varchar(32)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",4,"qlbh","桥梁编号","varchar(32)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",5,"pgsj","评估时间","timestamp","M"]
["ql_jg_fxpg","桥梁风险评估信息表",6,"fxmc","风险名称","varchar(64)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",7,"fxdj","风险等级","int4","M"]
["ql_jg_fxpg","桥梁风险评估信息表",8,"fxms","风险描述","varchar(255)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",9,"gkzt","管控状态","varchar(64)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",10,"bz","备注","varchar(255)","O"]
["ql_jg_fxpg","桥梁风险评估信息表",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jg_fxpg","桥梁风险评估信息表",14,"tbsj","同步时间","timestamp","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",3,"xmmc","项目名称","varchar(255)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",4,"xmlx","项目类型","varchar(8)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",5,"zgdw","主管单位","varchar(100)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",6,"xmnr","项目内容","varchar(255)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",7,"jhnd","计划年度","int4","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",8,"xmjszq","项目建设周期","int4","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",9,"xmtze","项目投资额","numeric(13,3)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",10,"bz","备注","varchar(255)","O"]
["ql_jg_jhxm","桥梁计划项目属性结构表",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jg_jhxm","桥梁计划项目属性结构表",14,"tbsj","同步时间","timestamp","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",3,"xmmc","项目名称","varchar(255)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",4,"xmdm","项目代码","varchar(50)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",5,"xmbm","项目编码","varchar(32)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",6,"xmlx","项目类型","varchar(8)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",7,"zgdw","主管单位","varchar(100)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",8,"xmnr","项目内容","varchar(255)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",9,"xmtze","项目投资额","numeric(13,3)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",10,"xxdz","详细地址","varchar(255)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",11,"lxxkxx","立项许可信息","varchar(255)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",12,"ghxkxx","规划许可信息","varchar(255)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",13,"sgxkxx","施工许可信息","varchar(255)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",14,"jgysxx","竣工验收信息","varchar(255)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",15,"jsdw","建设单位","varchar(100)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",16,"sjdw","设计单位","varchar(100)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",17,"sgdw","施工单位","varchar(100)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",18,"jldw","监理单位","varchar(100)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",19,"sjkssj","实际开始时间","date","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",20,"sjjssj","实际结束时间","date","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",21,"jsjd","建设进度","varchar(16)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",22,"ywctze","已完成投资额","numeric(13,3)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",23,"bz","备注","varchar(255)","O"]
["ql_jg_jsxm","桥梁建设项目属性结构表",24,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",25,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",26,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_jg_jsxm","桥梁建设项目属性结构表",27,"tbsj","同步时间","timestamp","M"]
["ql_js_jcd","桥梁监测点属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_js_jcd","桥梁监测点属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_js_jcd","桥梁监测点属性结构表",3,"dwmc","点位名称","varchar(64)","M"]
["ql_js_jcd","桥梁监测点属性结构表",4,"ssmc","设施名称","varchar(64)","O"]
["ql_js_jcd","桥梁监测点属性结构表",5,"ssbm","设施编码","varchar(17)","M"]
["ql_js_jcd","桥梁监测点属性结构表",6,"jcwz","监测位置","varchar(200)","O"]
["ql_js_jcd","桥梁监测点属性结构表",7,"gc","高程","numeric(10,3)","O"]
["ql_js_jcd","桥梁监测点属性结构表",8,"gcjz","高程基准","varchar(32)","O"]
["ql_js_jcd","桥梁监测点属性结构表",9,"bz","备注","varchar(255)","O"]
["ql_js_jcd","桥梁监测点属性结构表",10,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_js_jcd","桥梁监测点属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_js_jcd","桥梁监测点属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_js_jcd","桥梁监测点属性结构表",13,"tbsj","同步时间","timestamp","M"]
["ql_js_ql","桥梁属性结构表",1,"bsm","标识码","varchar(32)","M"]
["ql_js_ql","桥梁属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["ql_js_ql","桥梁属性结构表",3,"qlmc","桥梁名称","varchar(32)","M"]
["ql_js_ql","桥梁属性结构表",4,"jgny","竣工年月","varchar(8)","M"]
["ql_js_ql","桥梁属性结构表",5,"szdlmc","所在道路名称","varchar(32)","O"]
["ql_js_ql","桥梁属性结构表",6,"dldj","道路等级","int4","M"]
["ql_js_ql","桥梁属性结构表",7,"kjfl","跨径分类","int4","M"]
["ql_js_ql","桥梁属性结构表",8,"jglx","结构类型","int4","M"]
["ql_js_ql","桥梁属性结构表",9,"kjzh","跨径组合","varchar","O"]
["ql_js_ql","桥梁属性结构表",10,"qlzc","桥梁总长","numeric(12,2)","M"]
["ql_js_ql","桥梁属性结构表",11,"qlzk","桥梁总宽","numeric(8,2)","M"]
["ql_js_ql","桥梁属性结构表",12,"kydw","跨越地物","int4","M"]
["ql_js_ql","桥梁属性结构表",13,"thdj","通航等级","int4","M"]
["ql_js_ql","桥梁属性结构表",14,"sfdzd","是否独柱墩","bool","M"]
["ql_js_ql","桥梁属性结构表",15,"qmmj","桥面面积","numeric(12,2)","M"]
["ql_js_ql","桥梁属性结构表",16,"kzld","抗震烈度","int4","M"]
["ql_js_ql","桥梁属性结构表",17,"yhlb","养护类别","int4","M"]
["ql_js_ql","桥梁属性结构表",18,"yhdj","养护等级","int4","M"]
["ql_js_ql","桥梁属性结构表",19,"qlwhzk","桥梁完好状况","varchar(8)","O"]
["ql_js_ql","桥梁属性结构表",20,"qljgzk","桥梁结构状况","varchar(8)","O"]
["ql_js_ql","桥梁属性结构表",21,"jcrq","检测日期","date","O"]
["ql_js_ql","桥梁属性结构表",22,"jcbg","检测报告","bytea","M"]
["ql_js_ql","桥梁属性结构表",23,"jsdw","建设单位","varchar(100)","O"]
["ql_js_ql","桥梁属性结构表",24,"sjdw","设计单位","varchar(100)","O"]
["ql_js_ql","桥梁属性结构表",25,"sgdw","施工单位","varchar(100)","O"]
["ql_js_ql","桥梁属性结构表",26,"jldw","监理单位","varchar(100)","O"]
["ql_js_ql","桥梁属性结构表",27,"gldw","管理单位","varchar(100)","M"]
["ql_js_ql","桥梁属性结构表",28,"yhdw","养护单位","varchar(100)","M"]
["ql_js_ql","桥梁属性结构表",29,"sfjggz","是否加固改造","bool","M"]
["ql_js_ql","桥梁属性结构表",30,"sfyjjcxt","是否已建监测系统","bool","M"]
["ql_js_ql","桥梁属性结构表",31,"bz","备注","varchar(255)","O"]
["ql_js_ql","桥梁属性结构表",32,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["ql_js_ql","桥梁属性结构表",33,"yskzjbz","原始库主键标志","varchar(64)","M"]
["ql_js_ql","桥梁属性结构表",34,"sjtbzt","数据同步状态","varchar(16)","M"]
["ql_js_ql","桥梁属性结构表",35,"tbsj","同步时间","timestamp","M"]
["QL_JC_SJFXBG","数据分析报告",1,"BSM","标识码","字符型","M"]
["QL_JC_SJFXBG","数据分析报告",2,"BGMC","报告名称","字符型","M"]
["QL_JC_SJFXBG","数据分析报告",3,"BGSCSJ","报告生成时间","时间日期型","M"]
["QL_JC_SJFXBG","数据分析报告",4,"BGFJ","报告附件","二进制型","M"]
["QL_JC_SJFXBG","数据分析报告",5,"BZ","备注","字符型","O"]
["QL_JG_DQJC","定期检测",1,"BSM","标识码","字符型","M"]
["QL_JG_DQJC","定期检测",2,"XZQHDM","行政区划代码","字符型","M"]
["QL_JG_DQJC","定期检测",3,"JCDX","检测对象","字符型","M"]
["QL_JG_DQJC","定期检测",4,"JCSJ","检测时间","时间日期型","M"]
["QL_JG_DQJC","定期检测",5,"JCDW","检测单位","字符型","O"]
["QL_JG_DQJC","定期检测",6,"JCR","检测人","字符型","O"]
["QL_JG_DQJC","定期检测",7,"JCDWLXDH","检测单位联系电话","字符型","O"]
["QL_JG_DQJC","定期检测",8,"JCFF","检测方法","字符型","M"]
["QL_JG_DQJC","定期检测",9,"JCJL","检测结论","字符型","M"]
["QL_JG_DQJC","定期检测",10,"BZ","备注","字符型","O"]

{"sheet":"道路分类","index":6,"n_rows":346,"n_cols":7,"rows_kept":346,"cut":false,"hidden":false,"merged":[]}
["表名","表注释","字段序号","字段名","字段注释","字段类型","非空"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",3,"gcmc","工程名称","varchar(100)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",4,"jcdw","检测单位","varchar(100)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",5,"pgdybh","评估单元编号","varchar(64)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",6,"pgdylc","评估单元里程","int4","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",7,"pgfz","评估分值","numeric(6,2)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",8,"pgsj","评估时间","date","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",9,"dlmc","道路名称","varchar(32)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",10,"dlqd","道路起点","varchar(100)","O"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",11,"dlzd","道路终点","varchar(100)","O"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",12,"dldj","道路等级","int4","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",13,"fxdj","风险等级","int4","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",14,"fj","附件","bytea","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",15,"bz","备注","varchar(255)","O"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",16,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",17,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",18,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jc_dltxfx","道路塌陷风险属性结构表",19,"tbsj","同步时间","timestamp","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",3,"dlmc","道路名称","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",4,"sgmc","事故名称","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",5,"sgzt","事故状态","varchar(16)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",6,"sgdj","事故等级","varchar(16)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",7,"sgly","事故来源","varchar(128)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",8,"fxsj","发现时间","date","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",9,"sbdw","上报单位","varchar(100)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",10,"sbry","上报人员","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",11,"rylxdh","人员联系电话","varchar(16)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",12,"zrdw","责任单位","varchar(100)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",13,"zrr","责任人","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",14,"zrrlxdh","责任人联系电话","varchar(16)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",15,"sgdz","事故地址","varchar(255)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",16,"yfyy","引发原因","varchar","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",17,"ssrs","受伤人数","numeric(8)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",18,"swrs","死亡人数","numeric(8)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",19,"ccss","财产损失","numeric(18,2)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",20,"sgmj","事故面积","numeric(18,2)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",21,"sgtj","事故体积","numeric(18,2)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",22,"xczp","现场照片","bytea","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",23,"czdw","处置单位","varchar(100)","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",24,"czgc","处置过程","varchar","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",25,"czzp","处置照片","bytea","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",26,"czfzr","处置负责人","varchar(32)","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",27,"czfzrlxdh","处置负责人联系电话","varchar(16)","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",28,"czwcsj","处置完成时间","date","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",29,"cjr","创建人","varchar(32)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",30,"cjsj","创建时间","date","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",31,"fj","附件","bytea","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",32,"bz","备注","varchar(255)","O"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",33,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",34,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",35,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jc_dltxsg","道路塌陷事故属性结构表",36,"tbsj","同步时间","timestamp","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",3,"gcmc","工程名称","varchar(100)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",4,"jcdw","检测单位","varchar(100)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",5,"dlmc","道路名称","varchar(32)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",6,"yhbh","隐患编号","varchar(20)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",7,"yhmc","隐患名称","varchar(32)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",8,"yhlx","隐患类型","int4","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",9,"yhdz","隐患地址","varchar(255)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",10,"fxdj","风险等级","varchar(32)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",11,"cd","长度","numeric(8,2)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",12,"kd","宽度","numeric(8,2)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",13,"ms","埋深","numeric(8,2)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",14,"jg","净高","numeric(8,2)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",15,"ldyx","雷达影像","bytea","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",16,"xczp","现场照片","bytea","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",17,"yzyx","验证影像","bytea","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",18,"cyfx","成因分析","varchar(255)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",19,"fxsj","发现时间","date","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",20,"sbdw","上报单位","varchar(100)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",21,"sbry","上报人员","varchar(32)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",22,"rylxdh","人员联系电话","varchar(16)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",23,"czdw","处置单位","varchar(100)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",24,"czgc","处置过程","varchar","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",25,"czzp","处置照片","bytea","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",26,"czfzr","处置负责人","varchar(32)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",27,"fzrlxdh","负责人联系电话","varchar(16)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",28,"czwcsj","处置完成时间","date","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",29,"fj","附件","bytea","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",30,"bz","备注","varchar(255)","O"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",31,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",32,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",33,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jc_dltxyh","道路塌陷隐患属性结构表",34,"tbsj","同步时间","timestamp","M"]
["dl_jc_spjk","视频监控属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jc_spjk","视频监控属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jc_spjk","视频监控属性结构表",3,"sbmc","设备名称","varchar(50)","M"]
["dl_jc_spjk","视频监控属性结构表",4,"azdz","安装地址","varchar(255)","M"]
["dl_jc_spjk","视频监控属性结构表",5,"jkdx","监控对象","varchar(255)","M"]
["dl_jc_spjk","视频监控属性结构表",6,"sbxh","设备型号","varchar(255)","M"]
["dl_jc_spjk","视频监控属性结构表",7,"sccj","生产厂家","varchar(100)","O"]
["dl_jc_spjk","视频监控属性结构表",8,"cqdw","产权单位","varchar(100)","M"]
["dl_jc_spjk","视频监控属性结构表",9,"spdz","视频地址","varchar(255)","O"]
["dl_jc_spjk","视频监控属性结构表",10,"bz","备注","varchar(255)","O"]
["dl_jc_spjk","视频监控属性结构表",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_jc_spjk","视频监控属性结构表",12,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jc_spjk","视频监控属性结构表",13,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jc_spjk","视频监控属性结构表",14,"tbsj","同步时间","timestamp","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",3,"dlmc","道路名称","varchar(32)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",4,"zgdw","主管单位","varchar(100)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",5,"jcdx","检查对象","varchar(255)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",6,"bhly","病害来源","varchar(100)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",7,"bhbw","病害部位","varchar(100)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",8,"bhlx","病害类型","varchar(64)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",9,"bhsl","病害数量","int4","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",10,"bz","备注","varchar(255)","O"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",13,"tbsj","同步时间","timestamp","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",2,"xjyhbsm","巡检养护标识码","varchar(32)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",3,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",4,"sfsjgcjx","是否涉及工程机械","bool","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",5,"wtfl","问题分类","int4","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",6,"wtms","问题描述","varchar(255)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",7,"jcdz","检查地址","varchar(255)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",8,"wtsbdw","问题上报单位","varchar(100)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",9,"wtsbr","问题上报人","varchar(16)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",10,"wtsbsj","问题上报时间","timestamp","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",11,"wtczdw","问题处置单位","varchar(100)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",12,"wtczfzr","问题处置负责人","varchar(32)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",13,"wtczfzrlxdh","问题处置负责人联系电话","varchar(16)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",14,"wtczsj","问题处置时间","timestamp","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",15,"wtczjs","问题处置简述","varchar(255)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",16,"czzt","处置状态","int4","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",17,"czfj","处置附件","bytea","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",18,"xctp","现场图片","bytea","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",19,"bz","备注","varchar(255)","O"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",20,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",21,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",22,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",23,"tbsj","同步时间","timestamp","M"]
["dl_jg_yhwx","道路养护维修属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",3,"dlmc","道路名称","varchar(32)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",4,"bhbw","病害部位","varchar(100)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",5,"yhlx","养护类型","varchar(100)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",6,"yhzt","养护状态","varchar(100)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",7,"bz","备注","varchar(255)","O"]
["dl_jg_yhwx","道路养护维修属性结构表",8,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",9,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_jg_yhwx","道路养护维修属性结构表",10,"tbsj","同步时间","timestamp","M"]
["dl_js_csdl","城市道路属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_js_csdl","城市道路属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_js_csdl","城市道路属性结构表",3,"dlmc","道路名称","varchar(32)","M"]
["dl_js_csdl","城市道路属性结构表",4,"dlqd","道路起点","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",5,"dlzd","道路终点","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",6,"dlzx","道路走向","int4","O"]
["dl_js_csdl","城市道路属性结构表",7,"dldj","道路等级","int4","M"]
["dl_js_csdl","城市道路属性结构表",8,"glfl","管理分类","int4","M"]
["dl_js_csdl","城市道路属性结构表",9,"yhdj","养护等级","int4","M"]
["dl_js_csdl","城市道路属性结构表",10,"dlcd","道路长度","numeric(12,2)","M"]
["dl_js_csdl","城市道路属性结构表",11,"dlkd","道路宽度","numeric(8,2)","M"]
["dl_js_csdl","城市道路属性结构表",12,"dlmj","道路面积","numeric(12,2)","M"]
["dl_js_csdl","城市道路属性结构表",13,"jsdw","建设单位","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",14,"sjdw","设计单位","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",15,"sgdw","施工单位","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",16,"jldw","监理单位","varchar(100)","O"]
["dl_js_csdl","城市道路属性结构表",17,"gldw","管理单位","varchar(100)","M"]
["dl_js_csdl","城市道路属性结构表",18,"yhdw","养护单位","varchar(100)","M"]
["dl_js_csdl","城市道路属性结构表",19,"jgny","竣工年月","date","O"]
["dl_js_csdl","城市道路属性结构表",20,"bz","备注","varchar(255)","O"]
["dl_js_csdl","城市道路属性结构表",21,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["dl_js_csdl","城市道路属性结构表",22,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_js_csdl","城市道路属性结构表",23,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_js_csdl","城市道路属性结构表",24,"tbsj","同步时间","timestamp","M"]
["dl_js_dlfsss","道路附属设施属性结构表",1,"bsm","标识码","varchar(32)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",3,"dlmc","道路名称","varchar(32)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",4,"dlqd","道路起点","varchar(100)","O"]
["dl_js_dlfsss","道路附属设施属性结构表",5,"dlzd","道路终点","varchar(100)","O"]
["dl_js_dlfsss","道路附属设施属性结构表",6,"dx","灯型","varchar(32)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",7,"dgsl","灯杆数量","int4","M"]
["dl_js_dlfsss","道路附属设施属性结构表",8,"dzsl","灯盏数量","int4","M"]
["dl_js_dlfsss","道路附属设施属性结构表",9,"js","基数","int4","M"]
["dl_js_dlfsss","道路附属设施属性结构表",10,"zhdgsl","智慧灯杆数量","int4","M"]
["dl_js_dlfsss","道路附属设施属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["dl_js_dlfsss","道路附属设施属性结构表",13,"tbsj","同步时间","timestamp","M"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",1,"bsm","标识码","varchar(32)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",3,"dlmc","道路名称","varchar(32)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",4,"zgdw","主管单位","varchar(100)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",5,"jcdx","检查对象","varchar(255)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",6,"bhly","病害来源","varchar(100)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",7,"bhbw","病害部位","varchar(100)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",8,"bhlx","病害类型","varchar(64)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",9,"bhsl","病害数量","int4","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",10,"bz","备注","varchar(255)","否"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","是"]
["dl_jg_jcbhxx","道路检查病害信息属性结构表",13,"tbsj","同步时间","timestamp","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",1,"bsm","标识码","varchar(32)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",2,"xjyhbsm","巡检养护标识码","varchar(32)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",3,"xzqhdm","行政区划代码","varchar(6)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",4,"sfsjgcjx","是否涉及工程机械","bool","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",5,"wtfl","问题分类","int4","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",6,"wtms","问题描述","varchar(255)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",7,"jcdz","检查地址","varchar(255)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",8,"wtsbdw","问题上报单位","varchar(100)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",9,"wtsbr","问题上报人","varchar(16)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",10,"wtsbsj","问题上报时间","timestamp","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",11,"wtczdw","问题处置单位","varchar(100)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",12,"wtczfzr","问题处置负责人","varchar(32)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",13,"wtczfzrlxdh","问题处置负责人联系电话","varchar(16)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",14,"wtczsj","问题处置时间","timestamp","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",15,"wtczjs","问题处置简述","varchar(255)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",16,"czzt","处置状态","int4","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",17,"czfj","处置附件","bytea","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",18,"xctp","现场图片","bytea","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",19,"bz","备注","varchar(255)","否"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",20,"kjxx","空间信息","geometry(Geometry,4490)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",21,"yskzjbz","原始库主键标志","varchar(64)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",22,"sjtbzt","数据同步状态","varchar(16)","是"]
["dl_jg_xjxcdsfsgwt","巡检养护第三方施工问题属性结构表",23,"tbsj","同步时间","timestamp","是"]
["DL_JC_SPJK","视频监控",null,"BSM","标识码","字符型","M"]
["DL_JC_SPJK","视频监控",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JC_SPJK","视频监控",null,"SBMC","设备名称","字符型","M"]
["DL_JC_SPJK","视频监控",null,"AZDZ","安装地址","字符型","M"]
["DL_JC_SPJK","视频监控",null,"JKDX","监控对象","字符型","M"]
["DL_JC_SPJK","视频监控",null,"SBXH","设备型号","字符型","M"]
["DL_JC_SPJK","视频监控",null,"SCCJ","生产厂家","字符型","O"]
["DL_JC_SPJK","视频监控",null,"CQDW","产权单位","字符型","M"]
["DL_JC_SPJK","视频监控",null,"SPDZ","视频地址","字符型","O"]
["DL_JC_SPJK","视频监控",null,"BZ","备注","字符型","O"]
["DL_JG_JHXM","计划项目",null,"BSM","标识码","字符型","M"]
["DL_JG_JHXM","计划项目",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_JHXM","计划项目",null,"XMMC","项目名称","字符型","M"]
["DL_JG_JHXM","计划项目",null,"XMLX","项目类型","字符型","M"]
["DL_JG_JHXM","计划项目",null,"ZGDW","主管单位","字符型","M"]
["DL_JG_JHXM","计划项目",null,"XMNR","项目内容","字符型","M"]
["DL_JG_JHXM","计划项目",null,"JHND","计划年度","整型","M"]
["DL_JG_JHXM","计划项目",null,"XMJSZQ","项目建设周期","整型","M"]
["DL_JG_JHXM","计划项目",null,"XMTZE","项目投资额","浮点型","M"]
["DL_JG_JHXM","计划项目",null,"BZ","备注","字符型","O"]
["DL_JG_JSXM","建设项目",null,"BSM","标识码","字符型","M"]
["DL_JG_JSXM","建设项目",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_JSXM","建设项目",null,"XMMC","项目名称","字符型","M"]
["DL_JG_JSXM","建设项目",null,"XMDM","项目代码","字符型","O"]
["DL_JG_JSXM","建设项目",null,"XMBM","项目编码","字符型","O"]
["DL_JG_JSXM","建设项目",null,"XMLX","项目类型","字符型","M"]
["DL_JG_JSXM","建设项目",null,"ZGDW","主管单位","字符型","M"]
["DL_JG_JSXM","建设项目",null,"XMNR","项目内容","字符型","M"]
["DL_JG_JSXM","建设项目",null,"XMTZE","项目投资额","浮点型","M"]
["DL_JG_JSXM","建设项目",null,"XXDZ","详细地址","字符型","M"]
["DL_JG_JSXM","建设项目",null,"LXXKXX","立项许可信息","字符型","O"]
["DL_JG_JSXM","建设项目",null,"GHXKXX","规划许可信息","字符型","O"]
["DL_JG_JSXM","建设项目",null,"SGXKXX","施工许可信息","字符型","O"]
["DL_JG_JSXM","建设项目",null,"JGYSXX","竣工验收信息","字符型","O"]
["DL_JG_JSXM","建设项目",null,"JSDW","建设单位","字符型","M"]
["DL_JG_JSXM","建设项目",null,"SJDW","设计单位","字符型","O"]
["DL_JG_JSXM","建设项目",null,"SGDW","施工单位","字符型","O"]
["DL_JG_JSXM","建设项目",null,"JLDW","监理单位","字符型","O"]
["DL_JG_JSXM","建设项目",null,"SJKSSJ","实际开始时间","日期型","O"]
["DL_JG_JSXM","建设项目",null,"SJJSSJ","实际结束时间","日期型","O"]
["DL_JG_JSXM","建设项目",null,"BZ","备注","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"BSM","标识码","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"WHWXNR","维护维修内容","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"SBSS","设备设施","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"CLJG","处理结果","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"CLRQ","处理日期","日期型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"CLRY","处理人员","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"LXDH","联系电话","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"YHDW","养护单位","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"SSQSDW","设施权属单位","字符型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"JCFF","检测方法","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"JCJL","检测结论","字符型","M"]
["DL_JG_RCWHWX","日常维护维修",null,"FJ","附件","二进制型","O"]
["DL_JG_RCWHWX","日常维护维修",null,"BZ","备注","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"BSM","标识码","字符型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"SJMC","事件名称","字符型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"SJSM","事件说明","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"DZ","地址","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"GLJCSS","关联基础设施","字符型","M"]
["DL_JG_TFSJQX","突发事件抢修"]
["DL_JG_TFSJQX","突发事件抢修",null,"XYJB","响应级别","整型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"XCZP","现场照片","二进制型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"QXNR","抢修内容","字符型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"CLJG","处理结果","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"CLRQ","处理日期","日期型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"CLRY","处理人员","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"CLDW","处理单位","字符型","O"]
["DL_JG_TFSJQX","突发事件抢修",null,"FJ","附件","二进制型","M"]
["DL_JG_TFSJQX","突发事件抢修",null,"BZ","备注","字符型","O"]
["DL_JG_YHJL","养护记录",null,"BSM","标识码","字符型","M"]
["DL_JG_YHJL","养护记录",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_YHJL","养护记录",null,"YHDX","养护对象","字符型","M"]
["DL_JG_YHJL","养护记录",null,"YHRQ","养护日期","日期型","M"]
["DL_JG_YHJL","养护记录",null,"YHNR","养护内容","字符型","O"]
["DL_JG_YHJL","养护记录",null,"ZYRY","作业人员","字符型","M"]
["DL_JG_YHJL","养护记录",null,"FJ","附件","二进制型","O"]
["DL_JG_YHJL","养护记录",null,"BZ","备注","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"BSM","标识码","字符型","M"]
["DL_JG_XJJL","巡检记录",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_XJJL","巡检记录",null,"XJDX","巡检对象","整型","M"]
["DL_JG_XJJL","巡检记录",null,"JCDY","检查单元","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"JCXM","检查项目","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"JCFF","检查方法","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"JCNR","检查内容","字符型","M"]
["DL_JG_XJJL","巡检记录",null,"JCJG","检查结果","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"CZYH","存在隐患","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"JCRQ","检查日期","时间日期型","M"]
["DL_JG_XJJL","巡检记录",null,"JCRY","检查人员","字符型","O"]
["DL_JG_XJJL","巡检记录",null,"SSQSDW","设施权属单位","字符型","M"]
["DL_JG_XJJL","巡检记录",null,"ZGDW","主管单位","字符型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"BSM","标识码","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"XZQHDM","行政区划代码","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"XMMC","项目名称","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"XMNR","项目内容","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SZJD","所在街道","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"XXDZ","施工项目地址","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JHKSSJ","计划开始时间","日期型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JHJSSJ","计划结束时间","日期型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SJKSSJ","实际开始时间","日期型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SJJSSJ","实际结束时间","日期型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SGSD","施工深度","浮点型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JSDW","建设单位","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JSDWFZR","建设单位负责人","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JSDWFZRLXDH","建设单位负责人联 系电话","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SGDW","施工单位","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SGDWFZR","施工单位负责人","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"SGDWFZRLXDH","施工单位负责人联 系电话","字符型","M"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JLDW","监理单位","字符型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JLDWFZR","监理单位负责人","字符型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"JLDWFZRLXDH","监理单位负责人联 系电话","字符型","O"]
["DL_JG_DSFSGZX","第三方施工专项",null,"BZ","备注","字符型","O"]
["QL_JG_DQJC","定期检测",1,"BSM","标识码","字符型","M"]
["QL_JG_DQJC","定期检测",2,"XZQHDM","行政区划代码","字符型","M"]
["QL_JG_DQJC","定期检测",3,"JCDX","检测对象","字符型","M"]
["QL_JG_DQJC","定期检测",4,"JCSJ","检测时间","时间日期型","M"]
["QL_JG_DQJC","定期检测",5,"JCDW","检测单位","字符型","O"]
["QL_JG_DQJC","定期检测",6,"JCR","检测人","字符型","O"]
["QL_JG_DQJC","定期检测",7,"JCDWLXDH","检测单位联系电话","字符型","O"]
["QL_JG_DQJC","定期检测",8,"JCFF","检测方法","字符型","M"]
["QL_JG_DQJC","定期检测",9,"JCJL","检测结论","字符型","M"]
["QL_JG_DQJC","定期检测",10,"BZ","备注","字符型","O"]

{"sheet":"综合应用","index":7,"n_rows":105,"n_cols":7,"rows_kept":105,"cut":false,"hidden":false,"merged":[]}
["表名","表注释","字段序号","字段名","字段注释","字段类型","非空"]
["zy_js_bncs","避难场所",1,"bsm","标识码","varchar(32)","M"]
["zy_js_bncs","避难场所",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_bncs","避难场所",3,"csmc","场所名称","varchar(255)","M"]
["zy_js_bncs","避难场所",4,"szdz","所在地址","varchar(255)","M"]
["zy_js_bncs","避难场所",5,"cslb","场所类别","varchar(255)","M"]
["zy_js_bncs","避难场所",6,"kymj","可用面积(万m²)","varchar(255)","M"]
["zy_js_bncs","避难场所",7,"rnrs","容纳人数(万人)","varchar(255)","M"]
["zy_js_bncs","避难场所",8,"fzr","负责人","varchar(255)","M"]
["zy_js_bncs","避难场所",9,"lxdh","联系电话","varchar(255)","M"]
["zy_js_bncs","避难场所",10,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_bncs","避难场所",11,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_bncs","避难场所",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_bncs","避难场所",13,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zy_js_bncs","避难场所",14,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_bncs","避难场所",15,"extract_time","抽取时间","timestamp","M"]
["zy_js_bncs","避难场所",16,"partition_time","日分区字段","int4","M"]
["zy_js_ck","仓库信息",1,"bsm","标识码","varchar(32)","M"]
["zy_js_ck","仓库信息",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_ck","仓库信息",3,"ckmc","仓库名称","varchar(200)","M"]
["zy_js_ck","仓库信息",4,"ckdz","仓库地址","varchar(200)","M"]
["zy_js_ck","仓库信息",5,"lxr","联系人","varchar(50)","M"]
["zy_js_ck","仓库信息",6,"lxdh","联系电话","varchar(50)","M"]
["zy_js_ck","仓库信息",7,"wzzl","物资种类","int4","M"]
["zy_js_ck","仓库信息",8,"wzzs","物资总数","int4","M"]
["zy_js_ck","仓库信息",9,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_ck","仓库信息",10,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_ck","仓库信息",11,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_ck","仓库信息",12,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zy_js_ck","仓库信息",13,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_ck","仓库信息",14,"extract_time","抽取时间","timestamp","M"]
["zy_js_ck","仓库信息",15,"partition_time","日分区字段","int4","M"]
["zy_js_jydw","救援队伍",1,"bsm","标识码","varchar(32)","M"]
["zy_js_jydw","救援队伍",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_jydw","救援队伍",3,"dwmc","队伍名称","varchar(200)","M"]
["zy_js_jydw","救援队伍",4,"zyfzr","主要负责人","varchar(50)","M"]
["zy_js_jydw","救援队伍",5,"lxrdh","联系人电话","varchar(50)","M"]
["zy_js_jydw","救援队伍",6,"zbdh","值班电话","varchar(50)","M"]
["zy_js_jydw","救援队伍",7,"dyrs","队员人数","int4","M"]
["zy_js_jydw","救援队伍",8,"schy","擅长行业","varchar(100)","M"]
["zy_js_jydw","救援队伍",9,"xxdz","详细地址","varchar(200)","M"]
["zy_js_jydw","救援队伍",10,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_jydw","救援队伍",11,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_jydw","救援队伍",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_jydw","救援队伍",13,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zy_js_jydw","救援队伍",14,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_jydw","救援队伍",15,"extract_time","抽取时间","timestamp","M"]
["zy_js_jydw","救援队伍",16,"partition_time","日分区字段","int4","M"]
["zy_js_yjwz","应急物资",1,"bsm","标识码","varchar(32)","M"]
["zy_js_yjwz","应急物资",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_yjwz","应急物资",3,"ssck","所属仓库","varchar(50)","M"]
["zy_js_yjwz","应急物资",4,"wzmc","物资名称","varchar(20)","M"]
["zy_js_yjwz","应急物资",5,"wzlx","物资类型","varchar(20)","M"]
["zy_js_yjwz","应急物资",6,"kcsl","库存数量","int4","M"]
["zy_js_yjwz","应急物资",7,"jldw","计量单位","varchar(20)","M"]
["zy_js_yjwz","应急物资",8,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_yjwz","应急物资",9,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_yjwz","应急物资",10,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_yjwz","应急物资",11,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_yjwz","应急物资",12,"extract_time","抽取时间","timestamp","M"]
["zy_js_yjwz","应急物资",13,"partition_time","日分区字段","int4","M"]
["zy_js_yjzj","应急专家",1,"bsm","标识码","varchar(32)","M"]
["zy_js_yjzj","应急专家",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_yjzj","应急专家",3,"zjxm","专家姓名","varchar(50)","M"]
["zy_js_yjzj","应急专家",4,"js","角色","varchar(100)","M"]
["zy_js_yjzj","应急专家",5,"czd","常驻地","varchar(255)","M"]
["zy_js_yjzj","应急专家",6,"lxdh","联系电话","varchar(50)","M"]
["zy_js_yjzj","应急专家",7,"gzdw","工作单位","varchar(100)","M"]
["zy_js_yjzj","应急专家",8,"sczy","擅长专业","varchar(100)","M"]
["zy_js_yjzj","应急专家",9,"zjcc","专家职称","varchar(100)","M"]
["zy_js_yjzj","应急专家",10,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_yjzj","应急专家",11,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_yjzj","应急专家",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_yjzj","应急专家",13,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_yjzj","应急专家",14,"extract_time","抽取时间","timestamp","M"]
["zy_js_yjzj","应急专家",15,"partition_time","日分区字段","int4","M"]
["zy_js_ylwsjg","医疗卫生机构",1,"bsm","标识码","varchar(32)","M"]
["zy_js_ylwsjg","医疗卫生机构",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_ylwsjg","医疗卫生机构",3,"jgmc","机构名称","varchar(200)","M"]
["zy_js_ylwsjg","医疗卫生机构",4,"szdz","所在地址","varchar(200)","M"]
["zy_js_ylwsjg","医疗卫生机构",5,"jgjb","机构级别","varchar(200)","M"]
["zy_js_ylwsjg","医疗卫生机构",6,"kycw","可用床位","int4","M"]
["zy_js_ylwsjg","医疗卫生机构",7,"fzr","负责人","varchar(50)","M"]
["zy_js_ylwsjg","医疗卫生机构",8,"lxdh","联系电话","varchar(50)","M"]
["zy_js_ylwsjg","医疗卫生机构",9,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_ylwsjg","医疗卫生机构",10,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_ylwsjg","医疗卫生机构",11,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_ylwsjg","医疗卫生机构",12,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zy_js_ylwsjg","医疗卫生机构",13,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_ylwsjg","医疗卫生机构",14,"extract_time","抽取时间","timestamp","M"]
["zy_js_ylwsjg","医疗卫生机构",15,"partition_time","日分区字段","int4","M"]
["zy_js_zdwxy","重大危险源数据",1,"bsm","标识码","varchar(32)","M"]
["zy_js_zdwxy","重大危险源数据",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zy_js_zdwxy","重大危险源数据",3,"wxymc","危险源名称","varchar(200)","M"]
["zy_js_zdwxy","重大危险源数据",4,"wxjb","危险级别","varchar(200)","M"]
["zy_js_zdwxy","重大危险源数据",5,"zdwxyfl","重大危险源分类","varchar(200)","M"]
["zy_js_zdwxy","重大危险源数据",6,"dz","地址","varchar(200)","M"]
["zy_js_zdwxy","重大危险源数据",7,"qymc","企业名称","varchar(200)","M"]
["zy_js_zdwxy","重大危险源数据",8,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zy_js_zdwxy","重大危险源数据",9,"sjtbsj","数据同步时间","timestamp","M"]
["zy_js_zdwxy","重大危险源数据",10,"sjtbzt","数据同步状态","varchar(16)","M"]
["zy_js_zdwxy","重大危险源数据",11,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zy_js_zdwxy","重大危险源数据",12,"sscsdm","所属城市代码","varchar(6)","M"]
["zy_js_zdwxy","重大危险源数据",13,"extract_time","抽取时间","timestamp","M"]
["zy_js_zdwxy","重大危险源数据",14,"partition_time","日分区字段","int4","M"]

{"sheet":"综合管线","index":8,"n_rows":139,"n_cols":7,"rows_kept":139,"cut":false,"hidden":false,"merged":[]}
["表名","表注释","字段序号","字段名","字段注释","字段类型","非空"]
["zh_jg_fxjl","放线记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_fxjl","放线记录属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_fxjl","放线记录属性结构表",3,"ghxkzh","规划许可证号","varchar(50)","M"]
["zh_jg_fxjl","放线记录属性结构表",4,"xmmc","项目名称","varchar(255)","M"]
["zh_jg_fxjl","放线记录属性结构表",5,"xmdd","项目地点","varchar(255)","M"]
["zh_jg_fxjl","放线记录属性结构表",6,"fxfw","放线范围","varchar(255)","否"]
["zh_jg_fxjl","放线记录属性结构表",7,"fxsj","放线时间","timestamp","M"]
["zh_jg_fxjl","放线记录属性结构表",8,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_fxjl","放线记录属性结构表",9,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_fxjl","放线记录属性结构表",10,"tbsj","同步时间","timestamp","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",3,"xmmc","项目名称","varchar(255)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",4,"ghxkxx","规划许可信息","varchar(255)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",5,"sffx","是否放线","bool","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",6,"fxdw","放线单位","varchar(100)","否"]
["zh_jg_ghphgl","规划批后管理属性结构表",7,"sfgzcl","是否跟踪测量","bool","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",8,"gzcldw","跟踪测量单位","varchar(100)","否"]
["zh_jg_ghphgl","规划批后管理属性结构表",9,"sfyx","是否验线","bool","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",10,"yxdw","验线单位","varchar(100)","否"]
["zh_jg_ghphgl","规划批后管理属性结构表",11,"sfjgcl","是否竣工测量","bool","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",12,"jgcldw","竣工测量单位","varchar(100)","否"]
["zh_jg_ghphgl","规划批后管理属性结构表",13,"sfghhs","是否规划核实","bool","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",14,"bz","备注","varchar(255)","否"]
["zh_jg_ghphgl","规划批后管理属性结构表",15,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",16,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",17,"tbsj","同步时间","timestamp","M"]
["zh_jg_ghphgl","规划批后管理属性结构表",18,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",3,"ghxkzh","规划许可证号","varchar(50)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",4,"xmmc","项目名称","varchar(255)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",5,"xmdd","项目地点","varchar(255)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",6,"gtfw","供图范围","varchar","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",7,"sqgxlx","申请管线类型","varchar(8)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",8,"gtgls","供图公里数","numeric(10,2)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",9,"gtmj","供图面积","numeric(12,2)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",10,"gtsj","供图时间","timestamp","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_gxgtjl","管线供图记录属性结构表",13,"tbsj","同步时间","timestamp","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",3,"ghxkzh","规划许可证号","varchar(50)","否"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",4,"xmmc","项目名称","varchar(255)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",5,"xmdd","项目地点","varchar(255)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",6,"jgsj","竣工时间","timestamp","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",7,"hjfw","汇交范围","varchar(255)","否"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",8,"hjgxlx","汇交管线类型","varchar(8)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",9,"hjgls","汇交公里数","numeric(10,2)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",10,"hjsj","汇交时间","timestamp","否"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",11,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",12,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_jgcghjjl","竣工成果汇交记录属性结构表",13,"tbsj","同步时间","timestamp","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",3,"sbsj","上报时间","timestamp","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",4,"yhlx","隐患类型","int4","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",5,"yhmc","隐患名称","varchar(64)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",6,"yhddz","隐患点地址","varchar(255)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",7,"yhms","隐患描述","varchar(255)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",8,"yhxcwj","隐患现场文件","bytea","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",9,"sbr","上报人","varchar(32)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",10,"sbrlxdh","上报人联系电话","varchar(16)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",11,"yhczdw","隐患处置单位","varchar(100)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",12,"czfzr","处置负责人","varchar(32)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",13,"czfzrlxdh","处置负责人联系电话","varchar(16)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",14,"yhslsj","隐患受理时间","timestamp","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",15,"yhczjs","隐患处置简述","varchar","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",16,"yhczbg","隐患处置报告","varchar(255)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",17,"czwcsj","处置完成时间","timestamp","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",18,"bz","备注","varchar(255)","否"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",19,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",20,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",21,"tbsj","同步时间","timestamp","M"]
["zh_jg_jhfxyh","交互风险隐患属性结构表",22,"kjxx","空间信息","geometry(Geometry,4490)","M"]
["zh_jg_yxjl","验线记录属性结构表",1,"bsm","标识码","varchar(32)","M"]
["zh_jg_yxjl","验线记录属性结构表",2,"xzqhdm","行政区划代码","varchar(6)","M"]
["zh_jg_yxjl","验线记录属性结构表",3,"ghxkzh","规划许可证号","varchar(50)","M"]
["zh_jg_yxjl","验线记录属性结构表",4,"xmmc","项目名称","varchar(255)","M"]
["zh_jg_yxjl","验线记录属性结构表",5,"xmdd","项目地点","varchar(255)","M"]
["zh_jg_yxjl","验线记录属性结构表",6,"yxfw","验线范围","varchar(255)","否"]
["zh_jg_yxjl","验线记录属性结构表",7,"yxsj","验线时间","timestamp","M"]
["zh_jg_yxjl","验线记录属性结构表",8,"yskzjbz","原始库主键标志","varchar(64)","M"]
["zh_jg_yxjl","验线记录属性结构表",9,"sjtbzt","数据同步状态","varchar(16)","M"]
["zh_jg_yxjl","验线记录属性结构表",10,"tbsj","同步时间","timestamp","M"]
["GS_JG_JHXM","计划项目",null,"BSM","标识码","字符型","M"]
["GS_JG_JHXM","计划项目",null,"XZQHDM","行政区划代码","字符型","M"]
["GS_JG_JHXM","计划项目",null,"XMMC","项目名称","字符型","M"]
["GS_JG_JHXM","计划项目",null,"XMLX","项目类型","字符型","M"]
["GS_JG_JHXM","计划项目",null,"ZGDW","主管单位","字符型","M"]
["GS_JG_JHXM","计划项目",null,"XMNR","项目内容","字符型","M"]
["GS_JG_JHXM","计划项目",null,"JHND","计划年度","整型","M"]
["GS_JG_JHXM","计划项目",null,"XMJSZQ","项目建设周期","整型","M"]
["GS_JG_JHXM","计划项目",null,"XMTZE","项目投资额","浮点型","M"]
["GS_JG_JHXM","计划项目",null,"BZ","备注","字符型","O"]
["GS_JG_JSXM","建设项目",null,"BSM","标识码","字符型","M"]
["GS_JG_JSXM","建设项目",null,"XZQHDM","行政区划代码","字符型","M"]
["GS_JG_JSXM","建设项目",null,"XMMC","项目名称","字符型","M"]
["GS_JG_JSXM","建设项目",null,"XMDM","项目代码","字符型","O"]
["GS_JG_JSXM","建设项目",null,"XMBM","项目编码","字符型","O"]
["GS_JG_JSXM","建设项目",null,"XMLX","项目类型","字符型","M"]
["GS_JG_JSXM","建设项目",null,"ZGDW","主管单位","字符型","M"]
["GS_JG_JSXM","建设项目",null,"XMNR","项目内容","字符型","M"]
["GS_JG_JSXM","建设项目",null,"XMTZE","项目投资额","浮点型","M"]
["GS_JG_JSXM","建设项目",null,"XXDZ","详细地址","字符型","M"]
["GS_JG_JSXM","建设项目",null,"LXXKXX","立项许可信息","字符型","O"]
["GS_JG_JSXM","建设项目",null,"GHXKXX","规划许可信息","字符型","O"]
["GS_JG_JSXM","建设项目",null,"SGXKXX","施工许可信息","字符型","O"]
["GS_JG_JSXM","建设项目",null,"JGYSXX","竣工验收信息","字符型","O"]
["GS_JG_JSXM","建设项目",null,"JSDW","建设单位","字符型","M"]
["GS_JG_JSXM","建设项目",null,"SJDW","设计单位","字符型","O"]
["GS_JG_JSXM","建设项目",null,"SGDW","施工单位","字符型","O"]
["GS_JG_JSXM","建设项目",null,"JLDW","监理单位","字符型","O"]
["GS_JG_JSXM","建设项目",null,"SJKSSJ","实际开始时间","日期型","O"]
["GS_JG_JSXM","建设项目",null,"SJJSSJ","实际结束时间","日期型","O"]
["GS_JG_JSXM","建设项目",null,"BZ","备注","字符型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"BSM","标识码","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"XZQHDM","行政区划代码","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"XMMC","项目名称","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"XMNR","项目内容","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SZJD","所在街道","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"XXDZ","施工项目地址","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JHKSSJ","计划开始时间","日期型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JHJSSJ","计划结束时间","日期型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SJKSSJ","实际开始时间","日期型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SJJSSJ","实际结束时间","日期型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SGSD","施工深度","浮点型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JSDW","建设单位","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JSDWFZR","建设单位负责人","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JSDWFZRLXDH","建设单位负责人联 系电话","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SGDW","施工单位","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SGDWFZR","施工单位负责人","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"SGDWFZRLXDH","施工单位负责人联 系电话","字符型","M"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JLDW","监理单位","字符型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JLDWFZR","监理单位负责人","字符型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"JLDWFZRLXDH","监理单位负责人联 系电话","字符型","O"]
["GS_JG_DSFSGZX","第三方施工专项",null,"BZ","备注","字符型","O"]

{"sheet":"行政区划代码表","index":9,"n_rows":131,"n_cols":3,"rows_kept":131,"cut":false,"hidden":false,"merged":[[130,0,130,2]]}
["地市名称","行政区划名称","行政区划代码"]
["南京",null,320100]
[null,"玄武区",320102]
[null,"秦淮区",320104]
[null,"建邺区",320105]
[null,"鼓楼区",320106]
[null,"浦口区",320111]
[null,"栖霞区",320113]
[null,"雨花台区",320114]
[null,"江宁区",320115]
[null,"六合区",320116]
[null,"溧水区",320117]
[null,"高淳区",320118]
[null,"南京经开区",320193]
[null,"江宁经开区",320194]
[null,"江北新区",320195]
["无锡",null,320200]
[null,"锡山区",320205]
[null,"惠山区",320206]
[null,"滨湖区",320211]
[null,"梁溪区",320213]
[null,"新吴区",320214]
[null,"江阴市",320281]
[null,"宜兴市",320282]
[null,"经开区",320299]
["徐州",null,320300]
[null,"鼓楼区",320302]
[null,"云龙区",320303]
[null,"贾汪区",320305]
[null,"泉山区",320311]
[null,"铜山区",320312]
[null,"丰县",320321]
[null,"沛县",320322]
[null,"睢宁县",320324]
[null,"新沂市",320381]
[null,"邳州市",320382]
[null,"高新区",320391]
[null,"开发区",320383]
["常州",null,320400]
[null,"天宁区",320402]
[null,"钟楼区",320404]
[null,"新北区",320411]
[null,"武进区",320412]
[null,"溧阳市",320481]
[null,"金坛区",320413]
[null,"经开区",320491]
["苏州",null,320500]
[null,"高新区",320505]
[null,"吴中区",320506]
[null,"相城区",320507]
[null,"姑苏区",320508]
[null,"吴江区",320509]
[null,"常熟市",320581]
[null,"张家港市",320582]
[null,"昆山市",320583]
[null,"太仓市",320585]
[null,"工业园区",320594]
["南通",null,320600]
[null,"崇川区",320613]
[null,"如东县",320623]
[null,"启东市",320681]
[null,"如皋市",320682]
[null,"通州区",320612]
[null,"海门区",320614]
[null,"海安市",320685]
[null,"经开区",320671]
["连云港",null,320700]
[null,"连云区",320703]
[null,"海州区",320706]
[null,"赣榆区",320707]
[null,"东中西示范区",320720]
[null,"东海县",320722]
[null,"灌云县",320723]
[null,"灌南县",320724]
[null,"开发区",320725]
[null,"高新区",320772]
[null,"自贸区",320799]
["淮安",null,320800]
[null,"淮安区",320803]
[null,"淮阴区",320804]
[null,"经开区",320806]
[null,"涟水县",320826]
[null,"洪泽区",320829]
[null,"盱眙县",320830]
[null,"金湖县",320831]
[null,"清江浦区",320891]
[null,"生态文旅区",320813]
[null,"苏淮高新区",320811]
[null,"淮安工业园区",320812]
["盐城",null,320900]
[null,"亭湖区",320902]
[null,"盐都区",320903]
[null,"大丰区",320904]
[null,"经开区",320905]
[null,"响水县",320921]
[null,"滨海县",320922]
[null,"阜宁县",320923]
[null,"射阳县",320924]
[null,"建湖县",320925]
[null,"东台市",320981]
[null,"盐南高新区",320991]
["扬州",null,321000]
[null,"广陵区",321002]
[null,"邗江区",321003]
[null,"宝应县",321023]
[null,"经开区",321071]
[null,"仪征市",321081]
[null,"高邮市",321084]
[null,"江都区",321012]
["镇江",null,321100]
[null,"京口区",321102]
[null,"润州区",321111]
[null,"丹徒区",321112]
[null,"丹阳市",321181]
[null,"扬中市",321182]
[null,"句容市",321183]
["泰州",null,321200]
[null,"海陵区",321202]
[null,"高港区",321203]
[null,"姜堰区",321204]
[null,"兴化市",321281]
[null,"靖江市",321282]
[null,"泰兴市",321283]
[null,"医药高新区",321291]
["宿迁",null,321300]
[null,"宿城区",321302]
[null,"宿豫区",321311]
[null,"沭阳县",321322]
[null,"泗阳县",321323]
[null,"泗洪县",321324]
["注：各设区市可根据实际管理要求扩展。\n"]

{"sheet":"监测设备及指标字典","index":10,"n_rows":65,"n_cols":6,"rows_kept":65,"cut":false,"hidden":false,"merged":[[1,0,4,0],[5,0,11,0],[12,0,40,0],[41,0,61,0],[62,0,64,0],[1,1,4,1],[5,1,11,1],[12,1,40,1],[41,1,61,1],[62,1,64,1],[12,2,14,2],[15,2,17,2],[21,2,22,2],[43,2,44,2],[58,2,60,2],[12,3,14,3],[15,3,17,3],[21,3,22,3],[43,3,44,3],[58,3,60,3],[12,4,14,4],[15,4,17,4],[21,4,22,4],[43,4,44,4],[58,4,60,4]]}
["类型","监测设备大类","监测设备类型","监测设备小类","监测指标","备注"]
["燃气","RQ","可燃气体探测器",1,"可燃气体 浓度","单位： LEL%"]
[null,null,"燃气压力设备",2,"压力","单位： MPa"]
[null,null,"流量计",3,"流量","单位： m3/h"]
[null,null,"温度传感器",4,"温度","单位： C"]
["排水","PS","电子水尺",1,"积水深度","单位： cm"]
[null,null,"井盖异动监测仪",2,"异动情况"]
[null,null,"水位计",3,"液位","单位： m"]
[null,null,"液位计",4,"液位","单位： m"]
[null,null,"流量计",5,"流量","单位： m3/h"]
[null,null,"雨量计",6,"雨量","单位： mm"]
[null,null,"视频监控设备",7,"视频监控"]
["桥梁","QL","三向超声风速仪",1,"风速、风 向","单位："]
[{"$nulls":5},"风速： m/s；"]
[{"$nulls":5},"风向：°"]
[null,null,"机械式风速仪",2,"风速、风 向","单位："]
[{"$nulls":5},"风速： m/s；"]
[{"$nulls":5},"风向：°"]
[null,null,"温度传感器",3,"温度","单位：℃"]
[null,null,"湿度传感器",4,"湿度","单位： %"]
[null,null,"三向加速度传感器",5,"地震","单位： m/s2"]
[null,null,"动态称重系统",6,"车辆荷载","单位："]
[{"$nulls":5},"车重、轴重： kg； 车速： km/h"]
[null,null,"位移计",7,"位移、变 形","单位： mm"]
[null,null,"连通管系统",8,"位移、变 形","单位： mm"]
[null,null,"全球导航卫星系统(GNSS)",9,"位移、变 形","单位： mm"]
[null,null,"倾角传感器",10,"位移、变 形","单位： mm"]
[null,null,"光电挠度仪",11,"位移、变 形","单位： mm"]
[null,null,"电阻应变传感器",12,"应变","单位： με"]
[null,null,"振弦式应变传感器",13,"应变","单位： με"]
[null,null,"光纤光栅应变传感器",14,"应变","单位： με"]
[null,null,"测力支座",15,"支座反力","单位： kN"]
[null,null,"加速度传感器",16,"结构振动","单位： m/s2"]
[null,null,"加速度传感器(频率法)",17,"索力","单位： kN"]
[null,null,"力传感器",18,"索力","单位： kN"]
[null,null,"磁通量传感器",19,"索力","单位： kN"]
[null,null,"光纤光栅智能索力传感器",20,"索力","单位： kN"]
[null,null,"车船撞击报警系统",21,"车船撞击","单位： m/s2"]
[null,null,"梁体偏位报警器",22,"支座偏位","单位： mm"]
[null,null,"振弦式裂缝传感器",23,"裂缝","单位： mm"]
[null,null,"图像裂缝仪",24,"裂缝","单位： mm"]
["供水","GS","在线测温仪",1,"水温","单位：℃(水源水)"]
[null,null,"在线溶氧仪",2,"溶解氧","单位：mg/L(水源水)"]
[null,null,"在线 pH 计",3,"pH 值","无量纲量(水源水、"]
[{"$nulls":5},"出厂水、管网长水龄 区域等处)单位： NTU(水源水、"]
[null,null,"在线浊度仪",4,"浑浊度","工艺过程水、出厂水、管网水、二次供水)"]
[null,null,"电导率仪",5,"电导率","单位：µS/cm(水源 水等)"]
[null,null,"高锰酸盐指数在线测定仪",6,"高锰酸盐 指数","单位：mg/L(水源水、 出厂水)"]
[null,null,"氨氮在线测定仪",7,"氨氮","单位：mg/L(水源水、 出厂水)"]
[null,null,"叶绿素在线分析仪",8,"叶绿素 a","单位： µg/L  (湖库 型水源水)"]
[null,null,"蓝绿藻藻密度在线测定仪",9,"藻密度","单位：  cells/L (湖库型水源水)"]
[null,null,"石油类在线分析仪",10,"石油类","单位： mg/L  (江河 型水源水)"]
[null,null,"挥发酚在线分析仪",11,"挥发酚","单位： mg/L  (江河 型水源水)"]
[null,null,"在线余氯仪",12,"余氯","单位：mg/L(出厂水、 管网水、二次供水)"]
[null,null,"噪声探测仪",13,"漏水声波","单位：PC/g"]
[null,null,"在线压力检测仪",14,"压力","单位：MPa"]
[null,null,"在线高频压力仪",15,"压力","单位：MPa"]
[null,null,"流量监测设备",16,"流量","单位：m3/h"]
[null,null,"智能消火栓",17,null,"重要场所需要包含"]
[{"$nulls":5},"压力监测、防偷盗等"]
[{"$nulls":5},"功能"]
[null,null,"智能井盖",18,null,"人员密集区域"]
["第三方施工","SG","视频监控设备",1,"人员、设 备、围挡"]
[null,null,"定位终端设备",2,"坐标"]
[null,null,"光纤传感器",3,"振幅","单位： Hz"]